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Product Guide Specification

Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, including MasterFormat, SectionFormat, and PageFormat, as described in The Project Resource Manual—CSI Manual of Practice.
The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” when editing this section.

Section numbers and titles are from MasterFormat 2004 Edition.

SECTION 27 11 16

SWING-FRAME EQUIPMENT WALL RACKS

Specifier Notes:  This section covers Middle Atlantic Products, Inc. SFR Series Swing-Frame Wall Rack.  Consult Middle Atlantic Products for assistance in editing this section for the specific application.

PART 1
GENERAL

1.1
SECTION INCLUDES

A.
Swing-frame equipment wall racks.

1.2
RELATED SECTIONS

Specifier Notes:  List sections with work directly related to this section.

A.


1.3
REFERENCES

Specifier Notes:  List standards referenced in this section, complete with designations and titles.  This article does not require compliance with standards, but is merely a listing of those used.

A.
EIA/TIA 310D – Cabinets, Racks, Panels and Associated Equipment.

B.
ISO 9001:2000 – Quality Management Systems – Requirements.

1.4
SUBMITTALS

A.
Comply with Section 01 33 00 – Submittal Procedures.

B.
Product Data:  Submit manufacturer’s product data.

C.
Warranty:  Submit manufacturer’s standard warranty.
1.5
QUALITY ASSURANCE

A.
Manufacturer’s Qualifications:  ISO 9001:2000 registered company.

1.6
DELIVERY, STORAGE, AND HANDLING

A.
Delivery:  Deliver materials to site in manufacturer’s original, unopened containers and packaging, with labels clearly identifying product name and manufacturer.

B.
Storage:  Store materials in clean, dry area indoors in accordance with manufacturer’s instructions.

C.
Handling:  Protect materials and finish during handling and installation to prevent damage.

1.7
WARRANTY

A.
Warranty Period:  Product lifetime.
PART 2
PRODUCTS

2.1
MANUFACTURER

A.
Middle Atlantic Products, Inc.  Phone (973) 839-1011.  Fax (973) 839-1976.  Website middleatlantic.com.  E-mail info@middleatlantic.com.

2.2
SWING-FRAME EQUIPMENT WALL RACKS
A.
Swing-Frame Equipment Wall Racks:  SFR Series Swing-Frame Wall Rack.

Specifier Notes:  Specify swing-frame equipment wall rack model number.  Consult Middle Atlantic Products product information for available models.
1.
Model:  SFR-__________ .

2.
Type:  19-inch wall-mount swing gate rack.

3.
Compliance:  EIA/TIA 310D.

Specifier Notes:  Specify overall height and useable racking height.
4.
Overall Dimensions:

a.
Overall Height:  _____ inches ( _____ mm).

b.
Overall Depth:  18.00 inches (457 mm).

5.
Useable Dimensions:

a.
Useable Racking Height:  _____ inches ( _____ mm).

b.
Useable Depth:  17.50 inches (445 mm).

6.
Weight Capacity:  100 pounds.

7.
Materials:

a.
Side Plate:  16-gauge steel.

b.
Swing Gate:  14-gauge steel.

c.
Finish:  Black powder coat.
8.
Rackrail:

a.
11-gauge steel with tapped 10-32 mounting holes in universal EIA spacing.

b.
Finish:  Black e-coat.

c.
Rackspaces:  Marked.

9.
Positive Stop:  90 degrees.
PART 3
EXECUTION

3.1
EXAMINATION

A.
Examine areas to receive swing-frame equipment wall racks.

B.
Notify Architect of conditions that would adversely affect installation or subsequent use.

C.
Do not begin installation until unacceptable conditions are corrected.

3.2
INSTALLATION

A.
Install swing-frame equipment wall racks in accordance with manufacturer’s instructions at locations indicated on the Drawings.

B.
Install swing-frame equipment wall racks plumb, level, square, and secure.

3.3
ADJUSTING

A.
Adjust operating hardware to operate smoothly without binding.

B.
Repair minor damages to finish in accordance with manufacturer’s instructions and as approved by Architect.
3.4
PROTECTION

A.
Protect installed swing-frame equipment wall racks from damage during construction.
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