

Request and Rationale for Street Light on W. Lafayette Street in Bolton Hill
 to increase illumination for Brown Memorial Park Avenue Presbyterian Church in Bolton Hill
December 5, 2025
Brown Memorial Park Avenue Presbyterian Church's congregation is requesting a streetlight to replace the streetlight that was once located on W. Lafayette Street where electricity is still installed, in the middle of the block on West Lafayette Street between the NE corners of Park and W. Lafayette St. and Jenkins Alley and W. Lafayette St.  given the electricity is already in existence. All that is needed is an Otterbien light pole with an LED light and globe/diffuser for the lamp.

FYI, I have discussed this with Mr. David Framm, Real Estate Agent, Supervisor, Land Conveyance Section, Right of Way Services, for Baltimore City. He has authorized the return of the light but has no money for it in his current budget. He suggested I make a request to Baltimore City to include funds for this light for the next fiscal year, i.e., 2027 Budget

 It may help you to know that Brown Memorial Park Ave. Presbyterian Church received a grant of $150,000 from the Department of Homeland Security, Federal Emergency Management Agency to protect Brown Memorial congregation and its Church Building.  Brown Memorial received these funds in September 2024  given its historical designation in Bolton Hill,  for the beauty of the building, having the largest collection of Tiffany stained glass windows in the U.S. and to help protect the congregation from extremist groups and individuals given its long history of social justice work in Baltimore City, its work with LGBQT+ citizens, and refugees and immigrants.  Our grant money is permitted to be used to harden the church's perimeter, with security cameras, defense glass, lighting and communication equipment.  However, we are not permitted to purchase any lighting with Federal funds that is the responsibility of a city government - such as streetlights. Mr. Framm and the Bolton Hill Historical Society's representative from CHAP, Susan Van Buren, and Eddie Leone, Baltimore City Historical Society representative, have indicated support for the perimeter improvements to improve the Church's vulnerability. After touring and learning about the improvements to the building they determined them to be consistent with maintaining the historical designation of the neighborhood.  Furthermore, we have received training from the Baltimore Police Department, Detective Stephan Robinson, on how to make our church building more secure and how to protect our congregation from an active shooter incident.  We also learned from Detective Robinson that improved lighting assists the police department's patrols of the area.  

For this reason, we are requesting Baltimore City to support our efforts to protect the historic designation of our church, neighborhood, and the safety and security of our congregation. (See desired light fixture diagrams attached to this request.)
 

Submitted by,

Andrew L. Ross

Andrew L. Ross, Ph.D.
Chair of Safety Committee 
Member of Church Board of Directors
410-245-1936
arossinbalt@gmail.com
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Lumilock LED Specifications:

Ordering Guide

S5776AF: LUMINAIRE W/ INTERNAL GFl OUTLET (shown)
Modifications: Internal GFI outlet.

64, 4000K (neutral) LEDs, typical 75 Color Rendering Index (CRI), >100,000 hours of
operational life (at 25°C ambient temperature & 70% lumen maintenance), injection
molded Type 5 Short optical plates, IP66 rated optical system.

Integral Advance Xitanium LED driver, class 1, IP66 rated, 530mA, IntelliVolt

120-277 VAC, 50—-60Hz, RoHS compliant, field replaceable 10kV/10kA surge
suppression.

Delivered lumens: 12174, Wattage: 104W.

Field Adjustable Wattage Switch (FAWS), see chart below for settings.

Lumilock LED Certifications:

Color:
Black
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ETL/CcETL listed to U.S. & Canada safety standards for wet locations, manufactured
to ISO 9001:2008 Standards, vibration tested to ANSI C136.31 for Normal Applications,
UL8750 & UL1598 compliant, LM79 & LM80 tested, DLC listed.

FAWS SYSTEM Top View
posrion | “UMENS | warTace LED Module Assy.
1 3652 29
2 6452 50
3 7548 58
4 8887 70
5 9496 76
6 10104 81
7 10591 88
8 11078 93
9 11565 97
10 12174 104

*Factory set to position 10*

ROOF: CLEAR PRIMATIC ACRYLIC

LED MODULE:

TYPE 5 LUMILOCK W/ SHORT OPTICS
& 7—-PIN TWIST-LOCK RECEPTACLE,
(see specification notes)

GLOBE: CLEAR PRISMATIC ACRYLIC

DRIVER COVER:
DIE-CAST ALUMINUM, TOOL-LESS ENTRY

CAMDEN ADAPTOR:
DIE-CAST ALUMINUM, TOOL—LESS ENTRY emes

DRIVER ENCLOSURE:

DIE—-CAST ALUMINUM W/ SIDE HINGED
ACCESS DOOR, TWIST—LOCK RECEPTACLE
(eye supplied by others), INTERNAL GFI
OUTLET, 3" I.D. SLIP FITTER

FASTENERS:
STAINLESS STEEL HEX HEAD BOLTS

View w/ globe removed

CONFIDENTIAL:

This drawing is confidential and proprietary Littlestown, Pa 17340
to Hadco and may not be reproduced Phone 800-937—-5483 “nno
without the express written consent of

Hadco. Any use hereof or of any of the
information or detail herein shall be for

100 Craftway Drive

Fax 717-359-0618
www.signify.com

the sole benefit of Hadco. JOB NAME:
NOTICE: City of Baltimore, MD — Victorian LED
This drawing is for ref ly. Check
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