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320马力液力推土机 GTY320

320HP Hydraulic Standard Type Bulldozer GTY320
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适用范围：

GTY320 履带式推土机，采用国内领先的工艺生产技术，进行标准化量产的大功率推土机，整机采用先进的液力传动，液压操纵技术，结构先进合理，操纵轻便灵活，质量可靠。

Scope of Application:

GTY320 crawler bulldozer, carries out standardized mass production of high-power bulldozer. The whole machine adopts advanced hydraulic transmission, hydraulic control technology, advanced and reasonable structure, light and flexible operation, quality and reliable.

产品特点：

•搭配康明斯NTA855-C360S10发动机，动力强劲，高效节能。

•高可靠性的动力换挡变速箱，稳定的液力变矩器，二级直齿结构的终传动，均可高效的传输动力。

•具有独立的发动机冷却水箱，底盘油冷却器，重发发动机自配的水、空中冷器，均为本款设备提供了卓越的冷却性能和简易的保养操作，可确保机器连续作业。

•全箱型结构的主机架采用钢板焊接全箱型整体式结构，与后桥箱焊接为一体，具备较高的承载冲击载荷和抗弯扭的能力，高质量焊缝确保主机架具有全寿命周期。

•终传动低位驱动，可提供更加强大的驱动力和高效的爬坡能力。履带式行走底盘的工艺已经达到国际先进水平，适合各种复杂工况，具备较高的可靠性和承载能力。
•标配的直倾推土铲具有强大的切削力，大型单齿或三齿松土器具有可调节的入土角，可用于粘土、硬化的冻土等土层的疏松，还可用于砾石、板结的盐矿等较坚硬作业面的剥离。

Main Features:

•CUMMINS NTA855-C360S10 engine which can gives you more power and reliability you need.

•The highly reliable power shift transmission, stable torque converter and the two-stage straight-tooth structure final drive transmit power efficiently.

•With independent engine cooling water tank, chassis oil cooler, water and air intercooler provides excellent cooling performance and simple maintenance operation to ensure continuous operation of the machine.

•The main frame of the full box structure adopts steel plate welded full box type integral structure, which is welded with the rear axle box. It has high impact load bearing capacity and resistance to bending and twisting. High quality weld seam ensures the main frame has a full life cycle.

•The final drive is driven low and provides more powerful driving force and efficient gradeability. The crawler-type walking chassis has reached the international advanced level and is suitable for various complicated working conditions, with high reliability and carrying capacity.

•The standard straight tilt blade features powerful cutting force and the three-shank ripper can be equipped for the ripping of clay and frozen earth, featuring high working efficiency and super-strong penetrating force.
主要技术参数 Main Specifications

	型号 Model
	GTY320

	名称 Type
	 Standard Hydraulic Crawler Type

	发动机型号
	CUMMINS NTA855-C360S10

	发动机排量（L）Displacement
	14.01

	额定功率（kw/rpm）Rated power
	257/2000

	最大扭矩（N.m/rpm）Max.torque
	1509/1400

	使用重量 Operating weight(without ripper)
	37.2 Ton

	长×宽×高(mm) Dimension(without ripper)
	6535×4150×3515

	接地长度 (mm) Grounding length
	3150

	接地比压(MPa) Ground pressure
	0.105

	履带中心距（mm） Track gauge
	2140

	铲刀容量(m³) Dozing capacity
	10

	铲刀宽度（mm） Blade width
	4150

	铲刀高度（mm） Blade height
	1592

	铲刀提升高度（mm） Blade lifting height
	1560

	铲刀倾斜高度（mm） Height of blade tilt
	1000

	最大切削深度（mm） Max drop below ground
	560

	履带板宽度（mm） Track shoe width
	560

	链轨节距（mm） Pitch
	228.6

	链轨节数量 Quantity of track link
	41

	托轮数量 Quantity of Carrier rollers
	4

	支重轮数量 Quantity of Track rollers
	14

	液压系统最高工作压力（MPa） Max pressure
	14

	液压系统流量L/min Discharge
	335.5

	最大牵引力（kN） Max tractor force
	281

	前进各档速度 (Km/h) Forward Speed
	F1:0-3.6

	
	F2:0-6.6

	
	F3:0-11.5

	后退各档速度 (Km/h) Rear Speed
	R1:0-4.4

	
	R2:0-7.8

	
	R3:0-13.5


标准配置 Standard Configurations
	序号S/N
	名称Item
	厂家Manufacturer

	1
	发动机
Engine
	康明斯CUMMINS

	2
	液力变矩器
Torque converter
	SINOMACH

	3
	变速箱
Gear box
	SINOMACH

	4
	转向离合器
Steering clutch
	荣成金润通JINRUNTONG

	5
	制动器
Brake
	尚义五环WUHUAN

	6
	齿轮泵
Gear pump
	长治液压CHANGZHI

	7
	多路阀
Valve
	大连兴龙XINLONG

	8
	履带板
Track shoe
	辽鞍或攀钢LIAOAN

	9
	支重轮、托轮
Track roller, carrier roller
	济宁金牛JINNIU

	10
	油缸
Cylinder
	文登油缸厂WENDENG




