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100马力干地推土机 GT100

100HP  Standard Type Bulldozer GT100
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适用范围：

GT100履带推土机，采用机械传动，液压助力转向，操作简单，故障率低、保养维修成本低，性价比高。

鉴于小马力推土机转弯半径小、性能稳定、操作灵活等特点，多用于水利工程、电厂、码头、砖厂、煤场、小型垃圾填埋场、钢厂运输巷道等狭小地块环境，同样适用于军队相关工程项目建设。

Scope of Application:

GT100 crawler bulldozer adopts mechanical transmission, hydraulic power steering, simple operation, low failure rate, low maintenance and repair cost, and high cost performance.

In view of the characteristics of small turning radius, stable performance and flexible operation, small horsepower bulldozers are mostly used in water conservancy projects, power plants, wharfs, brick factories, coal yards, small landfills, steel mills and other narrow plot environments. Construction of military-related engineering projects.
产品特点：

1、本机采用东方红与英国里卡多公司合资技术生产的柴油发动机，符合国家II阶段排放要求，噪音低、扭距大、节能环保；可选装康明斯4BTA3.9-C110-II发动机；
2、采用组合式仪表，实时监控整车工作状态；

3、优化后的行走机构及加强型底盘，采用了特殊材料的定制型材，极大的提高了整机强度和耐冲击性。

4、液压系统采用氟胶圈，密封性高效可靠；

5、采用干式、多片结构、常结合主离合器，具有扭距储备大，工作可靠；

6、变速箱为4F﹢2R机械换档变速箱，操作简单，维修方便，使用可靠；

7、传动：采用两级、直齿、大模数齿轮传动，具有承载能力强，可靠性高等优点；

8、全车标配LED大灯，提高夜间施工效率；

9、可选装直倾铲、角铲、煤铲等多种工作装置满足多种工况施工需要。

Main Features:

1. This machine adopts the diesel engine produced by the joint venture technology of Dongfanghong and the British Ricardo Company, which meets the national stage II emission requirements, with low noise, large torque, energy saving and environmental protection; Cummins 4BTA3.9-C110-II engine is optional;

2. The combined instrument is used to monitor the working status of the vehicle in real time;

3. The optimized running mechanism and reinforced chassis adopt customized profiles of special materials, which greatly improves the strength and impact resistance of the whole machine.

4. The hydraulic system adopts fluorine rubber ring, and the sealing performance is efficient and reliable;

5. It adopts dry type, multi-plate structure, often combined with the main clutch, with large torque reserve and reliable operation;

6. The gearbox is a 4F﹢2R mechanical shift gearbox, which is easy to operate, easy to maintain and reliable to use;

7. Transmission: It adopts two-stage, straight teeth and large modulus gear transmission, which has the advantages of strong bearing capacity and high reliability;

8. The whole vehicle is equipped with LED headlights as standard to improve the construction efficiency at night;

9. Various working devices such as straight tilting shovel, angle shovel and coal shovel are optional to meet the construction needs of various working conditions.
主要技术参数 Main Specifications

	型号
	Model
	Unit
	GT100

	整机重量
	Total weight
	kg
	10400

	最大牵引力
	Max towing force
	kN
	95

	发动机型号
	Engine model
	 
	LR6A3-23 

	发动机标定功率/转速
	Engine rated power /speed
	kw/ r/min
	81/2300

	发动机燃油消耗率
	Fuel consumption of the engine
	g/km.h
	≤220

	发动机最大扭距
	Engine max torque
	N.m
	414

	前进1-4档
	Forward 1-4 gear
	km/h
	2.6～10.4

	后退1-2档
	Reverse 1-2 gear
	km/h
	3.7～6.7

	履带宽度
	Caterpillar track board width
	mm
	450

	接地比压
	Land pressure
	kPa
	54.4

	外型尺寸(长×宽×高)
	Overall dimension(L×W×H)
	mm
	4190×2935×3020

	推土铲(宽×高)
	Bulldozer shovel（W×H）
	mm
	2935×960

	铲刀最大提升高度
	Blade max lifting height
	mm
	830

	铲刀入土深度
	Blade max digging depth
	mm
	350

	牵引装置/松土器(选装)
	Towing equipment/Ripper(optional)
	 
	固定式/三齿


	标准配置Standard Configurations


	序号S/N
	名称Item
	型号Model
	厂家Manufacturer

	1
	发动机Engine
	LR6A3-23
	东方红 DONGFANGHONG 

	3
	变速箱
Gear box
	　
	洛推LUOTUI

	4
	转向离合器
Steering clutch
	　
	洛推LUOTUI

	5
	制动器
Brake
	　
	洛推LUOTUI

	6
	离合器

clutch
	ZTS90.21A　
	一拖YTO

	7
	多路阀
Valve
	　
	荆山液压JINGSHAN

	8
	履带板
Track shoe
	
	山推SHANTUI

	9
	支重轮、托轮
Track roller, carrier roller
	　
	济宁金牛JINNIU

	10
	油缸
Cylinder
	　
	金海JINHAI
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