[image: image1.png]



[image: image2.png]P EfE LEEEREZHRAR

SINOMACH INTERNATIONAL EQUIPMENT COMPANY LIMITED



       
                                                                                                 www.sinomach-hi.com

220马力液力推土机 GTY220 

220HP Hydraulic Standard Type Bulldozer GTY220
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适用范围：

GTY220 系列推土机，采用集中润滑、集中测压、履带自动涨紧等先进技术，可配装多种工作装置和驾驶室，可以满足各种工况的作业需求，是土石方施工、散料铲运的理想高效作业设备。

Scope of Application:

GTY220 series bulldozers adopt advanced technologies such as centralized lubrication, centralized pressure measurement and automatic tightening of crawlers. It can be equipped with a variety of working devices and cabs to meet the various working conditions. They are ideal and efficient equipment for earth and stone construction work and bulk scraping.
产品特点：

•搭配康明斯发动机，动力强劲，高效节能。

•高可靠性的动力换挡变速箱，稳定的液力变矩器，二级直齿结构的终传动，均可高效的传输动力。

•可实现故障自动诊断、全程监控。整体铸塑仪表盘集空调、电器、仪表为一体，更加美观高档。

•全箱型结构的主机架采用钢板焊接全箱型整体式结构，与后桥箱焊接为一体，具备较高的承载冲击载荷和抗弯扭的能力，高质量焊缝确保主机架具有全寿命周期。

•半刚性悬挂行走系统，增大履带的接地面积，提高车辆的牵引力。

•按照人体工程学设计，驾驶座椅和扶手可以上下前后调节，变速、转向和油门操纵置于左侧，并采用软轴结构，工作装置操纵置于右侧，采用伺服操纵系统，使操纵过程更加轻便灵活，减轻疲劳。
•标配的直倾推土铲具有强大的切削力，大型单齿或三齿松土器具有可调节的入土角，可用于粘土、硬化的冻土等土层的疏松，还可用于砾石、板结的盐矿等较坚硬作业面的剥离。

Main Features:

•CUMMINS engine which can meet gives you more power and reliability you need. Improved fuel economy over the previous model with strong torque output and low fuel consumption gives you excellent overall fluid efficiency.

•The highly reliable power shift transmission, stable torque converter and the two-stage straight-tooth structure final drive transmit power efficiently.

•It can realize automatic fault diagnosis and full monitoring.The overall cast instrument panel integrates air conditioning, electrical appliances and instruments into one, which is more beautiful and luxury.

•The main frame of the full box structure adopts steel plate welded full box type integral structure, which is welded with the rear axle box. It has high impact load bearing capacity and resistance to bending and twisting. High quality weld seam ensures the main frame has a full life cycle.

•According to the ergonomic design, the driver's seat and armrest can be adjusted up and down, the shifting, steering and throttle are placed on the left side, and the soft shaft structure is adopted. The working device is operated on the right side, and the servo control system is used to make the operation process more light and flexible.

•The standard straight tilt blade features powerful cutting force and the three-shank ripper can be equipped for the ripping of clay and frozen earth, featuring high working efficiency and super-strong penetrating force.
主要技术参数 Main Specifications

	型号 Model
	GTY220

	名称 Type
	 Standard Hydraulic Crawler Type

	发动机型号 Engine Model
	CUMMINS NT855-C280S10

	发动机排量（L）Displacement
	14.01

	额定功率（kw/rpm）Rated power
	175/1800

	最大扭矩（N.m/rpm）Max.torque
	1085/1300

	使用重量 Operating weight (without ripper)
	23.5 Ton

	长×宽×高(mm) Dimension (without ripper)
	5390×3735×3350

	接地长度 (mm) Grounding length
	2730

	接地比压(MPa) Ground pressure
	0.077

	履带中心距（mm） Track gauge
	2000

	铲刀容量(m³) Dozing capacity
	6.4

	铲刀宽度（mm） Blade width
	3735

	铲刀高度（mm） Blade height
	1317

	铲刀提升高度（mm） Blade lifting height
	1210

	最大切削深度（mm） Max drop below ground
	540

	铲刀倾斜高度（mm） Height of blade tilt
	735

	履带板宽度（mm） Track shoe width
	560

	链轨节距（mm） Pitch
	216

	链轨节数量 Quantity of track link
	38

	托轮数量 Quantity of Carrier rollers
	4

	支重轮数量 Quantity of Track rollers
	12

	液压系统最高工作压力（MPa） Max pressure
	14

	液压系统流量L/min Discharge
	262

	最大牵引力（kN） Max tractor force
	203

	前进各档速度 (Km/h) Forward Speed
	F1:0-3.6

	
	F2:0-6.5

	
	F3:0-11.2

	后退各档速度 (Km/h) Rear Speed
	R1:0-4.3

	
	R2:0-7.7

	
	R3:0-13.2


标准配置 Standard Configurations
	序号S/N
	名称Item
	厂家Manufacturer

	1
	发动机
Engine
	康明斯CUMMINS

	2
	液力变矩器
Torque converter
	SINOMACH

	3
	变速箱
Gear box
	SINOMACH

	4
	转向离合器
Steering clutch
	荣成金润通JINRUNTONG

	5
	制动器
Brake
	尚义五环WUHUAN

	6
	齿轮泵
Gear pump
	潍柴传控 WEICHAI

	7
	多路阀
Valve
	潍柴传控 WEICHAI

	8
	履带板
Track shoe
	辽鞍或攀钢LIAOAN




