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120马力干地推土机 GT120

120HP  Standard Type Bulldozer GT120
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适用范围：

GT120履带推土机，采用机械传动，液压助力转向，操作简单，动力传输损失小、故障率低、保养维修成本低，性价比高。

主要适用于垃圾场、水利、鱼塘、砖厂、基础建设工程、钢厂运输巷道、县乡级公路网的建设和水利工程、环保工程建设。
Scope of Application:

GT120 crawler bulldozer adopts mechanical transmission, hydraulic power steering, simple operation, small power transmission loss, low failure rate, low maintenance and repair cost, and high cost performance.

It is mainly suitable for the construction of garbage dumps, water conservancy, fish ponds, brick factories, infrastructure projects, transportation roadways of steel mills, county and township highway networks, water conservancy projects, and environmental protection projects.
产品特点：

1、本机采用东方红与英国里卡多公司合资技术生产的高压共轨柴油发动机，符合国家II阶段排放要求，噪音低、扭距大、节能环保；可选配康明斯6BT5.9-C125-II发动机。

2、国内知名品牌的四轮一带及优化后的行走机构及加强型底盘，采用了特殊材料的定制型材，极大的提高了整机强度和耐冲击性。

3、液压系统采用氟胶圈，密封性高效可靠，液压油箱与柴油箱分离，便于维修保养；

4、全车标配LED大灯，提高夜间施工效率；

5、配置沙漠型空气滤清器和散热器前端加装的防护装置，有效提高散热性能，增大保养间距，更适应煤场、沙漠、垃圾场等特殊工况作业需求；

6、采用电子监控电气系统，对整机实时监控，保障机器正常运行；

7、工作装置：具有直倾铲、环卫铲、角铲及松土器等多种装置可供选择。

Main Features:

1. This machine adopts the high-pressure common rail diesel engine produced by the joint venture technology of Dongfanghong and British Ricardo Company, which meets the national stage II emission requirements, with low noise, large torque, energy saving and environmental protection; optional Cummins 6BT5.9-C125- II engine.

2. The four-wheel belt, the optimized running mechanism and the reinforced chassis of the well-known domestic brand adopt customized profiles of special materials, which greatly improves the strength and impact resistance of the whole machine.

3. The hydraulic system adopts fluorine rubber ring, which has efficient and reliable sealing, and the hydraulic oil tank is separated from the diesel tank, which is convenient for maintenance;

4. The whole vehicle is equipped with LED headlights as standard to improve the construction efficiency at night;

5. Equipped with a desert-type air filter and a protective device installed at the front end of the radiator, which can effectively improve the heat dissipation performance, increase the maintenance distance, and be more suitable for special operating conditions such as coal yards, deserts, and garbage dumps;

6. The electronic monitoring electrical system is adopted to monitor the whole machine in real time to ensure the normal operation of the machine;

7. Working device: There are various devices such as straight tilting shovel, sanitation shovel, angle shovel and ripper to choose from.

主要技术参数 Main Specifications

	型号
	Model
	Unit
	GT120

	整机重量
	Total weight
	kg
	13000

	最大牵引力
	Max towing force
	kN
	115

	发动机型号
	Engine model
	
	LR6A3Z-20

	发动机标定功率/转速
	Engine rated power /speed
	kw/ r/min
	93/2000

	发动机燃油消耗率
	Fuel consumption of the engine
	g/kw.h
	≤246

	发动机最大扭距
	Engine max torque
	N.m
	526

	前进档行驶速度
	Forward travel speed
	km/h
	前进四档：
2.4～10.6

	后退档行驶速度
	Backward travel speed
	km/h
	后退二档：
3.8～7.0

	履带宽度
	Track board with
	mm
	500

	接地比压
	Land pressure
	kPa
	51

	履带中心距
	track-center distance
	mm
	1860

	外型尺寸(长×宽×高)
	Overall dimension(L×W×H)
	mm
	5560（含松土器）×3135×3230

	推土铲(宽×高)
	Bulldozer shovel（W×H）
	mm
	3135×970

	铲刀最大提升高度
	Blade max lifting height
	mm
	894

	铲刀入土深度
	Blade max digging depth
	mm
	400

	牵引装置/松土器(选装)
	Twing equipment/Scar fier(optional)
	
	固定式/三齿


	标准配置Standard Configurations

	序号S/N
	名称Item
	型号Model
	厂家Manufacturer

	1
	发动机Engine
	LR6A3Z-20
	东方红 DONGFANGHONG 

	3
	变速箱
Gear box
	　
	洛推LUOTUI

	4
	转向离合器
Steering clutch
	　
	洛推LUOTUI

	5
	制动器
Brake
	　
	洛推LUOTUI

	6
	离合器

clutch
	
	一拖YTO

	7
	多路阀
Valve
	　
	荆山液压JINGSHAN

	8
	履带板
Track shoe
	
	山推SHANTUI

	9
	支重轮、托轮
Track roller, carrier roller
	　
	济宁金牛JINNIU

	10
	油缸
Cylinder
	　
	金海JINGHAI /文登WENDENG 
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