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947H WHEEL LOADER SPECIFICATIONS
· Equipped with Dongfeng Cummins engine
· Luxury cabin decoration and A/C provide operator comfort
· 4 forward & 3 reverse power shift transmission
· Combined seal cylinder obtains high seal performance and more reliability

	· Overall Dimension整机尺寸

	1
	Length(with bucket on ground)整机长度
	7670(mm)

	2
	Width(to outside of wheels)整机宽度（到轮胎外侧）
	2570(mm)

	3
	Bucket width铲斗宽度
	2680(mm)

	4
	Height(To the top of the cab)高度（到驾驶室顶部）
	3375(mm)

	5
	Wheel base轴距
	3067(mm)

	6
	Tread轮距
	1860(mm)

	7
	Min. ground clearance最小离地间隙
	460(mm)

	Main Technical Specification主要技术参数

	1
	Rated load额定载荷
	4000(Kg)

	2
	Operating weight整机操作重量
	12300KG

	3
	Rated bucket capacity额定斗容
	2.35(m3) 

	4
	Max. breakout force最大崛起力
	        130kN

	5
	Max. dump clearance最大卸载高度
	3176(mm)

	6
	Dump reach卸载距离
	1095(mm)

	7
	Dump angle at any position 在任意位置卸载角
	≥450

	8
	Digging depth(with bucket bottom horizontal)挖掘深度
	190(mm)

	9
	Max. turning radius最大转弯半径

	
	(1) Outside of bucket 铲斗外侧
	6300(mm)

	
	(2) Outside of rear wheel后轮外侧
	6052(mm)

	10
	Pivot angle frame 转向角
	38+10

	11
	Oscillating angle of rear axle后桥摆动角
	+11o

	12
	Lifting time of bucket铲斗提升时间
	≤5.5(sec.)

	13
	Lowering time of bucket铲斗下降时间
	≤3.2(sec.)

	14
	Dumping time翻斗时间
	≤1.1(sec.)

	15                                                     
	Traveling speed(Km/h)，4 forward and 3 reverse 行驶速度，4前进档，3后退档

	
	(1) 1st gear forward前进一档
	6.5

	
	(2) 2nd gear forward前进二档
	12

	
	(3) 3rd gear forward前进三档
	25

	
	(4) 4th gear forward前进四档
	35

	
	(3) 1st gear reverse后退一档
	6.5

	
	(3) 2nd gear reverse后退二档
	12

	
	(3) 3rd gear reverse后退三档
	25

	Diesel engine发动机

	1
	Model型号
	Dongfeng Cummins engine 东风康明斯
6BTA5.9-C180

	
	Type形式
	Direct injection. Turbocharged. Water cooling
直喷式，涡轮增压，水冷

	3
	Rated output额定功率
	132 (kW)

	4
	Inter-bore of cylinder/stroke缸径/行程
	102X120  (mm)

	5
	Total exhaust of cylinder排气量
	5.9 (L)

	6
	Current of Alternator发电机电流
	70(A)

	7
	Power of start motor启动马达的功率
	6(KW)

	8
	Voltage of starting motor启动马达的电压
	24(V)

	9
	Rated speed额定转速
	2200(r/min)

	10
	Max. Torque最大扭矩
	750(N.M)/1500rpm

	11
	Starting type启动方式
	Electric

	12
	Min. specific fuel consumption最小燃油消耗率
	212(g/Kw.h)

	13
	Engine specific oil consumption机油消耗率
	0.9-1.6(g/Kw.h)

	14
	Net weight净重
	710(kg)

	Transmission System变速系统

	（一）Torque Converter变矩器

	1
	Model型号
	4WG180

	2
	Type形式
	4-elements. double stage    4元件、双级

	3
	Torque ratio变矩系数
	4

	4
	Cooling type冷却方式
	Pressure oil circulating循环压力油

	(二)、Transmission case变速箱

	1
	Model型号
	4WG180

	2
	Type型式
	Electronic control gear shift
电控换挡

	3
	Gear shift position
换档位置
	 4Forward and 3 reverse gears

	(三)、Axle and Tire桥和轮胎

	1
	Type of main reducer主传动形式
	spiral bevel gear, single stage螺旋伞齿轮、单级

	2
	Gear ratio of main reducer
主传动速比
	5.286

	3
	Type of final reducer轮边减速的形式
	Single stage planetary单级行星轮式

	4
	Gear of ratio of final reducer轮边减速速比
	4.26

	5
	Total ratios总速比
	22.52

	6
	Max. drawing force最大牵引力
	120kN

	7
	Size of tire轮胎尺寸
	20.5-25-16PR

	Working Device Hydraulic System工作液压系统

	1
	Model of oil pump油泵型号
	HGP2063-1010RC

	2
	System pressure系统压力
	180(kgf/cm2)

	3
	Model of Multi-way directional valve多路换向阀型号
	D32II

	4
	Pilot valve 先导阀型号
	DXS-00

	5
	(D*L)Dimension of lifting cylinder 提升油缸尺寸
	Ф125*70*771(mm)

	6
	(D*L)Dimension of tilting cylinder翻斗油缸尺寸
	Ф188*90*502(mm)

	Steering  System转向系统

	1
	Type型式
	Middle articulated frame. Full-hydraulic flow amp. Steering
中间铰接，流量放大全液压转向

	2
	Model of steering pump转向泵型号
	HGP 2063-1010RC-XF

	3
	Model of redirector转向器型号
	BZZ5-500

	4
	Model of distribution valve 分流阀型号
	FLD-F30W

	5
	System pressure系统压力
	14MPa

	6
	Dimension of steering cylinder转向油缸尺寸
	Ф80*45*327(mm)

	Brake System制动系统

	1
	Type of traveling  brake 行车制动形式
	Air over oil activate 4 wheel brake with capliar disc brake
气顶油作用4轮钳盘式制动器

	2
	Air pressure气压
	6-8(kgf/cm2)

	3
	Type of emergency brake
紧急制动
	Automatic cutting air brake自动断气制动

	4
	Type of parking brake
停车制动形式
	Drum brake鼓式制动
Manual control cutting-off air brake手动控制断气制动

	Oil Capacity油量

	1
	Fuel(diesel)柴油
	150(L)

	2
	Engine lubricating oil机油
	13 (L)

	3
	Oil for converter and gear box双变用油
	45(L)

	4
	Oil for hydraulic system液压系统用油
	150(L)

	5
	Oil for driving axles（F/R）前后桥用油
	24/24(L)

	6
	Oil for brake 刹车油
	2X1.0(L)
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