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980H WHEEL LOADER SPECIFICATIONS
· Equipped with reliable XIAN CUMMINS engine 
· KD switch allows better efficiency & easy operation
· Reliable ZF transmission case and Torque Converter
· Famous original ZF wet-type axles with multi-disc limited-slip differentials deliver maximum traction in changing traction conditions
· Bucket automatic leveling ability
· Combined seal cylinder obtains high seal performance and more reliability
· Dual brake valve  & dual pipe full hydraulic brake and central lubrication
	Overall Dimension外形尺寸

	1
	Length(with bucket on ground)整机长度（铲斗放置在地面上）
	8696 (mm)

	2
	Width(to outside of wheels)整机宽度（轮胎外沿）
	3099(mm)

	3
	Bucket width铲斗宽度
	3250(mm)

	4
	Height(To the top of the cab)整机高度（到驾驶室顶部）
	3710(mm)

	5
	Wheel base轴距
	3400(mm)

	6
	Tread轮距
	2350(mm)

	7
	Min. ground clearance最小离地间隙
	504(mm)

	Main Technical Specification

	1
	Rated load额定载荷
	7500(Kg)

	2
	Operating weight操作重量
	23500kg

	3
	Rated bucket capacity额定斗容
	4.2(m3)，可选3.2-4.8 (m3)

	4
	Max. breakout force最大掘起力
	218KN

	5
	Max. Drawing force最大牵引力
	222 KN

	6
	Max. dump clearance最大卸载高度
	 3220(mm)

	7
	Dump reach卸载距离
	1275(mm)

	8
	Dump angle at any position 卸载角（在任意位置）
	≥450

	9
	Digging depth(with bucket bottom horizontal)挖掘深度（铲斗水平放置）
	35(mm)

	10
	Min. turning radius最小转弯半径

	
	(1)Outside of bucket 铲斗外侧
	7042(mm)

	
	(2)Outside of rear wheel后轮外侧
	6486(mm)

	11
	Pivot angle frame 转向角
	38+10

	12
	Oscillating angle of rear axle后桥摆动角
	+12o

	13
	Lifting time of bucket铲斗提升时间
	6.2(sec.)

	14
	Lowering time of bucket铲斗下降时间
	3.9(sec.)

	15                                                     
	Dumping time倾翻时间
	1.9(sec.)

	16
	Traveling speed(Km/h)行驶速度

	
	(1)1st gear (Forward & reverse)1档速度（前/后）
	7.4

	
	(2)2nd gear (Forward & reverse) 2档速度（前/后）
	12.4

	
	(3)3rd gear (Forward & reverse) 3档速度（前/后）
	25.9

	
	(4)4th gear (Forward) 4档速度（前）
	37

	Diesel engine柴油机

	1
	Model型号
	XIAN Cummins QSM11-C290  西安康明斯QSM11-C290

	2
	Type型式
	Direct injection. Turbocharged. Air to air cooling
直喷、增压、空空中冷

	3
	Rated output额定功率
	216(Kw)

	4
	Inter-bore of cylinder/stroke缸径/行程
	125/147(mm)

	5
	Total exhaust of cylinder排气量
	10.8(L)

	6
	Model of starting motor启动马达型号
	42MT400

	7
	Power of starting motor启动马达功率
	7.5(KW)

	8
	Voltage of starting motor启动马达电压
	24(V)

	9
	Rated speed额定转数
	2100(r/min.)

	10
	Max. Torque最大扭矩
	1478(N.m)

	11
	Starting type起动方式
	Electric

	12
	Min. specific fuel consumption最小燃油消耗率
	212(g/Kw.h)

	13
	Engine specific oil consumption发动机机油消耗
	1.0 (g/Kw.h)

	14
	Net weight发动机重量
	980(Kg)

	Transmission System传动系统

	1. Torque Converter变矩器

	1
	Type型式
	3-element.single stage单级三元件

	2
	Torque ratio变矩系数
	2.985

	3
	Max. Dia. of flow path循环圆直径
	370(mm)

	4
	Cooling type冷却方式
	Pressure oil circulating压力油循环

	2. Gear  Box变速箱

	1
	Model型号
	ZF 4WG260

	2
	Type型式
	Power shift, spur gear constant-mesh动力换档，直齿常啮合

	3
	Gear shift position档位数
	4 Forward and 3 reverse gears前进4档后退3档

	3. Axle and Tire桥和轮胎

	1
	Type of main reducer主传动型式
	Spiral gear single stage螺旋伞齿轮单级

	
	
	

	2
	Type of final reducer轮边减速型式
	single stage planetary行星轮式单级

	
	
	

	3
	Total ratios总速比
	24.66

	4
	[bookmark: _GoBack]Size of tyre轮胎尺寸
	26.5-25 -20PR (L-3)

	Working Device Hydraulic System工作液压系统

	1
	Model of oil pump油泵型号(含制动泵)
	P360A367(DRPAA)ZA15-6/P124A082DXZA12-85

	2
	System pressure系统压力
	21(MPa)

	3
	Model of Muti-way directional valve多路阀型号
	GD40-00

	4
	Model of pilot valve先导阀型号
	CRV-00（W2）

	5
	(d*l)Dimension of lifting cylinder 提升油缸尺寸
	Ф180*100*767(mm)

	6
	(D*l)Dimension of tilting cylinder翻斗油缸尺寸
	Ф210*110*550(mm)

	Steering  System转向系统

	1
	Type型式
	Middle articulated frame. full hydraulic power中间铰接，全液压转向

	2
	Model of steering pump转向泵型号
	PB360A367DRZA17-6/P124ANSZA20

	3
	Model of redirector转向器型号
	150-1084/101-5TX-315-E

	4
	System pressure系统压力
	17.5MPa

	5
	Dimension of steering cylinder
转向油缸尺寸
	Ф100*50*441(mm)

	Brake System制动系统

	1
	Type of traveling  brake 行程制动系统
	Wet type multi-disc brake湿式多片制动器
Dual brake valve& dual pipe, full hydraulic brake
双制动阀和双管路，全液压制动

	2
	System  pressure系统压力
	16 (MPa)

	3
	Type of emergency brake紧急制动型号
	Lower pressure alarm brake低压报警制动

	4
	Type of parking brake停车制动型式
	Electric control brake电控制动

	Oil Capacity油量

	1
	Fuel(diesel)柴油
	423(L)

	2
	Engine oil发动机机油
	32(L)

	3
	Oil for converter and gear box双变用油
	38(L)

	4
	Oil for hydraulic system液压系统用油
	300(L)

	5
	Oil for driving axles（F/R）驱动桥用油（前桥/后桥）
	51(L) for each



980H装载机配置表
	序号
	名    称
	型号
	数量
	厂    家
	产地

	1
	发动机
	QSM11-C290
	1
	西安康明斯
	中国

	2
	变速器
	4WG2604646054110
	1
	ZF
	进口

	3
	驱动桥
	前桥4474 054 250
	1
	ZF
	进口

	
	
	后桥4474 054 251
	1
	ZF
	进口

	4
	轮胎
	26.5-25-20PR L-3
	4
	三角轮胎
	中国

	5
	转向器
	150-1084/101-5TX-315-E
	1
	DANFOSS
	进口

	6
	限位阀
	XF-B6
	1
	浙江临海
	中国

	7
	转向油泵:
	PB360A367DRZA17-6/P124ANSZA20
	1
	泊姆克
	进口

	8
	转向油缸
	Z75H.10.5
	1
	常林
	中国

	
	
	Z75H.10.14
	1
	常林
	

	9
	制动系统
	980H.9C
	1
	MICO
	进口

	10
	工作液压系统
	980H.14C
	1
	常林
	中国

	11
	工作液压油泵: 
	P360A367(DRPAA)ZA15-6/P124A082DXZA12-85
	1
	泊姆克
	进口

	12
	多路换向阀
	GD40-00
	1
	高宇
	中国

	13
	先导阀
	CRV-00（W2）
	1
	高宇
	中国

	14
	动臂油缸:
	Z75H.14.20
	2
	常林
	中国

	15
	转斗油缸:
	Z75H.14.21
	1
	常林
	中国

	16
	空调
	GQT-314
	1
	河南豫新
	中国




[image: 2.jpg]
image3.jpeg




image1.png
P EfE LEEEREZHRAR

SINOMACH INTERNATIONAL EQUIPMENT COMPANY LIMITED




image2.jpeg




