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918 WHEEL LOADER SPECIFICATIONS
· [bookmark: _GoBack]Equipped with reliable  Cummins or Chinese Luotuo engine
· 2 forward & 2 reverse power shift transmission
· Combined seal cylinder obtains high seal performance and more reliability

	· Overall Dimension

	1
	Length(with bucket on ground) 整机长度（铲斗放置地面）
	5880 (mm)

	2
	Width(to outside of wheels) 整机宽度（轮胎外沿）
	2060 (mm)

	3
	Bucket width铲斗宽度
	2110(mm)

	4
	Height(To the top of the cab) 高度（到驾驶室顶）
	2820 (mm)

	5
	Wheel base轴距
	2350 (mm)

	6
	Tread轮距
	1500 (mm)

	7
	Min. ground clearance最小离地间隙
	320(mm)

	Main Technical Specification

	1
	Rated load额定载重
	2000(Kg)

	2
	Operating weight操作重量
	6000KG

	3
	Rated bucket capacity额定斗容
	1.1(m3)

	4
	Max. breakout force最大掘起力
	         60kN

	5
	Max. dump clearance最大卸载高度
	2750(mm)

	6
	Dump reach卸载距离
	920(mm)

	7
	Dump angle at any position任意位置卸载角
	≥450

	8
	最大牵引力
	48KN

	9
	最大爬坡能力
	25°

	10
	Min. turning radius最小转弯半径

	
	(1) Outside of bucket铲斗外沿
	4650(mm)

	
	(2)Center of rear wheel后轮胎中心
	 4420(mm)

	11
	Pivot angle frame铰接角
	±380

	12
	Lifting time of bucket铲斗举升时间
	≤4.5(sec.)

	13
	Lowering time of bucket铲斗下降时间
	≤3. (sec.)

	14
	Dumping time翻斗时间
	≤1(sec.)

	15                                                     
	Traveling speed(Km/h)，2 forward and 2 reverse行驶速度，前2后2档位

	
	(1) 1st gear forward前进一档
	10

	
	(2) 2nd gear forward前进二档
	27

	
	(3) 1st gear reverse后退一档
	10

	
	(3) 2nd gear reverse后退二档
	27

	Diesel engine发动机

	1
	Model型号
	Chinese  LUOTUO LR4B3-G92X2A engine                                              

	2
	Type形式
	Direct injection. Natural Aspirate. Water cooling
直喷，自然吸气，水冷

	3
	Rated output额定功率
	60 (kW)

	4
	Rated speed额定转速
	2400(r/min)

	5
	max torque 
最大扭矩
	286N.m/1600-1800

	6
	Starting type启动形式
	Electric电启动

	7
	Voltage of starting motor
启动电压
	24V

	8
	Inter-bore of cylinder/stroke 
缸径×行程
	108×120

	9
	Total exhaust of cylinder
总排气量
	4.58L

	10
	Compression ratio压缩比
	17∶1

	11
	method of lubrication
润滑方式
	Pressure and splash compound 
压力与飞溅复合式

	12
	Min. specific fuel consumption燃油消耗率
	≤242g/kw.h

	13
	机油消耗率
	≤1.6g/kw.h

	Transmission System变速系统

	(一)Torque Converter变矩器

	1
	Model型号
	Jingyi brand

	2
	Type形式
	3-elements.single stage三相单级

	3
	Torque ratio变矩比
	3.06

	4
	Cooling type冷却形式
	Pressure oil circulating压力油循环

	5
	Oil pressure出口油压
	0.245~0.343MPa

	(二)、Transmission case变速箱

	1
	Model型号
	Jingyi

	2
	Type形式
	Mechanical control Fixed shaft-power shift
机械操纵定轴式动力换挡

	3
	Gearbox pump变速油泵
	CBGj1025齿轮泵（左）

	4
	clutch oil pressure
离合器油压
	1.46~1.86MPa

	5
	Transmission gear and ratio 
变速
档位及速比
	1st gear forward前进一档
	2.9862

	
	
	2nd gear forward前进二档
	0.6829

	
	
	1st gear reverse后退一速
	2.508

	
	
	2nd gear reverse后退二速
	0.599

	(三)、Axle and Tire桥和轮胎

	1
	Type of main reducer
主传动形式
	spiral bevel gear, single stage
单级螺伞锥齿轮

	2
	Gear ratio of main reducer
主传动速比
	5.83

	3
	Type of final reducer终传动形式
	Single stage planetary单级行星轮

	4
	Gear of ratio of final reducer终传动速比
	4.4

	5
	Gear ratio总速比
	32.66

	6
	Size of tire轮胎型号
	16/70-20

	7
	Tire pressure轮胎压力
	2.45kpa

	Working Device Hydraulic System工作液压系统

	1
	Model of oil pump工作油泵型号
	CBGJ2063

	2
	System pressure系统压力
	160(kgf/cm2)

	3
	Model of distribution valve分配阀型号
	ZS1-L20E-T-20

	4
	Priority-valve优先阀型号
	YX2-F160L-N7

	5
	(D*L)Dimension of lifting cylinder 举升油缸尺寸
	2-Ф80*45*530(mm)

	6
	(D*L)Dimension of tilting cylinder翻斗油缸尺寸
	Ф100*60*380(mm)

	Steering  System转向系统

	1
	Type
形式
	Middle articulated frame. Full-hydraulic Steering
车架铰接，全液压转向

	2
	Model of steering gear转向器型号
	BZZ-320

	3
	System pressure系统压力
	180(kgf/cm2)

	4
	Dimension of steering cylinder转向油缸规格
	Ф63*35*300(mm)

	Brake System制动系统

	1
	Type of traveling  brake 行车制动形式
	Assisted oil.4 wheel brake气顶液四轮制动

	2
	Air pressure制动气压
	5.88-7.85(kgf/cm2)

	3
	Type of parking brake停车制动形式
	Flexible shaft control Clamp brake
软轴操纵夹钳式制动器

	Oil Capacity油量

	1
	Fuel(diesel)燃油
	100(L)

	2
	Engine lubricating oil机油
	16(L)

	3
	Oil for converter and gear box变速箱油
	28(L)

	4
	Oil for hydraulic system液压油
	100(L)

	5
	Oil for driving axles（F/R）前后驱动桥油
	2x10(L)

	6
	Oil for brake制动液
	3(L)
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