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ZG012S技术规格Technical specification
	技术规格Specifications
	单位Unit
	参数Parameter

	基本参数Basic parameter

	整机质量Machine weight
	kg
	1200

	标配斗容Rated bucket capacity
	m3
	0.022

	标准斗宽Width of bucket
	mm
	360

	Overall length总长（运输状态）
	mm
	3025

	Overall width总宽（运输状态）
	mm
	830/1000

	Overall height总高（运输状态）
	mm
	2245

	Width of undercarriage履带宽度(车宽）
	mm
	830/1000

	Length of track履带长度
	mm
	1335

	Width of track履带板宽度
	mm
	180

	Track gauge履带轴距
	mm
	650/820

	Height between undercarriage and ground

最小离地间隙
	mm
	102

	Height between platform and ground

平衡重离地高度（配重)
	mm
	375

	Platform tail turning radius尾部回转半径
	mm
	700（840）

	Arm length斗杆长度
	mm
	890

	Boom length动臂长度
	mm
	1450

	性能参数Performance parameter

	发动机Engine model
	
	KUBOTA D782

	发动机额定功率Engine power
	kW/rpm
	9.8/2300

	排放Emission
	
	EPA Tier 4 Final/Europe Stage V

	爬坡能力Max. Grade ability
	
	25°

	斗杆最大挖掘力Max. digging force of arm
	kN
	5.4

	铲斗最大挖掘力Max. Digging force of bucket
	kN
	10.4

	行驶速度Traveling speed
	km/h
	2.0/3.5

	平台回转速度Slewing speed of platform
	rpm
	11

	液压系统流量Hydraulic system flow
	L/min
	18.4

	作业参数Operating parameter

	最大挖掘高度Max.digging height
	mm
	2980

	最大挖掘深度Max.digging depth
	mm
	1860

	最大垂直挖掘深度Max.vertical digging depth
	mm
	1550

	最大挖掘半径Max.digging radius
	mm
	3390

	最大地面挖掘半径Max.digging radius on ground level
	mm
	3340

	最大卸载高度Max.dumping height
	mm
	2130

	最小回转半径Min.slewing radius
	mm
	1335

	推土铲最大提升高度Max. lifting height of dozers
	mm
	220

	推土铲最大切土深度Max. depth of cut for dozers
	mm
	188

	转向头向左转角度Boom swing angle left
	°
	57

	转向头向右转角度Boom swing angle right
	°
	61

	加注容量Tank capacity

	燃油箱容量Fuel tank capacity
	L
	10

	液压油箱容量Hydraulic oil tank capacity
	L
	16.3

	冷却系统Cooling system
	L
	3.1

	发动机机油Engine lubricating oil
	L
	3.8
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属具管路：标配，实现管路单双向切换功能。

Attachment Pipeline：AUX1 is Standard, Single and double direction switching.

选配属具：机械快换，破碎锤，拇指夹等属具。

Optional Attachment：Mechanical Coupler，Hammer breaker，Thumb bucket.

动臂偏摆：向左57°，向右61°，实现挖墙脚作业。

Deflection Boom：57°Left，61°right.

底盘变幅：830~1000mm。

Width adjustable undercarriage: 830~1000mm.

推土铲：可根据底盘伸缩的范围调整推土铲宽度.

Foldable Dozer blade: The width of the Dozer blade can be adjusted according to the telescopic range of undercarriage. 

可折叠防护架：方便运输和室内操作

Foldable Seat Frame: Convenient for transportation and indoor operation.

后开启座箱：开启角度80°，维护保养便利。

Open the Engine Cover at 80°:The engine cover tilt-up operation exposes most of the engine—providing easier access to components.

座椅：可前后滑动，满足不同用户对空间的需求。

Sliding Seat: Can slide forward and backward to meet the space needs of different users

