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1、产品简介Introduction：
东风康明斯大功率发动机，动力强劲、高效节能、可靠耐用；先进的负流量液压系统，操作舒适，作业效率高，性价比极佳；全功率控制，四种功率模式适应不同工况；可靠、精准的燃油喷射系统，燃烧更加充分，效率更高；有限元分析技术，保证了结构件的可靠性和稳定性。
CUMMINS high-power engine, strong power, high efficiency and energy saving, reliable and durable; advanced negative flow hydraulic system, comfortable operation, high operating efficiency, excellent cost performance; full power control, four power modes to adapt to different working conditions; reliable and accurate fuel injection system, combustion is more adequate, higher efficiency; finite element analysis technology to ensure the reliability and stability of the structural components.
2.性能特点Characteristics：
(1)东风康明斯大功率发动机，动力强劲，燃油消耗低，可靠性高；
CUMMINS high power engine, strong power, low fuel consumption, high reliability.
(2)新型的液压系统，大排量主泵，大流量主阀，通流面积大，压力损失小，流量分配更合理，协调性更好，操作更加轻松；
New hydraulic system, large displacement main pump, large flow main valve, large flow area, small pressure loss, more reasonable flow distribution, better coordination and easier operation.
(3)配备大缸径油缸，优化各关键铰点的布置，提升整机挖掘力，设置自动增压功能，随着负载的增加自动增加挖掘力；
Equipped with large bore cylinders, optimizing the arrangement of each key hinge point to enhance the whole machine's digging force, and setting the automatic booster function to automatically increase the digging force with the increase of load.
(4)针对极端恶劣的矿山作业工况，标配重载强化型动臂、矿山专用短斗杆和大容量岩石铲斗，标配加长加宽型重载底盘，工作稳定性好；
For the extreme mining conditions, it is equipped with heavy-duty reinforced boom, mine-specific short bucket bar and large-capacity rock bucket, and a longer and wider heavy-duty chassis for good working stability.
(5)新一代控制系统，根据工况需要智能调节液压吸收功率，最优化的系统匹配，保证整机的综合性能充分发挥；
A new generation of control system, according to the working conditions need to intelligently adjust the hydraulic absorption power, optimized system matching, to ensure that the comprehensive performance in full play.
(6)配备高分辨率、高亮度的 8 寸彩色防炫目监控仪表，智能电子监控系统，具备整车保养信息提示、故障的自诊断和报警等多种功能；
Equipped with high-resolution, high-brightness 8-inch color anti-glare monitoring instrument, intelligent electronic monitoring system, with the vehicle maintenance information prompts, self-diagnosis of faults and alarms and other functions.
(7)采用安全可靠的新型驾驶室，全新注塑内饰件，美观大方，宽敞舒适， 配置全自动冷暖空调；
Adopting safe and reliable new cab, brand-new injection molding interior parts, beautiful and generous, spacious and comfortable, equipped with full-automatic cold and warm A/C.
(8)具备防滑安全、过热保护、运动件保护和驾驶室防护设计，安全性高；
With anti-skid safety, overheating protection, moving parts protection and cab protection design, high safety.
(9)人性化的集中、远程式地面维护设计，保养更轻便；
Humanized centralized and remote ground maintenance design, lighter maintenance.




3．技术规格Technical specification	
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	名   称ITEM
	单   位UNIT
	技术规格
Technical specifications

	
	
	GE365D

	操作重量Operating weight
	kg
	35000

	功率 Rated power
	kW/rpm
	241/2000

	标准斗容 
Rated bucket capacity
	
	m3
	1.7

	总长 Overall length
	A
	mm
	10921

	总宽（600mm履带）
Overall width（600mm track）
	B
	mm
	3280

	总高 Overall height
	C
	mm
	3546

	转台宽度 Platform width
	D
	mm
	3060

	驾驶室离地高 
Height of cabin
	E
	mm
	3145

	配重离地间隙 Ground clearance of counterweight
	F
	mm
	1193

	发动机罩高
Engine cover height
	G
	mm
	2640

	最小离地间隙
Min. ground clearance
	H
	mm
	471

	转台尾端长度
Tail length
	I
	mm
	3440

	尾端回转半径
Turning radius of turntable
	I’
	mm
	3512

	履带轴距
Wheel base of track shoe
	J
	mm
	4030

	底盘长度
Length of chassis
	K
	mm
	4950

	底盘宽度
Width of chassis
	L
	mm
	3280

	履带轨距
Track shoe gauge
	M
	mm
	2680

	标准履带宽度
Standard track width
	N
	mm
	600

	最大牵引力
Max. traction
	
	kN
	345

	行走速度（高/低）
Traveling speed （H/L）
	
	km/hr
	4.7/2.5

	回转速度
Swing speed
	
	rpm
	9.2

	爬坡能力 Gradeability
	
	Degree(%)
	35（70%）

	接地比压 
Ground pressure
	
	Kgf/cm2
	0.724














4.工作范围 Working range
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	类    别 ITEM
	6.2m动臂，2.65m斗杆，1.7m3铲斗
6.2m Boom，2.65m Stick，1.7m3 Bucket

	
	GE365D

	最大挖掘半径
Maximum digging radius
	A
	10233 mm

	地面最大挖掘半径
Ground maximum digging radius 
	A’
	10028 mm

	最大挖掘深度
Maximum digging depth
	B
	6536 mm

	地面最大挖掘深度（2438mm水平）
Ground maximum digging depth
	B’
	6331 mm

	最大垂直挖掘深度
Maximum vertical digging depth
	C
	4758 mm

	最大挖掘高度
Maximum digging height
	D
	9617 mm

	最大卸载高度
Maximum dumping height
	E
	6666 mm

	最小前部回转半径
Min. front turning radius
	F
	4256 mm

	铲斗挖掘力
Bucket digging force
	ISO
	225 kN

	斗杆挖掘力
Stick digging force
	ISO
	182 kN



5. 发动机性能参数 Engine specifications
	发动机型号 Model
	
	康明斯 CUMMINS
6LTAA8.9-C325

	规格参数
Specifications
	型  式 Type
	
	4冲程，6缸，直列式，直喷，涡轮增压
4 Stroke，6 Cylinder in line ，direct injection， turbocharged

	
	冷却方法 Cooling type
	
	水冷 Water cooled

	
	缸径×行程 Bore diameter × stroke
	mm
	114×145

	
	活塞排量Displacement
	L
	8.9

	
	功率rated power
	kW/rpm
	241/2000

	
	最大扭矩 Max. torque
	N.m/rpm
	1400/1400

	
	额定油耗率 
Rated diesel consumption
	g/kW.h（rpm）
	194（1200）

	
	发动机机油油量
Engine oil capacity
	L
	18.1-28.5

	
	启动马达Starter
	
	24V 8.5kW

	
	发电机Generator
	
	28V 70A

	
	蓄电池 Battery
	
	2×12V×120Ah



6. 主要部件配置 Main configuration
	部件         机型
	GE365D

	
	

	排放等级 Emission
	国二 Stage Ⅱ

	发动机 Engine
	东风康明斯 CUMMINS
6LTAA8.9-C325

	主泵Main pump
	韩川 FLUTEK
FP3V180DTP

	主控阀 Main valve
	[bookmark: _GoBack]恒立 INLINE
HVME400B

	回转马达 Slewing motor
	韩川 FLUTEK
F5X180CHB

	行走马达 Travelling motor
	纳博 NABTESCO
GM75VA
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