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[bookmark: _Toc6159]vehicle parameter table
	CHL5310JSQD6 Type Truck Crane Transport Vehicle for Steel Plant

	Vehicle name:
	truck with loading crane
	[image: IMG_256]

	class of vehicle ：
	truck with loading crane
	

	Vehicle model:
	CHL5310JSQD6
	

	exemption ：
	deny
	

	fuel oil ：
	yes
	

	exemption from conscription ：
	deny
	

	environmental protection ：
	deny
	

	Chinese brand:
	Sinomach Heavy Industry brand
	manufacturer ：
	Sinomach Heavy Industry Group Changlin Co., Ltd.

	engine type ：
	L9NS6B360
	engine power ：
	265/360

	engine displacement ：
	8900
	Engine manufacturer:
	Dongfeng Cummins Engine Co., Ltd.

	Chassis model:
	Dongfeng Tianlong 1130
	Fuel type:
	diesel oil

	Dimensions (length/width/height):
	12000×2550×3525(mm)
	Trunk (length/wide/height):
	8400×2430×600(mm)

	gross mass （Kg）：
	31000 
	load utilization factor:
	1.61 

	Preparation mass (Kg):
	14260(Kg)
	Rated load capacity (Kg):
	16610(Kg)

	ABS ：
	have
	Front passenger(s):
	2 

	Approach angle/Departure angle:
	22/7 
	Front/rear suspension (mm):
	1500/2700(mm)

	wheel base （mm）：
	2050+4400+1350(mm)
	axle weight ：
	

	number of axles ：
	3 
	Maximum speed (km/h):
	89

	oil wear ：
	30.74
	Number of spring tabs:
	12/10

	Number of wheels:
	12
	tyre size ：
	11.00R20

	Chassis standard: National VI


Note: The vehicle parameters are based on actual measurements.



This model features a 6.3-ton folding arm specifically designed for steel mill material handling, with a maximum load capacity of 16.5 tons, making it the highest-capacity model available in the current lineup.
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(1) Rotary device
The planetary reducer is used to reduce the speed, the rotation is more stable, the rotation angle is 360 degrees, and there is no dead point.
(2) Support leg system
horizontal support leg hydraulic cylinder
The front leg of the crane adopts an extended span to enhance stability, with a full extension span of 5.7 meters.
oil cylinder of front vertical support leg
The standard hydraulic support leg can adapt to various chassis heights.
posterior leg
The standard configuration features fixed rear outriggers for normal operation. An optional hydraulic rear outrigger can be installed to enhance overall stability, making it suitable for more complex and challenging conditions.

(3) Lifting Arm System
The hexagonal cross-section is adopted, and the lateral stability and arm cylinder stiffness are greatly improved compared with the traditional quadrilateral. One basic arm, three telescopic arms, double-stage hydraulic telescopic cylinder, three and four arms extend synchronously.
   
(4) Control System
crane control system
The crane is controlled by the main valve, which is located at the seat.
support leg control system
The support leg is independently controlled by the leg valve to prevent misoperation and enables bilateral manipulation.

(5) Safety devices
The standard configuration includes a height limit switch and over-rolling alarm device to provide maximum protection for the working equipment.
Optional high-power LED working lights are available for low-light conditions or nighttime operations.
Optional torque limiter for enhanced safety and reliability in the working environment.
1

image3.jpeg




image4.jpeg




image5.jpeg




image6.jpeg




image7.jpeg
SNpERED
)§136398358





image1.jpeg
PR
PN EiET




image2.png




