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GE150H SPECIFICATIONS
[image: C:\Users\XC\Desktop\图片\GE150.png]
[image: ]

[bookmark: _Hlk19554108]1.产品简介 Introduction：
康明斯电喷发动机(符合三阶段排放法规)，动力强劲、高效节能、可靠耐用；先进的负流量液压系统，操作舒适，作业效率高，性价比极佳；全功率控制，四种功率模式适应不同工况；可靠、精准的燃油喷射系统，实时控制喷油量，使燃烧更加充分，燃油效率更高；全三维建模和有限元分析技术，保证了结构件的可靠性和稳定性。
[bookmark: _Hlk19554142]Cummins EFI engine (conforming to Ⅲ-stage emission regulations), powerful, energy efficient, reliable and durable; advanced negative flow hydraulic system, comfortable operation, high operating efficiency, excellent cost performance; full power control, four power modes to adapt to different work; reliable and accurate fuel injection system, real-time control of fuel injection, making combustion more complete, fuel efficiency; full 3D modeling and finite element analysis technology to ensure the reliability and stability of structural parts.
[bookmark: _Hlk19554158]2.性能特点 Characteristics：
[bookmark: _Hlk19554322](1)康明斯新一代大功率电喷发动机，动力强劲，燃油消耗低，可靠性高；
CUMMINS new generation of high-power EFI engines with strong power, low fuel consumption and high reliability.
(2)新型的川崎液压系统，大排量主泵，大流量主阀，通流面积大，压力损失小，流量分配更合理，协调性更好，操作更加轻松；
New KAWASAKI hydraulic system, large displacement main pump, large flow main valve, large flow area, small pressure loss, more reasonable flow distribution, better coordination and easier operation.
(3)配备大缸径油缸，优化各关键铰点的布置，提升整机挖掘力，设置自动增压功能，随着负载的增加自动增加挖掘力；
Equipped with large bore cylinders, optimizing the arrangement of each key hinge point to enhance the whole machine's digging force, and setting the automatic booster function to automatically increase the digging force with the increase of load.
(4)大排量回转马达、大速比的回转齿轮设计，回转启动力矩更大，回转制动效果更佳；
Large-displacement slewing motor, large-ratio slewing gear design, greater slewing starting torque, better slewing braking effect.
(5)针对恶劣的作业工况，标配强化型动臂、斗杆和铲斗，标配加长加宽型重载底盘，优化箱形结构，工作稳定性好；
For severe working conditions, it is equipped with reinforced boom, stick and bucket, standard long and wide heavy-duty chassis, optimized box structure, and good working stability.
(6)新一代控制系统，根据工况需要智能调节液压吸收功率，最优化的系统匹配，保证整机的综合性能充分发挥；
New generation control system intelligently adjusts the hydraulic absorption power according to the working conditions, and optimizes the system matching to ensure the full performance.
(7)配备高分辨率、高亮度的 8 寸彩色防炫目监控仪表，智能电子监控系统，具备整车保养信息提示、故障的自诊断和报警等多种功能；
Equipped with high-resolution, high-brightness 8-inch color anti-glare monitoring instrument, intelligent electronic monitoring system, with vehicle maintenance information prompts, fault self-diagnosis and alarm and other functions;
(8)采用安全可靠的新型驾驶室，全新注塑内饰件，美观大方，宽敞舒适，配置全自动冷暖空调；
Adopting safe and reliable new cab, brand-new injection molding interior parts, beautiful and generous, spacious and comfortable, equipped with full-automatic A/C.
(9)整机防滑安全设计、过热保护设计、运动件保护设计、驾驶室防护设计，安全性高；
Anti-skid safety design of the whole machine, overheating protection design, moving parts protection design, cab protection design, high safety.
(10)人性化的集中、远程式地面维护设计，保养更轻便；
Humanized centralized and remote ground maintenance design, lighter maintenance
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	名   称 ITEM
	单   位
UNIT
	技术规格
Technical specifications

	
	
	GE150H

	操作重量 Operating weight
	kg
	13890

	功率 Power
	kW/rpm
	86/2200

	标准斗容 
Rated bucket capacity
	
	m3
	0.6

	总长 Length
	A
	mm
	7762

	总宽（500mm履带）
Width（500mm track）
	B
	mm
	2510

	总高 Height
	C
	mm
	2983

	转台宽度 Turntable width
	D
	mm
	2510

	驾驶室离地高
Height of cabin
	E
	mm
	2825

	配重离地间隙 Ground clearance of counterweight
	F
	mm
	915

	发动机罩高 
Engine cover height
	G
	mm
	2243

	最小离地间隙
Min. ground clearance
	H
	mm
	416

	转台尾端长度 Tail length
	I
	mm
	2306

	尾端回转半径
Turning radius of turntable
	I’
	mm
	2387

	履带轴距 
Wheel base of track shoe
	J
	mm
	3010

	底盘长度
Length of chassis
	K
	mm
	3751

	底盘宽度
Width of chassis
	L
	mm
	2490

	履带轨距 
Track shoe gauge
	M
	mm
	1990

	标准履带宽度
Standard track width
	N
	mm
	500

	最大牵引力
Max. traction
	
	kN
	122

	行走速度（高/低）
Traveling speed （H/L）
	
	km/hr
	5.4/3.3

	回转速度
Swing speed
	
	rpm
	13.1

	爬坡能力 Gradeability
	
	Degree(%)
	35（70%）

	接地比压 
Ground pressure
	
	Kgf/cm2
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[bookmark: _Hlk19554543]4.工作范围 Working range
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	类    别 ITEM
	4.6m动臂，2.491m斗杆，0.6m³铲斗
4.6m Arm，2.491m Stick，0.6m³Bucket

	
	GE150H

	最大挖掘半径
Maximum digging radius
	A
	8335 mm

	地面最大挖掘半径
Ground maximum digging radius 
	A’
	8203 mm

	最大挖掘深度
Maximum digging depth
	B
	5491 mm

	地面最大挖掘深度（2438mm水平）
Ground maximum digging depth
	B’
	5288 mm

	最大垂直挖掘深度
Maximum vertical digging depth
	C
	4826 mm

	最大挖掘高度
Maximum digging height
	D
	8679 mm

	最大卸载高度
Maximum dumping height
	E
	6174 mm

	最小前部回转半径
Min. front turning radius
	F
	2605 mm

	铲斗挖掘力
Bucket digging force
	ISO
	100 kN

	斗杆挖掘力
Stick digging force
	ISO
	68 kN



[bookmark: _Hlk19554799]5. 发动机性能参数 Engine specifications
	规格参数
Specifications
	型号 Model
	
	康明斯 CUMMINS
QSF3.8-C115

	
	型式 Type
	
	四缸直列、四冲程涡轮增压
Four-cylinder in-line, four-stroke turbocharger

	
	排放 Emission
	
	国Ⅲ National Ⅲ

	
	冷却方式 Cooling method
	
	水冷 Water cooled

	
	缸径×行程 Bore diameter × stroke
	mm
	102×125

	
	气缸排量 Displacement
	L
	3.76

	
	额定功率 Rated power
	
	86kW/2220rpm

	
	最大扭矩(1400r/min) Max. torque
	N.m
	470

	
	机油量 Engine oil capacity
	L
	17-26

	
	额定油耗率 Rated diesel consumption
	g/KW.h
	199（1600rpm）

	
	起动马达 Starter
	
	24V/4.8KW

	
	发电机 Generator
	
	28V/70A



[bookmark: _Hlk19555277]6. 主要部件配置 Main configuration
	部件          机型
	GE150H

	
	

	排放等级 Emission
	国三 National Ⅲ

	发动机 Engine
	福田康明斯 CUMMINS
QSF3.8-C115

	主泵 Main pump
	日本川崎KAWASAKI
K7V63DTP

	主控阀 Main valve
	日本川崎KAWASAKI
KMX13RB

	回转马达 Swing motor
	日本川崎 KAWASAKI
M5X80CHB

	行走马达Travelling motor
	艾迪 EDDIE
FTM22A
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