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ZG3210-9C HYDRAULIC EXCAVATOR SPECIFICATIONS
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1.产品简介 Introduction：
配备康明斯发动机，动力强劲、高效节能、可靠耐用；先进的负流量液压系统，操作舒适，作业效率高，性价比极佳；全功率控制，四种功率模式适应不同工况；步进电机精确控制油门，显著降低油耗；全三维建模和有限元分析技术，保证了结构件的可靠性和稳定性。
Equipped with CUMMINS engine, strong power, high efficiency, energy saving, reliable and durable; advanced negative flow hydraulic system, comfortable operation, high operating efficiency, excellent cost performance; full power control, four power modes to adapt to different working conditions; stepper motor accurately controls the throttle , Significantly reduce fuel consumption; full 3D modeling and finite element analysis technology to ensure the reliability and stability of structural parts.

2.性能特点 Characteristics：

(1)配备康明斯发动机，高耐负荷、大马力输出，可靠性高、油耗低，显著降低使用和维护成本。
Equipped with CUMMINS engine, high load resistance, high horsepower output, high reliability, low fuel consumption, significantly reduce the use and maintenance costs

(2)采用先进的负流量液压系统，系统稳定性、可靠性更好,复合动作速度更快，作业效率更高。
Advanced negative flow hydraulic system is adopted, which has better system stability and reliability, faster compound action speed and higher operating efficiency.
(3)机动灵活，多种铲斗、破碎器选配，可广泛应用于市政、道路、管网、厂矿企业等施工场地。
Flexible maneuvering, a variety of buckets, crusher options, can be widely used in municipal, roads, pipe networks, factories and mining enterprises and other construction sites.
(4)高强度的加强型箱型侧梁和X型中框架，高可靠性的拖链轮、支重轮，能承受超大负荷引起的冲击。
High-strength reinforced box-type side beams and X-shaped middle frames, high-reliability towline wheels and track rollers, can withstand the impact caused by excessive loads.

(5)采用含油树脂垫片和高密度铜基子润滑轴套，低摩擦，耐磨损。
Low friction and wear-resistant with oil-containing resin gaskets and high-density copper-based sub-lubricated bushings.
(6)智能化的电子监控系统，实时监测，自诊断故障报警、维护保养信息提示。
Intelligent electronic monitoring system, real-time monitoring, self-diagnostic fault alarm, maintenance information prompts.
(7)符合人体工程学的司机室，宽敞安全，低噪音，视野和通风条件更好。
Ergonomic driver's compartment, spacious and safe, low noise, better visibility and ventilation.
3、Overall Dimension整机尺寸
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	名   称ITEM
	单   位UNIT
	技术规格Specifications

	
	
	ZG3210-9C

	操作重量Operating weight
	kg
	21000

	标配斗容(加强斗)

Rated bucket capacity
	
	m3
	1.0

	总长 Overall length
	A
	mm
	9660

	总宽（600mm履带）
Overall width（600mm track shoe）
	B
	mm
	2800

	总高 Overall height
	C
	mm
	3030

	转台宽度Trunable width
	D
	mm
	2700

	驾驶室离地高Cabin height
	E
	mm
	2958

	配重离地间隙 
Groundclearance of counterweight
	F
	mm
	1025

	发动机罩高
Engine cover height
	G
	mm
	2338

	最小离地间隙
Min. ground clearance
	H
	mm
	470

	转台尾端长度
Tail length
	I
	mm
	2800

	尾端回转半径
Turning radius of turnable
	I’
	mm
	2800

	履带轴距 Wheel base of track shoe
	J
	mm
	3370

	底盘长度 Chassis length
	K
	mm
	4160

	底盘宽度 Chassis width
	L
	mm
	2800

	履带轨距 Track shoe gauge
	M
	mm
	2200

	标配履带宽度 
Standard track shoe width
	N
	mm
	600

	最大牵引力 Max. traction
	
	kN
	194

	行走速度（高/低）
Travelling speed (H/L)
	
	km/hr
	5.5/3.6

	回转速度 Swing speed
	
	rpm
	12

	爬坡能力 Grade ability
	
	Degree(%)
	35（70%）

	接地比压 Ground pressure
	
	kgf/cm2
	0.47


4、工作范围 Working range
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	类    别 ITEM
	5.68m动臂 2.91m斗杆 1.0m³铲斗

5.68m Boom 2.91m Stick 1.0m³ Bucket

	
	ZG3210-9C

	最大挖掘半径
Maximum digging radius
	A
	9953

	地面最大挖掘半径
Ground maximum digging radius 
	A’
	9794

	最大挖掘深度
Maximum digging depth
	B
	6690

	地面最大挖掘深度（2438mm水平）
Ground maximum digging depth
	B’
	6505

	最大垂直挖掘深度
Maximum vertical digging depth
	C
	6104

	最大挖掘高度
Maximum digging height
	D
	9642

	最大卸载高度
Maximum dumping height
	E
	6813

	最小前部回转半径
Min. front turning radius
	F
	3560

	铲斗挖掘力
Bucket digging force
	ISO
	137 kN

	斗杆挖掘力
Stick digging force
	ISO
	102 kN


5. 发动机性能参数 Engine specifications

	规格参数
Specifications
	型号 Model
	
	康明斯 CUMMINS
6B5.9-C150

	
	型式 Type
	
	六缸直列、四冲程
6-cylinder in-line, four-stroke

	
	排放 Emission
	
	国Ⅱ National Ⅱ

	
	冷却方式 Cooling method
	
	水冷 Water cooled

	
	缸径×行程 Bore diameter × stroke
	mm
	102×120

	
	气缸排量 Displacement
	L
	5.883

	
	额定功率 Rated power
	
	112kW（150HP）@1950rpm

	
	最大扭矩Max. torque
	N.m
	614N.m（1500rpm）

	
	机油量 Engine oil capacity
	L
	24

	
	额定油耗率 Rated diesel consumption
	g/ps.hr(rpm)
	208g/ps.hr(1500rpm)

	
	起动马达 Starter
	
	DENSO 24V/4.5KW

	
	发电机 Generator
	
	DELCO 24SI 28V/70A 

	
	蓄电池 Accumulators
	
	2×12V×120Ah


6. 主要部件配置 Main configuration
	部件          机型
	ZG3210-9C

	
	

	排放等级 Emission
	国二 National Ⅱ

	发动机 Engine
	东风康明斯DONGFENG CUMMINS
6B5.9-C150

	主泵 Main pump
	韩川 PNMFK
K3V112DT

	主控阀 Main valve
	恒立 INLINE
HVME270B

	回转马达 Swing motor
	韩川 PNMFK
M5X130CHB

	行走马达Travelling motor
	斗山 DOOSAN
TM40VD


