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GYA6000 沥青稳定土摊铺机        

ASPHALT STABLIZED SOIL  PAVER
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摊铺机用途广泛，可用于市政道路，，中、小型区域工程等等。
东风康明斯电喷发动机, 功率强劲, 可靠性高；低温启动性能好。
行走驱动系统采用原装进口的液压柱塞泵、行星减速机、柱塞马达，可靠性高；闭式控制左右独立驱动方式,保证履带驱动系统运行平稳，可实现灵活转向，转场方便。
左右输分料采用四套独立的全液压传动，料位采用传感器控制，实现输、分料全比例均匀供料。
螺旋布料器叶片和输料底板等部位均选用耐磨钢板,可靠性高,使用寿命长。
配置振捣系统无级调速，保证摊铺密实度。
电加热系统、操作方便、加热速度快且均匀
Uses for municipal roads, expressway and small-area projects and so on.
Adopting Cummins electronic-injection engine, strong power, high reliability and excellent performance on paving.
Original imported hydraulic plunger pomp, planetary reduction gear, plunger motor on travel drive system, high reliability, independent drive type under closed control, good stability and flexibility of changing working site.
Independent hydraulic system, sensor control to material level, Conveyor and auger in proportional collaboration.
The blade and under-plate made of high wearable alloy material or imported wearable armor plate, high-durability.
Tamping system with stepless speed regulation, perfect compactioness effect.
Electric heating system, convenience for operation and fast heating.




	项目Item
	单位/unite
	GYA6000

	基本摊铺宽度/Basic paving width
	m
	2.5

	伸缩范围/extensive rang
	m
	2.5~4.5

	最大摊铺宽度/Max. paving width
	m
	6.0

	最大摊铺厚度/Max. paving thickness
	mm
	300

	摊铺工作速度/working speed
	m/min
	0-20

	行驶速度/ Running speed
	km/h
	0-3.0

	理论生产率 /Theoretical productivity
	t/h
	600

	料斗容量/Hopper capacity
	t
	14

	爬坡能力/Grade.ability
	%
	≥20

	平整度误差(纵波)Leveling Tolerance(wave)
	mm/3m
	2

	横波误差Transverse wave Error
	%
	±0.02

	拱度调节范围Arch degree adjusting range
	%
	-1～+3

	生产厂商 manufacturer
	　
	康明斯/Cummins

	型号model
	　
	QSB5.9-C190

	额定功率 Rated power
	kW
	133

	排放标准Emission standard
	　
	国3 /Stage Ⅲ

	振捣频率/tamping frequency
	HZ
	25

	振捣振幅/vibrating amplitude
	mm
	5

	加热方式 Heating type
	　
	电加热 electric

	整机尺寸/Machine Dimension
	mm
	6610x2690x3730/2890

	总质量/Overall mass
	t
	18.5


      因产品改进技术参数如果变动恕不通知

       With the improvement of product, the design or specification are subject to change without notice
主要性能  FEATURE OF MACHINE








主要尺寸   Main Dimension





主要技术参数 Main Technical Parameters








