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GYS122J单钢轮全液压振动压路机
GYS122J FULL HYDRAULIC SINGLE DRUM VIBRATORY ROLLER
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适用范围 Application
适用于高等级公路、大坝、铁路、机场等大型工程基础的压实，可碾压砂土、砾石、碎石、岩石填方等非粘性材料及半粘性材料
Suitable for compaction of large-scale engineering foundations such as high-grade roads, dams, railways, airports, etc., non-stick materials and semi-viscous materials such as sand, gravel, gravel, rock fill, etc.

性能特点:Performance characteristic
1. 液压前后轮驱动，多档无级变速，爬坡能力强；
Hydraulic front drum and rear wheel drive, multi-speed stepless speed change, strong climbing ability
2. 液压振动，电控延时起振，激振力大，压实性能好；
Hydraulic vibration, electronically controlled delay start, high excitation force, good compaction performance
3. 液压转向，铰接式车架，转向轻便灵活，操作轻便灵活；
Hydraulic steering, articulated frame, light and flexible steering, light and flexible operation
4. 配置压路机专用驱动桥，驱动性能优越；
Equipped with a dedicated drive axle for the roller, which has superior drive performance.
5. 液压行走制动，电控盘刹停车制动，设有制动释放装置，可供近距离拖行，安全性能好；
Hydraulic travel brake, electric control disc brake parking brake, with brake release device for short-distance towing, good safety performance;
6. 后机罩可大角度翻起，维修保养方便；
The rear hood can be turned up at a large angle for easy maintenance
7. 驱动和振动系统均配置进口国际知名品牌液压元件，性能可靠；
The drive and vibration system are equipped with imported international famous brand hydraulic components, and the performance is reliable.
8.可选配不同花纹轮胎；可选配其它品牌柴油机;标配驾驶室，可选装冷暖空调。可选配凸块式钢轮。
Optional different pattern tires; optional other brands of diesel engines; standard cab, optional air conditioning. Optional bump type steel wheel



技术参数 Technical parameters
	产品型号 Model
	GYS122J

	工作质量Operating weight (kg)
	12000

	振动轮直径Vibratory drum diameter (mm)
	1500

	压实宽度Compaction width (mm)
	2130

	静线载荷Static line pressure
	312 N/cm

	最小离地间隙Min. ground clearance (mm)
	420

	轴距 Wheel base (mm)
	3100

	最小转弯半径 Min. turning radius (mm)
	6400

	[bookmark: _GoBack]理论爬坡能力 Gradeability
	50%

	振动频率Vibratory frequency(Hz)
	30/35

	名义振幅Vibratory amplitude (mm)
	1.9/0.9

	激振力Centrifugal force  (kN)
	280/180

	行驶速度 Travelling speed (km/h)
	(L)0～5.5 ，(F)0～10

	发动机型号 Engine model
	WP4G110E22

	发动机功率/转速 Engine power/speed (kW /rpm)
	82/2200

	外形尺寸（长×宽×高）(mm)
Dimension (Length ×Width × Height)
	6140×2280×3080



主要配置说明 Main configuration
	序号
S/N
	名称
ITEM
	型号
MODEL
	数量
NO.
	生产厂家
MANUFACTURER

	1
	柴油机
Engine
	WP4G110E301
	
	WEICHAI

	2
	振动泵
Vibratory pump
	HPV055
	1
	LINDE

	3
	振动马达
Vibratory motor
	HMF055
	1
	LINDE

	4
	驱动泵
Hydraulic pump
	HPV075
	1
	LINDE

	5
	前驱动马达
Front drive motor
	HMF055
	1
	LINDE

	6
	桥驱动马达
Axle drive motor
	HMV055
	1
	LINDE
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