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液压单驱单钢轮振动压路机系列
HYDRAULIC REAR WHEEL DRIVE SINGLE DRUM VIBRATORY ROLLER SERIES

适用范围 Application
适用于高等级公路、大坝、铁路、机场等大型工程基础的压实，可碾压砂土、砾石、碎石、岩石填方等非粘性材料及半粘性材料
Suitable for compaction of large-scale engineering foundations such as high-grade roads, dams, railways, airports, etc., non-stick materials and semi-viscous materials such as sand, gravel, gravel, rock fill, etc.

性能特点 Characteristic
1. 液压后轮驱动，两档行驶速度；
Hydraulic rear wheel drive, two speeds
2. 液压开式振动，单频双幅电控起振，激振力大，压实性能好；
Open type hydraulic vibration, single frequency and double amplitude electric control, large excitation force, good compaction performance
3. 液压转向，铰接式车架，转向轻便灵活，操作轻便灵活；
Hydraulic steering, articulated frame, light and flexible steering, light and flexible operation
4. 配置压路机专用驱动桥，传动扭矩大，换挡轻便；
Equipped with the special drive axle of the roller, the transmission torque is large, and the shifting is light.
5. 液压行车制动，盘式停车制动，安全可靠；
Hydraulic service brake, disc parking brake, safe and reliable
6. 后机罩可大角度翻起，维修保养方便；
The rear hood can be turned up at a large angle for easy maintenance
7. 液压元件采用国际知名品牌，性能可靠；
Hydraulic components adopt internationally renowned brands with reliable performance
8. 标配驾驶室，可选装冷暖空调；
Standard cab, optional air conditioning
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技术参数 Parameter
	产品型号 
MODEL
	
	GYS161J
	GYS181J
	GYS201J

	工作质量
Operating weight
	kg
	16000
	18000
	20000

	钢轮直径
Drum diameter
	mm
	1550
	1550
	1600

	压实宽度
Compaction width
	mm
	2130
	2130
	2130

	静线压力
Static line Pressure
	N/cm
	370
	415
	460

	振动频率
Vibratory frequency
	Hz
	32
	32
	32

	名义振幅
Vibratory amplitude
	mm
	1.8/0.9
	1.9/1.0
	2.0/1.0

	激 振 力
Centrifugal force
	kN
	325/165
	365/190
	405/220

	行驶速度
Travelling speed
	km/h
	0-6/0-10
	0-6/0-10
	0-6/0-10

	爬坡能力
Gradeability
	%
	30
	30
	30

	发动机型号
Engine model
	
	WP6G160E22
	WP6G175E22
	WP6G175E22

	发动机额定功率/转速 
Rated power/speed
	kW/ rpm
	118/2200
	129/2200
	129/2200

	轮胎规格
Tyre
	
	20.5-25
	20.5-25
	20.5-25

	外形尺寸（长×宽×高）
Dimension （L×W×H）
	mm
	6240×2280×3080
	6240×2280×3080
	6240×2300×3080
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