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GYS22J单钢轮振动压路机
GYS22J SINGLE DRUM VIBRATORY ROLLER
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主要性能:Main features
1、 配置6缸增压具有世界先进水平的发动机，功率储备大，效率高，超低油耗，清洁环保。
Equipped with 6-cylinder supercharger with world-class engine, large power reserve, high efficiency, ultra-low fuel consumption, clean and environmentally friendly 
2、 振动系统配置美国PERMCO齿轮泵和齿轮马达，效率高，质量可靠。
The vibration system is equipped with American PERMCO gear pump and gear motor, with high efficiency and reliable quality.
3、 采用带同步器的压路机专用变速箱，变速换档轻便舒适，性能可靠。
Adopting a special gearbox for the roller with a synchronizer, the shifting shift is light and comfortable, and the performance is reliable.
4、 选配带差速器和钳盘式制动器的驱动桥，牵引力强大，通过性能良好。
Driving axle with differential and caliper disc brakes for powerful traction and good performance
5、 电控起振，操作方便，具有高低振幅两种振动型选择，压实性能优良。
Electric control start-up, easy to operate, with high and low amplitude vibration type selection, excellent compaction performance
6、 具有两套制动系统，行车制动为气顶油钳盘式，停车制动为内涨型鼓式，安全性能好。
With two sets of brake system, the service brake is a gas-top oil tongs disc type, the parking brake is an internal rising drum type, and the safety performance is good.
7、 后罩壳为流线型设计，可大角度起翻，维修保养方便。
The rear cover is streamlined and can be turned up at a large angle for easy maintenance.
8、 整机采用三级减震，减震性能好。
The whole machine adopts three-stage damping and has good shock absorption performance.

  











	规格型号：GYS22J型单钢轮振动压路机

	MODEL: GYS22J Single drum vibratory roller

	主要技术参数    Main parameter 

	1、工作质量 Operating weight
	22000 kg

	2、振动频率 Vibratory frequency
	30 Hz

	3、激振力（大振/小振）Centrifugal force （L/S）
	420/230 kN

	4、振幅（大振/小振）Vibratory amplitude (L/S)
	2.0/1.0 mm

	5、静线压力 Static line pressure
	516 N/cm

	6、工作速度  Travelling speed Ⅰ/Ⅱ/Ⅲ
	2.5/5.0/10.5 km/h WEICHAI
2.7/5.5/11.5 km/h CUMMINS

	7、爬坡能力 Gradeability
	30%

	8、转弯半径（外侧） Min. turning radius
	6500 mm

	9、最小离地间隙 Min. ground clearance
	450 mm

	10、轴距 Wheelbase
	3200 mm

	11、外形尺寸（长×宽×高）Overall dimension
	6240×2320×3080 mm

	12、压轮参数（直径×宽度） Drum dimension
	φ1600×2130 mm

	13、驱动形式 Drive type
	Mechanical drive

	[bookmark: _GoBack]14、柴油机型号 Engine model
	WP6G175E301

	额定转速 Rated speed
	2000r/min

	额定功率 Rated power
	129kW

	柴油机型号 Engine model
	6BTA5.9-C180

	额定转速 Rated speed
	132 kW

	额定功率 Rated power
	2200 r/min

	14、轮胎规格 Tyre model
	20.5-25-16PR






主要配置说明 Main configuration
	序号
S/N
	名称
ITEM
	型号
MODEL
	数量
NO.
	生产厂家
MANUFACTURER

	1
	Engine
	WP6G175E301
6BTA5.9-C180
	1
	WEICHAI
CUMMINS

	2
	Gear box
	CAPGF5-90JM
	1
	HNC

	3
	Drive axle
	GY2203A
	1
	JINGDA

	4
	Vibratory pump
	P7600-F100
	1
	PERMCO

	5
	Vibratory motor
	M7600-F112J
	1
	PERMCO
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