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GYD06J型振动压路机
GYD06J DOUBLE DRUM VIBRATORY ROLLER
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性能特点 Main features:
1.机械驱动，两档速度；
Mechanical drive, two-speed gears.
2.液压后轮振动，单频单幅，电控起振，激振力大，压实效率高；
Hydraulic rear wheel vibration, single-frequency single amplitude, electronically controlled starting vibration, large excitation force, high compaction efficiency.
3.铰接车架，转向灵活；
Articulated frame, flexible steering.
4.电控压力喷洒水，防腐洒水箱和系统；
Electronically controlled pressure spray water, anti-corrosion sprinkler tank and system.
5.液压元件采用知名品牌，性能可靠；
Hydraulic components adopt well-known brands, reliable performance.
6.可选购平板拖车，便于施工转移；
Optional flatbed trailer for easy construction transfer.



	主要技术参数 Main parameters

	整机重量：Operating weight
	6000 kg

	振动轮直径：Vibratory drum diameter
	950 mm

	压实宽度：Vibratory drum width
	1320 mm

	振动频率：Vibratory frequency
	48 Hz

	振幅：Vibratory amplitude	
	0.62 mm

	静线载荷：Static line pressure
	260 N/cm

	行驶速度：Travelling speed
	Forward Ⅰ 2.7km/h   Ⅱ 8km/h

	
	Reverse Ⅰ 2.7km/h   Ⅱ 8km/h

	激振力：Centrifugal force
	60 kN

	爬坡能力：Gradeability
	20%

	转弯半径：Min. turning radius
	5600 mm

	轴距：Wheel base
	2570 mm

	最小离地间隙： Ground clearance
	240 mm

	燃油箱 Fuel tank
	60 L

	洒水箱 Sprinkler tank
	480 L

	液压油箱 Hydraulic oil tank
	80 L

	外形尺寸(长×宽×高)：Dimension
	3660×1550×2630 mm

	发动机 Engine

	发动机型号： Model
	4L68

	制 造 厂：Manufacture
	常柴 CHANGCHAI

	功    率： Rated power
	40 kw

	转    速：Rated speed
	2600 r/min




[bookmark: _Hlk12284727]主要配置说明 Main configuration
	序号
S/N
	部件名称
ITEM
	型号规格
MODEL
	数量
NO.
	制造商
MANUFACTURE

	1
	柴油机
Engine
	4L68
	1
	常柴股份有限公司
[bookmark: _GoBack]CHANGCHAI

	2
	转向泵
Steering pump
	CBW-F310
	1
	合肥长源
CHANGYUAN

	3
	振动马达
Vibratory motor
	GM5-16
	1
	派克(天津)特精液压有限公司
PAIKER

	4
	振动泵
Vibration pump
	G5-20
	1
	派克(天津)特精液压有限公司
PAIKER
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