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	GYR162 Pneumatic tire roller series are designed for the compact cohesive and non-cohesive materials, such as asphalt concrete, cement or lime 

	stabilized soils, gravels, sands and clay mixtures, Rolling Cement Concrete(PCC)in the construction projects, especially suitable for the preparation of the 

	upper courses of high grade highway.

	Main Features:

	1,GYR162 low gravitational center designed for safe and comfortable operation.

	2,With step-less speed changes GYR162 is easy and reliable to operate.. Glass fiber reinforced plastic spraying box and mufti-layer water

	3,filter ensure the stability of the system.

	4,Power strength,GYR162which adopted 4BT Cummins engine, is suitable to all environments.

	5,Front wheel with automatic adjusting Heating structure to perform better compactness.

	Model
	
	GYR162

	Operating mass
	kg
	10000-16000

	Max Travel apeed
	Km/h
	0-14

	Tire quantity (Front+Rear)
	
	4+5

	Tire seize
	
	11.0-20-16

	Wheel rim seize
	
	8.00V-20

	Minimum Turning radius
	mm
	7500

	Rolling compaction width
	mm
	2280

	Ground clerance
	mm
	340

	Electrial voltage
	V
	24

	Grade ability
	%
	30

	Overall dimension (LxWxH)
	mm
	4780x2280x3200

	Wheel base
	mm
	3700

	Diesel egnine power
	Kw
	75Kw/2200rpm

	Diesel egnine model
	
	CUMMINS4BT3.9

	Fuel tank capacity
	L
	223

	Hydraulic tank capacity
	L
	91
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