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GYR303轮胎压路机
GYR303 PNEUMATIC TIRE ROLLER

	规格型号：GYR303轮胎压路机

	MODEL：GYR303 Pneumatic tire roller
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适用范围：Application
适用于高等级公路沥青面层、稳定土等路基的压实
Suitable for compaction of roadbeds such as high-grade highway asphalt layers and stabilized soils
性能特点：Characteristic
1、 采用特制充气光面轮胎对压实材料无破损作用，可通过改变轮胎负荷和充气压力来改变基础压实性能；
The special inflated smooth tire has no damage to the compacted material, and the basic compaction performance can be changed by changing the tire load and the inflation pressure;
2、 具有无级变速功能，操作简单可靠；
With step-less speed changes， easy and reliable to operate
3、 全封闭驾驶室，宽敞明亮，视野开阔；
Fully enclosed cab, spacious and bright with a wide view
4、 可选配洒油装置。 Optional oiling device 。


GYR303轮胎压路机技术参数
GYR303 PARAMETER
	    
	GYR303

	工作质量 Operating weight （kg）
	20000

	最大工作质量Max. operating weight（kg）
	30000

	压实宽度Compaction width （mm）
	2790

	轮胎数量 Tire number
	前5后6   F5R6

	轮胎规格 Tire model
	11.00-20

	行驶速度MAX . Travelling speed
	0-10km/h

	轴距 Wheel base  (mm)
	3800

	爬坡能力 Gradeability
	30%

	最小转弯半径 Min. turning radius (mm)
	8000

	发动机型号 Engine model
	CUMMINS 6BT5.9

	额定功率Rated power (kW)
	125

	额定转速Rated speed (rpm)
	2300

	外形尺寸Dimension L×W×H （mm）
	4950x2790x3240

	传动形式 Transmission form
	液压传动 Hydraulic

	燃油箱 Fuel tank
	193L

	液压油箱 Hydraulic oil tank
	99L
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