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GYS202J全液压单钢轮振动压路机
GYS202J FULL HYDRAULIC SINGLE DRUM VIBRATORY ROLLER
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主要性能特点：Main characteristic
1.液压前后轮驱动，两档无级变速，爬坡能力强。
Fully hydraulic drive, two speeds, continuously variable.
2.液压振动，双频双幅，电控延时起振。
Hydraulic vibration, dual-frequency double amplitude, electronically controlled delayed vibration.
3.液压转向，铰接式车架，转向灵活
Hydraulic steering, articulated frame, flexible steering.
4.液压行走制动，电控钳盘停车制动
Hydraulic service brake, electronically controlled caliper disk parking brake.
5.后机罩可大角度翻起，方便维修保养
Engine hood can be flipped up at a wide angle for easy maintenance.
6.主要液压元件采用国外知名品牌
The main hydraulic components adopt foreign famous brands.
7.标配驾驶室，可选装空调
Standard cabin with optional A/C.



	规格型号：GYS202J全液压单钢轮振动压路机

	MODEL：GYS202J FULL HYDRAULIC SINGLE DRUM VIBRATORY ROLLER

	主要技术参数 Main parameter

	1、工作质量 Operating mass
	20000kg

	2、外形尺寸 Overall dimensions

	总长 Length
	6360 mm

	总宽 Width
	2300 mm

	总高 Height
	3100 mm

	最小离地间隙 Min. ground clearance
	450 mm

	轴距 Wheel base
	3150 mm

	3、发动机 Engine

	生产商 Manufacturer
	WEICHAI

	型号 Model
	WP6G190E22（Ⅱ）

	额定功率 Rated power
	140 kW

	额定转速 Rated speed
	2200 r/min

	冷却型式 Cooling type
	Water cooled

	4、工作装置 Working equipment

	振动轮直径 Diameter of drum
	1600 mm

	压实宽度 Width of compaction
	2130 mm

	静线载荷 Static line pressure
	575 N.m

	名义振幅 Vibratory amplitude
	1.9/0.9 mm

	振动频率 Vibratory frequency
	28/32 Hz

	激振力 Centrifugal force
	385/260 kN

	5、行走系统 Walking system

	前进 Forward speed
	0-4/0-5.5/0-6.5/0-11 km/h

	后退 Reverse speed
	0-4/0-5.5/0-6.5/0-11 km/h

	最大爬坡能力 Gradeability
	40%

	最小转弯半径 Min. turning radius
	6500 mm

	轮胎规格 Tyre model
	20.5-25
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	Item
	Model
	Q’ty
	Manufacturer

	Engine
	WP6G190E22
Optional MEE Ⅲ
	1
	WEICHAI

	Travel pump
	HPV105
	1
	LINDE

	Front travel motor
	HMV075
	1
	LINDE

	Rear travel motor
	HMV105
	1
	LINDE

	Vibration pump
	HPV055
	1
	LINDE

	Vibration motor
	HMF055
	1
	LINDE
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