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724H MOTOR GRADER SPECIFICATIONS
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· Equipped withCummins6CTA8.3-C240 engine
· Sing-handle electro-hydraulic controlled power-shift T/M, 6forward &3reverse shifts makes operation easy and convenient
· Hydraulic lock, auto lock/unlock NO-SPIN differential ensures stability and powerful traction
· Ideal axel load allocation provides excellent stability while cutting hard surface
· Serviceable, efficient hydraulic system enables every part to be fully used
· Box-typed frame and advanced T/M enable it to complete heavy-duty work
· A wide working range is accomplished through flexible blade suspension system and articulated frame 

	Overall Dimension整机尺寸

	1
	Length总长
	9980mm

	2
	Width总宽
	[bookmark: _GoBack]2830mm

	3
	Height(To the top of the cab)总高（到驾驶室顶部）
	3630mm

	4
	Wheel base轴距
	6900mm

	5
	Tread轮距
	2580(mm)

	Main Technical Specification主要技术参数

	1
	Operating weight操作重量
	18000kg

	2
	Blade length 刀板长度
	4420mm

	3
	Blade height刀板高度
	580mm

	4
	Shovel Blade thickness 铲刃板厚度
	20mm

	5
	Traveling speed(Km/h)，6 forward and 3 reverse行驶速度，前六后三

	
	(1)forward前进
	4.96/8.55/11.3/19.32/24.25/40

	
	(2) reverse后退
	4.96/11.3/23

	Diesel engine发动机

	1
	Model型号
	Cummins6CTA8.3-C240 engine                                                  

	2
	Type型式
	[bookmark: OLE_LINK2][bookmark: OLE_LINK1]Direct injection. Turbocharged. Water cooling
直喷、增压、水冷

	3
	Rated output额定功率
	179 kW

	4
	Rated speed额定转速
	2200(r/min)

	5
	Max. Torque最大扭矩
	1028(N.m)/(1500r/min)

	Transmission case变速箱

	1
	Model型号
	6WG200（ZF）

	2
	Type形式
	power shift, single-shift lever, netural-shift lock device
动力换挡、单手柄、中位自锁

	3
	Gear shift position档位
	 6 Forward and 3 reverse gears
前六后三

	Axle and Tire桥和轮胎

	1
	Max. drawing force 最大牵引力
	103KN

	2
	Size of tire轮胎型号
	20.5-25-16PR L-2 (standard) 标配

	Working Device Hydraulic System工作液压系统

	1
	Model of oil pump(include steering pump)
油泵型号(双联泵)
	CBGj1032/1032


	2
	System pressure系统压力
	17.5MPa

	3
	Model of distribution valve多路阀型号
	HUSCO  5000 

	4
	Model of oil motor回转马达型号
	604-0663

	Steering  System转向系统

	1
	Type型号
	Fore Tiredeflexion前轮偏摆式转向

	2
	Model of steering gear转向器型号
	BZZ5-E160BG-1+FKB-3020C

	3
	System pressure系统压力
	16MPa

	Brake System制动系统

	1
	Type of traveling  brake
行车制动系统型式
	Hydraulic and inner-expanding brake
全液压内涨蹄式制动

	2
	Model of brake pump制动泵型号
	CBGj1032/1032

	3
	System pressure系统压力
	10MPa

	4
	Type of parking brake停车制动型式
	Mechanical and inner-expanding brake 
机械式内涨蹄式制动器

	Oil Capacity用油量

	Fuel(diesel)燃油箱
	515L

	Engine lubricating oil发动机机油
	28L

	Oil for converter and gear box变速箱
	28L

	Oil for hydraulic system液压系统
	90L

	Oil for driving rear axles后桥
	80L

	Tandem  box 平衡箱
	165L×2



	


3、724H平地机标准配置表
Standard configuration table for Motor Grader 724H
	序号
NO.
	名称
Item
	型号
Model
	厂家
Manufacturer
	产地
Origin

	1
	发动机
Engine

	6CTA8.3-C240
	东风康明斯
Cummins
	中国
China

	2
	变速箱
Transmission
	6WG200
	ZF
	中国
China

	3
	驱动桥
Axle
	18MRD-X243JC
	[bookmark: _Hlk39062675]美驰
Meritor
	中国
China

	4
	轮胎
Tire
	20.5-25-16PR
	徐轮或前进
Triangle
	中国
China

	5
	工作液压油泵: 
Working Pump
	CBGj1032/1032

	济南
JiNan
	中国
China

	6
	转向装置
Steering System
	BZZ5-E160BG-1+FKB-3020C
	镇江液压件厂
ZhenJiang
	中国
China

	7
	回转马达
Rotary motor
	604-0663
	 伊顿
EATON
	 中国
CHINA

	8
	多路阀
Valve
	5000
	HUSCO
	美国
USA
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