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735T MOTOR GRADER SPECIFICATIONS
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· Equipped with reliable Cummins QSM11-C360 engine
· Sing-handle electro-hydraulic controlled power-shift T/M, 6 forward & 3reverse shifts makes operation easy and convenient
· Hydraulic lock, auto lock/unlock NO-SPIN differential ensures stability and powerful traction
· Ideal axel load allocation provides excellent stability while cutting hard surface
· Serviceable, efficient hydraulic system enables every part to be fully used
· Box-typed frame and advanced T/M enable it to complete heavy-duty work
· A wide working range is accomplished through flexible blade suspension system and articulated frame 
	Overall Dimension整机尺寸

	1
	Length总长
	12500mm

	2
	Width总宽
	3300mm

	3
	Height(To the top of the cab)总高（到驾驶室顶部）
	3700mm

	4
	Wheel base轴距
	7760mm

	5
	Tread轮距
	2650mm

	6
	Min. turning radius 最小转弯半径
	9000mm

	Main Technical Specification主要技术参数

	1
	Operating weight操作重量
	28000kg

	2
	Blade length 刀板长度
	4920mm

	3
	Blade height刀板高度
	695mm

	4
	Blade width 刀板厚度
	25mm

	5
	Max. lift above ground 最大提升高度
	515mm

	6
	Max. grading depth 最大切削深度
	735mm

	7
	Max. shoulder reach outside rear tire 铲刀最大侧伸距离
	2260mm（L）/1950mm（R）

	8
	Traveling speed(Km/h)，6 forward and 3 reverse行驶速度，前六后三

	
	(1) forward前进
	5.4/8.2/12.7/19.3/27.5/41 km/h

	
	(2) reverse后退
	5.4/12.7/27.5 km/h

	Diesel engine发动机

	1
	Model型号
	Cummins QSM11-C360
康明斯QSM11-C360发动机

	2
	Type型式
	EFI,turbocharger,air-to-aircooling,temperature control independent cooling system
电喷、涡轮增压、空空中冷；温控独立散热系统

	3
	Rated output额定功率
	268(kW)

	4
	Rated speed额定转速
	2100(r/min)

	5
	Max. Torque最大扭矩
	1830(N.m)/(1400r/min)

	Transmission case变速箱

	1
	Model型号
	6WG310 （ZF technology）

	2
	Type型式
	electro-hydraulic controlled power shift single handle operation，automatic transmission
电液控制动力换档、自动变速箱，单手柄操作

	3
	Gear shift position
档位数
	 6 Forward and 3 reverse gears
前六后三

	Axle and Tire桥和轮胎

	1
	Max.drawing force 最大牵引力
	144kN

	2
	Size of tire轮胎型号
	18.00-25-28PR

	Working Device Hydraulic System工作液压系统

	1
	Model of oil pump油泵型号
	丹佛斯 FRR074BLS2520-3S1N2A1

	2
	System pressure系统压力
	25MPa

	3
	Model of distribution valve多路阀型号
	Walvoil DRFC22132 DPX100/5
Walvoil DRFC22133 DPX100/5

	4
	Model of oil motor回转马达型号
	Eaton 604-1113

	Steering  System转向系统

	1
	Type型式
	ForeTiredeflexion前轮偏摆式转向

	2
	Model of steering gear转向器型号
	Eaton Xcel45-320

	3
	System pressure系统压力
	16MPa

	Brake System制动系统

	1
	Type of traveling brake 行车制动系统型式
	Full Hydraulic Wet Brakes全液压湿式制动

	2
	Model of brake pump制动泵型号
	泊姆克HPT2-35/HPT1-20/9

	3
	System pressure系统压力
	6.9MPa

	4
	Type of parking brake停车制动型式
	Hydraulically Operated Disc Brake
液压操纵盘式制动

	Oil Capacity用油量

	1
	Fuel(diesel)燃油箱
	540L

	2
	Engine lubricating oil发动机机油
	28L

	3
	Oil for converter and gear box变速箱
	35-40L

	4
	Oil for hydraulic system液压系统
	200L

	5
	Oil for driving rear axles后桥
	35L

	6
	Tandem box 平衡箱
	2*60L




3、735T平地机标准配置表
Standard configuration table for Motor Grader 735T
	序号
NO.
	名称
Item
	型号
Model
	厂家Manufacturer
	产地
Origin

	1
	发动机
Engine
	QSM11-C360
	康明斯
Cummins
	中国
China

	
	
	
	
	

	2
	变速箱
Transmission
	6WG310
	采埃孚
ZF
	[bookmark: _GoBack]德国
GER

	3
	驱动桥
Axle
	19MRW-X245E
	美驰
XZmeritor
	中国
China

	4
	轮胎
Tire
	18.00-25-28PR
	轮胎

	中国
China

	5
	工作液压油泵: 
 Working Pump
	FRR074BLS2520-3S1N2A1
	丹佛斯
Danfoss
	丹麦
Denmark

	6
	转向器
Steering Gear
	Xcel45-320
	伊顿
Eaton
	 美国
USA

	7
	回转马达
Rotary motor
	604-1113
	 伊顿
Eaton
	 美国
USA

	8
	差速器: 
Differential

	NO-SPIN
	美驰
XZmeritor
	中国
China

	9
	多路阀
Valve
	DRFC22132 DPX100/5
DRFC22133 DPX100/5
	沃尔福
Walvoil
	 意大利
Italy

	10
	空调
Air conditioner
	TY50D02
	徐州天一
Tianyi
	中国
China
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