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713H MOTOR GRADER SPECIFICATIONS
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· Sing-handle electro-hydraulic controlled power-shift T/M, 6forward & 3reverse shifts makes operation easy and convenient
· Hydraulic lock, auto lock/unlock NO-SPIN（OPTIONAL） differential ensures stability and powerful traction
· Ideal axle load allocation provides excellent stability while cutting hard surface
· Serviceable, efficient hydraulic system enables every part to be fully used
· Reliable full hydraulic brake system ensures safety
· Box-typed frame and advanced T/M enable it to complete heavy-duty work
· A wide working range is accomplished through flexible blade suspension system and articulated frame 

	Overall Dimension整机尺寸

	1
	Length整机长度
	8290mm

	2
	Width整机宽度
	2600mm

	3
	Height(To the top of the cab)总高（到驾驶室顶部）
	3465mm

	4
	Wheel base轴距
	5780mm

	5
	Tread轮距
	2120(mm)

	6
	Min. turning radius 最小转弯半径
	6.6（m）

	Main Technical Specification主要技术参数

	1
	Operating weight操作重量
	12000kg

	2
	Blade length 刀板长度
	3658mm

	3
	Blade height刀板高度
	545mm

	4
	Shovel Blade thickness 铲刃板厚度
	20mm

	5
	Max. lift above ground 最大提升高度
	410mm

	6
	Max. grading depth 最大切削深度
	560mm

	7
	Max. shoulder reach outside rear tire 铲刀最大侧伸距离
	2000mm

	8
	Traveling speed(Km/h)，6 forward and 3 reverse行驶速度，前六后三

	
	(1) forward前进
	6.9/10.7/17.3/26/37.8/53.4

	
	(2) reverse后退
	6.9/17.3/37.8

	Diesel engine发动机

	1
	Model型号
	DongFeng Cummins 6BT5.9-C130 东康6BT5.9-C130                                                               

	2
	Type型式
	Direct injection. Turbocharged. Water cooling
直喷、增压、水冷

	3
	Rated output额定功率
	97kW

	4
	Rated speed额定转速
	2200(r/min)

	5
	Max. Torque最大扭矩
	560(N.M)/1500rpm

	Transmission case变速箱

	1
	Model型号
	YD13 （CHINESE HANGCHI）

	2
	Type形式
	power shift, single-shift lever, natural-shift lock device
动力换挡、单手柄、中位自锁

	3
	Gear shift position档位
	 6 Forward and 3 reverse gears前6后3

	Axle and Tire桥和轮胎

	1
	Max. drawing force 最大牵引力
	61.7KN（f=0.75）

	2
	Size of tire轮胎型号
	17.5-25-12PR(standard) 标配
13.00-24-12PR(optional)选配

	Working Device Hydraulic System工作液压系统

	1
	Model of  tandempump
油泵型号
	HP51B678-07-07-7N

	2
	System pressure系统压力
	17.5MPa

	3
	Model of distribution valve多路阀型号
	PD15.5CLR-00；PD15.5CLL-00

	4
	Model of oil motor回转马达型号
	EATON, 604-0663

	Steering  System转向系统

	1
	Type形式
	Fore Tires deflexion前轮偏移式转向

	2
	Model of redirector转向器型号
	BZZ5-E160B+FKB-3022

	3
	System pressure系统压力
	16MPa

	Brake System制动系统

	1
	Type of service brake
行车制动系统型式
	Full hydraulic and inner-expanding brake
全液压内涨蹄式制动

	2
	Oil pressure系统压力
	10Mpa

	3
	Type of parking brake停车制动形式
	Mechanical and inner expand hoof brake
机械式内涨蹄式制动器

	Oil Capacity油量

	1
	Fuel(diesel)燃油箱
	370L

	2
	Engine lubricating oil发动机机油
	14L

	3
	Oil for converter and gear box变速箱
	32L

	4
	Oil for hydraulic system液压系统
	65L

	5
	Oil for driving rear axles后桥
	17L

	6
	Tandem box 平衡箱
	90L




3、713H平地机标准配置表
	序号
	名称
	型号
	厂家
	产地

	1
	发动机
	6BT5.9-C130
	康明斯
	中国

	2
	变速箱
	YD13
	杭齿
	中国

	3
	驱动桥
	
	常林
	中国

	4
	轮胎
	17.5-25-12PR
	徐轮/贵轮
	中国

	5
	工作液压油泵: 
	HP51B678-07-07-7N
	海克力斯
	中国

	6
	转向装置
	BZZ5-E160B+FKB-3022
	镇江液压件厂
	中国

	7
	回转马达
	604-0663
	 伊顿
	 中国

	8
	链条:
	
	东华/椿本（选）
	中国/日本

	9
	差速器: 
	NO-SPIN（选）
	常林/伊顿（选）
	中国/美国

	10
	多路阀
	PD15.5CL
	海宏
	中国

	11
	液压锁
	 WBCDELU-03-B等
	  奇威/EATON
	 中国/美国

	12
	空调（选配）
	
	豫新
	中国
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