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732T-5 MOTOR GRADER 
Front wheel auxiliary drive configuration and parameters
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· Equipped with reliable Cummins QSM11-C330 engine
· Sing-handle electro-hydraulic controlled power-shift T/M, 6 forward & 3reverse shifts makes operation easy and convenient
· Hydraulic lock, auto lock/unlock NO-SPIN differential ensures stability and powerful traction
· Hydraulic system: dual handle electric control load sensitive system
· Steering system: fully hydraulic front wheel steering, articulated steering
· Service braking: fully hydraulic wet braking
· Parking brake: hydraulic operated disc brake
	Overall Dimension整机尺寸

	1
	Length总长
	12750mm

	2
	Width总宽
	3300mm

	3
	Height(To the top of the cab)总高（到驾驶室顶部）
	3700mm

	4
	Wheel base轴距
	8010mm

	5
	Tread轮距
	2650mm

	6
	Min. turning radius 最小转弯半径
	9000mm

	Main Technical Specification主要技术参数

	1
	Operating weight操作重量
	30000kg

	2
	Blade length 刀板长度
	4620mm

	3
	Blade height刀板高度
	695mm

	4
	Blade width 刀板厚度
	25mm

	5
	Max. lift above ground 最大提升高度
	515mm

	6
	Max. grading depth 最大切削深度
	735mm

	7
	Max. shoulder reach outside rear tire 铲刀最大侧伸距离
	2260mm(R)/1950mm(L)

	8
	Maximum inclination angle 最大倾斜角
	65 °

	9
	Cutting angle adjustment range切削角调整范围
	23-73 °

	10
	Max. swing angle of the front axle: 前桥最大摆动角
	15 °

	11
	Max. inclination angle of front wheel 前轮最大倾斜角
	17 °

	12
	Max. front wheel steering angle 前轮最大转向角
	49 °

	13
	Max. turning angle of articulation 铰接最大转向角
	25 °

	14
	Traveling speed(km/h)，6 forward and 3 reverse行驶速度，前六后三

	
	(1) forward前进
	5.5、8.6、13.3、20.3、29、43

	
	(2) reverse后退
	5.5、13.3、29

	Diesel engine发动机

	1
	Model型号
	Cummins QSM11-C330
康明斯QSM11-C330发动机

	2
	Type型式
	EFI,turbocharger,air-to-aircooling;temperaturecontrolindependentcoolingsystem
电喷、涡轮增压、空空中冷；温控独立散热系统

	3
	Rated output额定功率
	246(kW)

	4
	Rated speed额定转速
	2100(r/min)

	5
	Max. Torque最大扭矩
	1674(N.m)/(1400r/min)

	Transmission case变速箱

	1
	Model型号
	ZF 6WG260 

	2
	Type型式:电液控制动力换档、自动变速箱，单手柄操作
	electro-hydraulic controlled power shift single handle operation，automatic transmission

	3
	Gear shift position
档位数
	6 Forward and 3 reverse gears
前六后三

	Axle and Tire桥和轮胎 Rear axle balance box:Meritor

	1
	Max. drawing force（f=0.73）最大牵引力
	200kN

	2
	Size of tire轮胎型号
	18.00-25-28PR

	Working Device Hydraulic System工作液压系统

	1
	Model of oil pump油泵型号
	丹佛斯FRR074BLS2520-3S1N2A1

	2
	System pressure系统压力
	25MPa

	3
	Model of distribution valve多路阀型号
	Walvoil DRFC22132 DPX100/5
Walvoil DRFC22133 DPX100/5

	4
	Model of oil motor回转马达型号
	Eaton 604-1113

	Steering  System转向系统

	1
	Type型式
	Fore Tire deflexion前轮偏摆式转向

	2
	Model of steering gear转向器型号
	Eaton Xcel45-320

	3
	System pressure系统压力
	16MPa

	Brake System制动系统

	1
	Type of traveling brak额行车制动系统型式
	Full Hydraulic Wet Brakes全液压湿式制动

	2
	Model of brake pump制动泵型号
	泊姆克HPT3-50/HPT1-22/9

	3
	System pressure系统压力
	6.9MPa

	4
	Type of parking brake停车制动型式
	Hydraulically Operated Disc Brake
液压操纵盘式制动

	Front wheel auxiliary drive system前轮辅助驱动系统

	1
	Model of front wheel drive pump
前驱油泵型号
	驱动泵FRR090CLS2620--3S1C2A1

	2
	Model of front wheel drive motor
前驱马达型号
	左前轮马达4073601313
右前轮马达4073601213
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