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GKM90P矿用自卸车
GKM90P Mine Dump Truck
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	GKM90P Off-road mining dump truck

	型号 Type 
	GKM90P

	驾驶室 Driving cab： 
	可翻转式宽体偏置驾驶室
Reversible wide-body offset cab 

	发动机Engine Type/ Horsepower:： 
	WEICHAI 430马力WP12G430E310国三
WEICHAI 420马力WD12G420E211国二

	变速箱
Transmission Type: 
	[bookmark: _GoBack]FAST 7DS220 Manual (without liquid retardation)

	转向器
Steering Engine:
	全液压转向Full hydraulic power steering engine

	前/后车桥
Front/rear axle:
	19T前桥/ 35T铸钢双级减速中后桥（鼓式制动）
19Tcasting steel front axle/35Tcasting dual reduction middle/rear axle

	车架
Frame:： 
	焊接式刚性箱型车架  450*140
Welded rigid cube type frame 450*140

	上装描述
Description:
	高强耐磨板400 底16mm Q345钢板边12mm 后12mm、前举、海沃举升系统、矿用厢
steel plate, bottom plate 16mm, side plate 12mm, HYVA hydraulic system, mining square box
货厢内尺寸（mm）Inner dimension of body：5850*3200*1750

	轮胎Tyre: 
	14.00R25 Mining Tubed Wire Tire矿用有内胎钢丝胎轮胎
14.00-25 Mining Tubed Bias Tire 矿用有内胎斜交胎

	悬挂
Front/rear suspension: 
	前油气悬挂/后整体焊接式平衡悬挂，加强型可拆换式平衡轴
Front oil and gas suspension/rear integral welded balance suspension, reinforced removable balance shaft

	板簧
Leaf spring for front, middle, rear axle:
	前：油气弹簧/后：钢板弹簧14*120*27
Front: Oil-gas spring Rear: 14*120*27

	制动系统
Breaking system:
	瑞立
SORL system

	其他
Others:
	油浴式空气滤清器、排气制动、大箱底板加热、淋水、剔石器，底盘防护，油箱防护，挡泥板，LED侧灯和尾灯，电子空调
Oil bath air filter, exhaust brake, box floor heating, drenching, stone picker, chassis protection, fuel tank protection, fenders, LED side and tail lights, electronic air conditioning

	整车质量
Curb Weight(kg): 
	30000

	额定载质量
Rated load(kg):
	60000

	总质量
Rated total weight(kg):
	90000

	外形尺寸
Overall Dimension(mm):
	9100×3450×4130

	最大速度
Max speed(km/h):
	42

	最小离地间隙
Min ground clearance(mm):
	380

	最小转弯半径
Min turning radius(m):
	≤12m

	最大爬坡度
Max gradeability(%):
	33%

	接近角/离去角
Approach angle/Departure angle(°):
	32°/39°

	轴距
Axle base(mm):
	3800+1560

	前后轮距
Wheel span (front /rear)(mm):
	PX90 :2792/2526 

	油箱
Oil tank Capacity(L):
	450L/600L

	货箱容积
Body Capacity:
	32.8m³ 

	备注：（CNY）
	出口左侧驾驶室加2000元，出口右侧驾驶室加4000元
集中润滑加9200元
倒车影像加2500元，360度环视影像加4200元
液力缓速器加20000元，加液力缓速器需增加电子散热器，电子散热器加5000元
淋水刹车加4800元，铜水箱加12500元
海运整车打蜡加1000元
货箱材质全提升至高强耐磨板400材质加价12000元
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SINOMACH-HI International Equipment Co.,Ltd.
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