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GKM95P矿用自卸车
GKM95P Mine Dump Truck

	GKM95P Off-road mining dump truck

	型号Type:
	GKM95P

	驾驶室Driving Cab:
	矿用宽体驾驶室（左驾）
Reversible wide-body offset cab （Left  hand）

	发动机Engine Type/ Horsepower:
	玉柴520马力发动机 YuChai YC6K520-GT30 E3

	变速箱
Transmission Type:
	 艾里逊Allison 4800 ORS-RP （AT）

	转向器
Steering Engine:
	伊顿全液压转向系统EATON Full hydraulic power steering engine

	前/后车桥
Front/rear axle:
	25吨前桥35吨中后桥
25Tcasting steel front axle/35T  casting dual reduction middle/rear axle

	车架
Frame:
	焊接式半刚性车架 480*140
Welded Semi-rigid cube type frame 480*140

	货箱尺寸
Inner dimension of body(mm):
	6000*3400*1300

	上装描述
Description:
	Q345钢板，底板16mm边板12mm，海沃179液压系统，矿用方箱
Q345 steel plate, bottom plate 16mm, side plate 12mm, Hyward 191 hydraulic system, mining square box


	轮胎Tyre:
	 16.00-25 矿用轮胎 Mining tires

	悬挂
Front/rear suspension:
	全焊接平衡悬挂，加强可拆卸平衡轴
Whole welded equalizing suspension, reinforced removable equalizing shaft

	板簧
Leaf spring for front, middle, rear axle:
	前：油气弹簧 后：钢板弹簧
Front: Oil-gas spring Rear: leaf spring

	制动系统
Breaking system:
	瑞立制动系统
SORL system,Front / mid / rear axle drum brake

	其他
Others:
	油浴式滤清器，排气制动，底板加热，排石器，底盘防护，继电器防水保护，后视镜加固，LED侧灯和尾灯
Oil bath filter, exhaust brake, floor heating, stone ejector, chassis protection, relay waterproof protection, mirror reinforcement, LED side and tail lights

	整车质量
Curb Weight(kg):
	34000 

	额定载质量
Rated load(kg):
	65000

	总质量
Rated total weight(kg):
	99000

	外形尺寸
Overall Dimension(mm):
	9100×3650×4150

	最大速度
Max speed(km/h):
	50

	最小离地间隙
Min ground clearance(mm):
	435

	最小转弯半径
Min turning radius(m):
	≤12

	最大爬坡度
Max gradeability(%):
	33

	接近角/离去角
Approach angle/Departure angle(°):
	37/39

	轴距
Axle base(mm):
	3800+1690

	前后轮距
Wheel span (front /rear)(mm):
	Front2792, Rear 2526

	油箱
Oil tank Capacity(L):
	600L Steel oil tank

	货箱容积
Body Capacity:
	平装Flat 38.7m³
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A SINOMACH-HI International Equipment Co.,Ltd.
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