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GKM65P矿用自卸车
GKM65P Mine Dump Truck
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	GKM65P Off-road mining dump truck

	型号 Type
	GKM65P

	驾驶室 Driving cab：
	可翻转式宽体偏置驾驶室
Reversible wide-body offset cab

	发动机Engine Type/ Horsepower:：
	WEICHAI 380马力国三

	变速箱
Transmission Type:
	FAST 7DS220 Manual (without liquid retardation)

	转向器
Steering Engine:
	液压助力Hydraulic power

	前/后车桥
Front/rear axle:
	13T 前桥 / 25T 铸钢双级减速中后桥
13T front axle/ 25T casting dual reduction tandem axle

	车架
Frame:：
	焊接式刚性箱型车架  450*130
Welded rigid cube type frame 450*130

	上装描述
Description:
	底板 16mm 边板 12mm、前举、海沃 Hyva 油缸、方箱
Bottom 16mm, side 12mm, front hoisting, Hyva cylinder, square box
货厢内尺寸（mm）Inner dimension of body：5600*2850*1550

	轮胎Tyre:
	14.00R25 Mining Tubed Wire Tire矿用有内胎钢丝胎轮胎
14.00-25 Mining Tubed Bias Tire 矿用有内胎斜交胎

	悬挂
Front/rear suspension:
	钢板弹簧 Steel plate springs

	制动系统
Breaking system:
	瑞立
SORL system

	其他
Others:
	三级沙尘空滤、排气制动、大箱底板加热、排石器、底盘防护、电瓶防护、油箱防护、挡泥板、LED侧灯和尾灯、电子空调
Triple sand air filter, exhaust brake, heated big box floor, stone evacuator, chassis protection, battery protection, fuel tank protection, fenders, LED side and tail lights, electronic air conditioning

	整车质量
Curb Weight(kg):
	23000

	额定载质量
Rated load(kg):
	40000

	总质量
Rated total weight(kg):
	63000

	外形尺寸
Overall Dimension(mm):
	8700*3000*3700

	最小离地间隙
Min ground clearance(mm):
	380

	最小转弯半径
Min turning radius(m):
	≤12

	最大爬坡度
Max gradeability(%):
	30

	轴距
Axle base(mm):
	3650+1560

	油箱
Oil tank Capacity(L):
	400L

	货箱容积
Body Capacity:
	25m³
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