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I. Product Performance Advantages and Features
1. An energy-efficient electric drive system with zero emissions and low noise, ideal for eco-friendly and convenient installation in office buildings, hospitals, schools, and similar environments.
2. Active safety features like pothole protection mechanisms and intelligent safety control systems fully meet customers' demands for safety, reliability, and smart functionality.
3. The compact structural design enables flexible utilization in confined spaces.
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1. Standard configuration

• Foldable guardrail
• Self-locking platform door
• Unidirectional extension platform
• Non-slip metal platform
• Safety maintenance support
• Standard transport forklift hole
• Tethering point
• Fixing and lifting points
• front-wheel drive
• front-wheel steer
• Action Beep
• strobe light
• Emergency stop button
• Manual brake release
• ratio control
• Full range of motion
• High-altitude low-speed protection
• Pit protection
• Inclined protection
• Charging protection
• self-actuating brake
• fault diagnosis
• emergency descent
• GPS








2. Optional configurations
• Connect the AC power cord to the platform
• The compressed air pipe is connected to the platform
• Platform work light
Handle protection bracket
• Weight alarm system
• Collision Protection System


III. Main Technical Parameters Table
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	parameter

	maximum working height
	13.8m

	maximum platform height
	11.8m

	minimum platform height
	1.47m

	Total length (excluding ladder/legs)
	2477（2267）mm

	Machine width
	1190mm

	Total height (platform folded)
	2610(2060)mm

	Workbench length
	2280mm

	Workbench width
	1120mm

	platform extension length
	900mm

	Guardrail height
	1138mm

	Treadboard height
	150mm

	wheel base
	1877mm

	Minimum ground clearance (pit protection support/retract)
	20mm/100mm

	

	function
	parameter

	specified load
	320kg

	stretching platform load
	115kg

	Maximum occupancy (indoor/outdoor)
	2/0

	maximum walking speed at low position
	3.2km/h

	maximum walking speed at high altitude
	0.8km/h

	maximum gradability
	25%

	Minimum turning radius (inner wheel)
	0m

	Minimum turning radius (outer wheel)
	2.3m

	Work platform lifting time
	45-70s

	Workbench downtime
	52-78s

	Maximum allowable working angle (lateral/forward/backward)
	1.5°/3°

	tyre size
	381mm×127mm

	

	motive power
	parameter

	cell voltage
	24V-25.76V

	Battery capacity (3hr)
	200Ah-225Ah

	oil tank capacity
	16L

	

	weight
	parameter

	Total weight of the machine
	2920kg


Note: (1) Battery capacity varies depending on the device configuration.
(2) The total weight varies according to the configuration of the machine.

IV. Vehicle Driving Status Dimension Diagram


Figure 1: Dimensional diagram of the vehicle in operation


Figure 2: Dimensional diagram of the complete machine in transport condition
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