This is the condition of bearing plate straight after removal. Suface is badly damage. Pin is gone too.

