


User:admin passw:administrator 


System>endpoints (go to action unlocked ) default LAN-IPAddress 192.168.0.10 WAN 192.168.0.1




Network>Status Active




Network>Host (IPv4 Static, 192.168.0.1 default gateway)




Network>Host>SNTP and Time Zone (UTC-3:45)




Network>Interfaces Lan1-192.168.0.10/24, router 192.168.0.1




POTS>Status “idle”




POTS>Config




POTS>FXS Config(refer to above config and change it accordingly)




SIP>Gateway>Status Port=5060 Secure Port=0



SIP>Servers OSO or SIP Proxy Provider IPaddress



SIP>Registrations



SIP>Transport