Flintec Device Configurator (FDC)
=================================

To install:

1. Copy or Extract file installation file 'Flintec Device Configurator Vx.xx.exe' from the zip file to a directory or desktop.
2. Double-click to start installation.

Important FDC/EM100 Compatibility Information:
==============================================

FDC V1.80 is compatible with EM100:

    V1.02
    V1.03
    V1.04
    V1.50
    V1.60
    V1.70
 
FDC V4.0 and above is compatible with EM100:

    V1.80
    V1.90
    V2.0.0


Introduction:
=============

The FDC is a powerful PC application that can be used to configure upto four Flintec Load-cell Digitising Units such as the EM100.

The application can communicate with the EM100 using a number of interfaces such as:

1. RS232
2. USB-CDC
3. RS485
4. CANopen (EM100)

Settings that can be configured include:

1. Serial and CAN Communication settings such as Address, Baudrate, Half/Duplex and Termination.
2. Calibration - both manual and electronic (eCal).
3. Filtering and Samples per Second (SPS).
4. Rising Edge/ Falling Edge Triggering.
5. Set-Point switching.
6. For the EM100-C model - Re-Trigger Settings.
7. For the EM100-F model - Bottle Filling parameters.

As well as setting up and configuring the EM100/TR2, the FDC can also:

1. Display the readings as a large scale display with Tare / Reset Tare controls.
2. Display readings in a Real-Time Chart to show response.
3. Save / Restore settings between devices or file.
4. Serial / CAN Terminals. Allows the user to access commands not supported by the FDC or indepth fault-finding.  


Included Flintec Documents
==========================

0088642: FDC Quick Start Guide.
0087171: EM100 FDC User Manual.

