HAT to Panel Bracket FAQ

**Q What systems can this product be used with?**

**A** The HAT to Panel bracket is compatible with Stride, Terrace, and Optimize panel systems. There are also separate models that attach to Gallery Panels, which require a separate installation template model to be ordered.

**Q What height-adjustable tables can this product be used with?**

**A** The HAT to Panel bracket is compatible with all Altitude height-adjustable tables. There are separate models that attach to T-leg and C-leg bases, and the connection type is handed. The handedness is specified based on the user’s orientation.

**Q Can the bracket be retrofitted on existing installations?**

**A** Yes, the bracket wraps around the table leg and hooks into the slotted standard. It can be attached to an existing installation and is non-defacing.

**Q Are there separate models depending on the worksurface depth?**

**A** No, there is a telescoping feature within the bracket that allows it to be installed at varying lengths depending on the application. The same bracket can be installed with a 24”D worksurface and a 30”D worksurface.

**Q Can this bracket be used on a table with a surface-mounted screen?**

**A** Yes, the telescoping feature also allows the bracket to adjust in length to accommodate added screen depth. IF the application requires a 30”D C-Leg table with a screen, the T-leg bracket must be specified.

**Q Does this bracket take the place of a worksurface or storage tie-in for panel stability requirements?**

**A** No, this bracket is for panel rigidity purposes only, it does not function as a structural component for panel stability requirements.

**Q What paint options are available?**

**A** The bracket can be painted in any standard Allsteel paint color and can match the system trim. Note: the HAT bases are not available in Allsteel standard colors, so the silver, white, and black will not be an exact match.