,Model##OTHER##,Description##OTHER##,Bracket Width##LENGTH##FEET,Width##LENGTH##FEET,Height##LENGTH##FEET,Panel##OTHER##,Hinge Finish##OTHER##,Hinge##OTHER##
"LK-MPR-96H - Removable Laminate Modesty Panel,HPL, 8x96",LK-MPR-96H , "96""W  Laminate Modesty Panel With HPL, 8""x96""",6.26083,7.95833,0.6666,JSI-Laminate HPL,JSI-Metal,1
"LK-MPR-84H - Removable Laminate Modesty Panel,HPL, 8x84",LK-MPR-84H , "84""W  Laminate Modesty Panel With HPL, 8""x84""",5.26083,6.95833,0.6666,JSI-Laminate HPL,JSI-Metal,1
"LK-MPR-72H - Removable Laminate Modesty Panel,HPL, 8x72",LK-MPR-72H , "72""W  Laminate Modesty Panel With HPL, 8""x72""",4.26083,5.95833,0.6666,JSI-Laminate HPL,JSI-Metal,1
"LK-MPR-66H - Removable Laminate Modesty Panel,HPL, 8x66",LK-MPR-66H , "66""W  Laminate Modesty Panel With HPL, 8""x66""",4.1250,5.45833,0.6666,JSI-Laminate HPL,JSI-Metal,1
"LK-MPR-60H - Removable Laminate Modesty Panel,HPL, 8x60",LK-MPR-60H , "60""W  Laminate Modesty Panel With HPL, 8""x60""",3.6250,4.95833,0.6666,JSI-Laminate HPL,JSI-Metal,1
"LK-MPR-48H - Removable Laminate Modesty Panel,HPL, 8x48",LK-MPR-48H , "48""W  Laminate Modesty Panel With HPL, 8""x48""",2.26083,3.95833,0.6666,JSI-Laminate HPL,JSI-Metal,0
"LK-MPR-36H - Removable Laminate Modesty Panel,HPL, 8x36",LK-MPR-36H , "36""W  Laminate Modesty Panel With HPL, 8""x36""",1.26083,2.95833,0.6666,JSI-Laminate HPL,JSI-Metal,0
"LK-MPR-96T - Removable Laminate Modesty Panel,TFL, 8x96",LK-MPR-96T , "96""W  Laminate Modesty Panel With TFL, 8""x96""",6.26083,7.95833,0.6666,JSI-Laminate TFL,JSI-Metal,1
"LK-MPR-84T - Removable Laminate Modesty Panel,TFL, 8x84",LK-MPR-84T , "84""W  Laminate Modesty Panel With TFL, 8""x84""",5.26083,6.95833,0.6666,JSI-Laminate TFL,JSI-Metal,1
"LK-MPR-72T - Removable Laminate Modesty Panel,TFL, 8x72",LK-MPR-72T , "72""W  Laminate Modesty Panel With TFL, 8""x72""",4.26083,5.95833,0.6666,JSI-Laminate TFL,JSI-Metal,1
"LK-MPR-66T - Removable Laminate Modesty Panel,TFL, 8x66",LK-MPR-66T , "66""W  Laminate Modesty Panel With TFL, 8""x66""",4.1250,5.45833,0.6666,JSI-Laminate TFL,JSI-Metal,1
"LK-MPR-60T - Removable Laminate Modesty Panel,TFL, 8x60",LK-MPR-60T , "60""W  Laminate Modesty Panel With TFL, 8""x60""",3.6250,4.95833,0.6666,JSI-Laminate TFL,JSI-Metal,1
"LK-MPR-48T - Removable Laminate Modesty Panel,TFL, 8x48",LK-MPR-48T , "48""W  Laminate Modesty Panel With TFL, 8""x48""",2.26083,3.95833,0.6666,JSI-Laminate TFL,JSI-Metal,0
"LK-MPR-36T - Removable Laminate Modesty Panel,TFL, 8x36",LK-MPR-36T , "36""W  Laminate Modesty Panel With TFL, 8""x36""",1.26083,2.95833,0.6666,JSI-Laminate TFL,JSI-Metal,0