,Model##OTHER##,Description##OTHER##,Bracket Width##LENGTH##FEET,Width##LENGTH##FEET,Height##LENGTH##FEET,Panel##OTHER##,Hinge Finish##OTHER##,Hinge##OTHER##
"LK-MPR-96A - Removable Acrylic Modesty Panel, 8x96",LK-MPR-96A , "96""W  Acrylic Modesty Panel With Acrylic, 8""x96""",6.26083,7.96875,0.71875,JSI-Acrylic,JSI-Metal,1
"LK-MPR-84A - Removable Acrylic Modesty Panel, 8x84",LK-MPR-84A , "84""W  Acrylic Modesty Panel With Acrylic, 8""x84""",5.26083,6.96875,0.71875,JSI-Acrylic,JSI-Metal,1
"LK-MPR-72A - Removable Acrylic Modesty Panel, 8x72",LK-MPR-72A , "72""W  Acrylic Modesty Panel With Acrylic, 8""x72""",4.26000,5.96875,0.71875,JSI-Acrylic,JSI-Metal,1
"LK-MPR-66A - Removable Acrylic Modesty Panel, 8x66",LK-MPR-66A , "66""W  Acrylic Modesty Panel With Acrylic, 8""x66""",3.76083,5.46875,0.71875,JSI-Acrylic,JSI-Metal,1
"LK-MPR-60A - Removable Acrylic Modesty Panel, 8x60",LK-MPR-60A , "60""W  Acrylic Modesty Panel With Acrylic, 8""x60""",3.26083,4.96875,0.71875,JSI-Acrylic,JSI-Metal,1
"LK-MPR-48A - Removable Acrylic Modesty Panel, 8x48",LK-MPR-48A , "48""W  Acrylic Modesty Panel With Acrylic, 8""x48""",2.26000,3.96875,0.71875,JSI-Acrylic,JSI-Metal,0
"LK-MPR-36A - Removable Acrylic Modesty Panel, 8x36",LK-MPR-36A , "36""W  Acrylic Modesty Panel With Acrylic, 8""x36""",1.26000,2.96875,0.71875,JSI-Acrylic,JSI-Metal,0