,_CreatedBy##OTHER##,Wattage Comments##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Warranty(Years)##OTHER##,Voltage Loss##OTHER##,UG4H8H(20%,50%,70%) C0/ C90##OTHER##,Total Light Loss Factor##OTHER##,Temperature Loss##OTHER##,Temperature Color##OTHER##,Surface Depreciation Loss##OTHER##,Luminous Intensity##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,LuminaireEfficacy##OTHER##,Luminaire Dirt Depreciation##OTHER##,LightOutputRatio##OTHER##,LightDistribution##OTHER##,Light Source Symbol Size##LENGTH##MILLIMETERS,Light Loss Input Method##OTHER##,Light Loss Factor##OTHER##,Lamp Tilt Loss##OTHER##,Lamp Lumen Depreciation##OTHER##,LBtRatedLife##OTHER##,LBS2G8##OTHER##,LBS1G4##OTHER##,Initial Light Intensity Input Method##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,Illuminance##ELECTRICAL_ILLUMINANCE##LUX,Hours##OTHER##,Frequency##OTHER##,Emit from Line Length##LENGTH##MILLIMETERS,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Driver##OTHER##,Dimming Lamp Color Temperature Shift##OTHER##,Color Filter##OTHER##,CIEFluxCodes##OTHER##,IKRating##OTHER##,LBS2R2##OTHER##,ManufacturerWebsite##OTHER##,CRI##OTHER##,Height##LENGTH##MILLIMETERS,Weight (kg)##OTHER##,UpwardComponent##OTHER##,URLToEnergyTechnologyList##OTHER##,URL##OTHER##,Type Comments##OTHER##,TotalLightOutput##OTHER##,Temp##OTHER##,ResponsibleSourcingOfMaterials##OTHER##,ResponsibleExtractionOfMaterials##OTHER##,ProductRange##OTHER##,ProductLiterature##OTHER##,OverallLightOutputRatio##OTHER##,Model##OTHER##,MaterialIngredientReporting##OTHER##,Manufacturer##OTHER##,Lum/lms##OTHER##,LocationOfManufacturer##OTHER##,Load##OTHER##,LightOutputPattern##OTHER##,BodyMaterial##OTHER##,LightFixtureMountingType##OTHER##,LifeCycleAnalysis##OTHER##,Lamps##OTHER##,LED##OTHER##,Keynote##OTHER##,IntendedMarket##OTHER##,IPRating##OTHER##,GreenGuideForSpecification##OTHER##,PolycarbonateDiffuser##OTHER##,EnivornmentProductDeclaration##OTHER##,Emergency##OTHER##,EmbodiedCarbon##OTHER##,Efficacy.##OTHER##,DownwardComponent##OTHER##,Description##OTHER##,Length##LENGTH##MILLIMETERS,Default Elevation##LENGTH##MILLIMETERS,CEApproval##OTHER##,TempRange(°C)##OTHER##,Ballast Loss##OTHER##,At a distance##LENGTH##MILLIMETERS,ApplicationEnvironment##OTHER##,AmbientTemp.RatedLife(°C)##OTHER##
LBS1G4,IN,4.5,4.500000000000,3 Years,1,"(20%, 50%, 70%) C0 / C90: 23.1/23.3",1,1,12,1,31.512678732195,396.000000000000,100%,1,100%,A31↓91.2%↑8.8%,609.6,0,,1,1,L70/B50,0,1,0,,4000.000000000000,,3.391996508639,30k,50-60,609.6,88.000000000000,Fixed Output,0,16777215,39 68 89 91 100,IK08,0,http://luceco.com/uk,>80,115,0.2,0%,n/a,http://luceco.com/uk,n/a,400lms,4000K Netural White,n/a,n/a,Storm Bulkhead,n/a,0%,LBS1G4,n/a,Luceco,400lms,Luceco plc Caparo House 103 Baker Street,4.50 W,n/a,BodyMaterial,Suitable for 230V or 110V use,0,n/a,Yes,n/a,n/a,IP65,n/a,Polycarbonate,n/a,No,n/a,88.00 lm/W,0%,,115,0,Yes,-20+25,1,3048,Internal,25
LBS2G8,IN,7,7.000000000000,3 Years,1,24.3/24.7,1,1,12,1,59.603526187915,749.000000000000,100%,1,100%,A31↓92.1%↑7.9%,609.6,0,,1,1,L70/B50,1,0,0,,4000.000000000000,,6.415670164067,30k,50-60,609.6,107.000000000000,Fixed Output,0,16777215,40 70 90 92 100,IK08,0,http://luceco.com/uk,>80,115,0.3,0%,n/a,http://luceco.com/uk,n/a,750lms,4000K Netural White,n/a,n/a,Storm Bulkhead,n/a,0%,LBS2G8,n/a,Luceco,750lms,Luceco plc Caparo House 103 Baker Street,7.00 W,n/a,BodyMaterial,Suitable for 230V or 110V use,0,n/a,Yes,n/a,n/a,IP65,n/a,Polycarbonate,n/a,No,n/a,107lm/W,0%,,175,0,Yes,-20+25,1,3048,Internal,25
LBS2G8MW,IN,7.5,7.500000000000,3 Years,1,24.3/24.7,1,1,12,1,59.683103659461,750.000000000000,100%,1,100%,A31↓92.1%↑7.9%,609.6,0,,1,1,L70/B50,0,1,0,,4000.000000000000,,6.424235811816,30k,50-60,609.6,100.000000000000,Fixed Output + Sensor,0,16777215,,IK08,0,http://luceco.com/uk,>80,115,0.4,0%,n/a,http://luceco.com/uk,n/a,750lms,4000K Netural White,n/a,n/a,Storm Bulkhead,n/a,0%,LBS2G8MW,n/a,Luceco,750lms,Luceco plc Caparo House 103 Baker Street,7.50 W,n/a,BodyMaterial,Suitable for 230V or 110V use,0,n/a,Yes,n/a,n/a,IP65,n/a,Polycarbonate,n/a,No,n/a,100lm/W,0%,,175,0,Yes,-20+25,1,3048,Internal,25
