200W LED PROFILE

(WW+CW)
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USER MANUAL

	KEEP THIS USER MANUAL FOR FUTURE NEEDS


ADVICE BEFORE USE
Please read these safety rules carefully before use.

After the equipment has been transported to its destination, please unpack it carefully and check for any transportation damage. If any defects or damages are found, contact the freight company immediately and file a complaint according to the situation of the defects/damages.Please check and verify that the model, quantity of the goods are consistent with those listed in the shipping document and the order. If there is any discrepancy, contact the supplier immediately.

Scope of Application

This luminaire is a professional stage lighting equipment, used in professional scenarios such as large indoor theaters, film and television studios, etc.

Installation and Operation

The grounding wire must be reliably connected to the ground;Do not open the enclosure during operation to avoid electric shock;It is prohibited to use it in flammable, strongly corrosive and variable environments.

Maintenance and Replacement

If the lens has cracks or severe scratches, stop the machine immediately for replacement and reduce the power.If the light source is damaged or deformed due to overheating, it is necessary to replace it with original accessories in time.Internal inspection and repair of the luminaire must be carried out by professionals, and the power plug must be unplugged before operation.

Power Safety
Users shall operate the equipment within its specified scope of use and check that the wiring of the equipment is correctly connected.Applicable voltage: 230V AC, standard configuration with 1.2M silicone cable (1.5mm²)When plugging or unplugging, hold the plug itself and never pull the power cable.For safety, it is essential to keep the grounding wire (yellow-green) connected to the ground.In case of a fault, unplug the power plug before opening the luminaire's enclosure.Check the cables and interfaces regularly or before use. If any damage is found, stop using immediately.Do not bundle the power cables with other signal cables to avoid confusion.The manufacturer shall not be liable for any damage caused by the unauthorized replacement of other types of light sources.
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Warning:

Contains dangerous voltage inside!
USE & OPERATION
Draw out 4Lighting Adjustment Flakes⑧,connect the power supply,until the light spots are the brightest,loosen the Nut for the Front Draw tube⑤,adjust the Front Draw tube③fore and aft until the margin of the light spots are the clearest.

PACKAGE SPECIFICATION 

	NO
	DESCRIPTION
	PICTURES
	UNITS
	QUANTITY

	1
	Body
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	PCS
	1

	2
	Power Cord    
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	3
	Signal Cords
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	1

	4
	Instruction manual
	
	PCS
	1


OPTIONAL ACCESSORIES (PURCHASED SEPARATELY) 

	NO
	DESCRIPTION
	PICTURES
	UNITS
	QUANTITY

	1
	LOGO Clamp
	[image: image5.png]



	PCS
	1

	2
	Shrink aperture
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	3
	Lights Hook
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	4
	safely cable
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PRODUCT INTRODUCTION

[image: image9.png]



The 200W Profile Spotlight is a lighting device that integrates professional light control and high color rendering performance. It emits bright and stable 3200K warm light, and with a high color rendering index (CRI > 95), it can accurately restore the true colors and delicate textures of illuminated objects, making every detail vivid and lifelike.Meanwhile, its fixed 19° beam angle, combined with soft light, spotlight, and light-cutting functions, allows precise control of light shape, delivering uniform and gentle light spots. It supports 0%-100% linear dimming and independent electronic strobing, flexibly adapting to different brightness requirements and dynamic light and shadow needs.Made of high-strength die-cast aluminum alloy, it features a streamlined appearance that balances aesthetics and durability. With an IP20 protection rating, it is suitable for indoor environments, boasting a stable structure and easy installation.Ideal for scenarios such as stage close-up lighting, exhibition hall exhibit focusing, and film/television shooting lighting setup, it efficiently creates a professional light and shadow atmosphere for various spaces, significantly enhancing the overall visual appeal.

COMPONENTS
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1.Color Chip frame Fixer     9.Four-star small bake lite screw  


2.Color Flake Calipers       10.Aluminum upper cover  

3.Aluminum cylinder         11.Aluminum side cover 

4.Focusing slot              12.Cooperate with the activity slot

5.Hexagon Socket Screw
13.Slotted plastic bake lite

6.Design Adjustment Tube
14.Handle fit piece

7.Slot for Iris
15.Slot for Gobo Holder

8.Lighting Adjustment Flake 
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MENU

A．MENU             

B．UP


       

C．DOWN





D．ENTER
  
    

Instructions: Press function key a to cycle out 6 different function effects. The first two digits of the nixie tube represent the current function (refer to the menu). The last two digits represent the. Address code. Or speed, mode and parameter of the function. Press B or C key to modify the parameter value. Press D to confirm.

Function Comparison Table of Key Display Window (All functions can be confirmed and saved by pressing the D key after selection)
	NO.
	MENU
	 FEATURES 
	INTRODUCTIONS

	1
	DMX-ADDR 001
	DMX512 address code setting001
	Press the up and down key to adjust address code, according to determine the key.

	2
	R-DIMMER 255
	LED brightness control 255
	According to the up and down keys to adjust the LED brightness, save according to determine the key.

	3
	G-DIMMER 255
	LED brightness control 255
	According to the up and down keys to adjust the LED brightness, save according to determine the key.

	4
	P-STROBE 255
	Strobe speed regulation255
	Press up and down key to adjust stroboscopic speed, (0-127) pulse stroboscopic from slow to fast（ 128-255). OK key to save.

	5
	DMX-KEEP ON/OFF
	DMX signal choice
	According to choose whether to keep up and down key, according to determine the key to save.

	6
	BK-LIGHT

ON/OFF
	Backlight switch selection.
	Press up and down to select the backlight screen saver. OK key to save.

	7
	Now Temp
	LED bead temperature display.


	Display the current working temperature of the lamp bead


CHANNEL DESCRIPTION

1.Channel Mode: (4CH）
	CH
	FUNCTION
	INTRODUCTIONS

	CH1
	Dimmer
	(0－255）LED dimming, linear dimming, from dark to bright

	CH2
	Strobe
	(0-127)  pulse stroboscopic from slow to fast（ 128-255).

	CH3
	WW Dim


	Linear dimming, from dark to bright

	CH4
	CW Dim
	Linear dimming, from dark to bright


PRODUCT SPECIFICATIONS 

Input voltage:AC100-240V、50/60HZ、SXPL 21K
Power: 200W 

LED Luminous: LED 3200K+6500K 
Control: Standard DMX512

Channels: 4CH


Linear dimming: 0-100%

Beam angle: 19°
Functional effects:Soft light, focused light, and blocking light

Color rendering index (CRI): >95
Product Appearance: High-strength die-cast aluminum alloy, streamlined appearance design
Protection class: IP20
Max.Ambient Temperature : <40℃

Max.Surface Temperature : <75℃

Light size: 650×280×184MM
Net Weigh: 8.4KG

FIXTURE SIZE
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ILLUMINANCE PARAMETERS

Illuminance Meter
[image: image12.jpg]Full 1250 325 185 92 55 38
CcW 720 188 110 56 33 23
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Range (m) 5 10 15 20 25 30
Beam (m) 2.5 4.8 7.2 9.6 12 14.4



    
 Spectrum diagram
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Design Flake 

If you want to achieve a pattern effect, you must first purchase a pattern plate. Loosen the nut of the pattern plate slot ⑮, then move it forward until the pattern holder can be placed in. Take out and insert the pattern plate. Adjust the position of foot ③ back and forth until the clearest pattern is obtained, then fix the position of the foot.

Color Flake 

If wanting colors,please clip the color flake with the color flake clip,open the Color Flake Calipers & then insert the color flake.

REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.

Thank you again for your patronage!
We will be offering sincere service as always,

Wish you have a good lighting journey!


