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USER MANUAL

	KEEP THIS USER MANUAL FOR FUTURE NEEDS


ADVICE BEFORE USE 
Read these instruction carefully.As soon as the equipment is delivered,Open packing and inspect the equipment Carefully. If you notice any damage,immediately contact the transport company and register your Complaint in due form listing the defects. Be sure that this equipment left our factory in perfect condition. Check if the received equipment is consistent with the delivery notice and if this delivery notice is consistent with your order.If it is not ,immediately contact with you supplier. 
GENERAL REMARKS 
This luminaire is lighting equipment designed for professional use only indoors in theatres and television or film studios.It must imperatively be connected to earth by means of its earth wire. To prevent any electrical shock,this equipment should not be opened when functioning. 
NEVERTHELESS
Any part or lenses have to be replaced if they are visibly damaged and their efficiency might be reduced,for example in case of deep cracks or scratches.The lamp must be changed if damaged or distorted by heat.If internal access is needed for control,service or repair purposes always refer to qualified personnel. In all events,always unplug the power supply cable before opening. It is the user’s responsibility to use the luminaire for its intended purpose and to check 
the equipment that might be connected to it. This luminaire is a piece of professional equipment designed for easy and simple use. Nevertheless,always refer to qualified personnel for any installation or repair work. 
IMPORTANT REMARK 
Power supply cables and other connections are essential for your equipment and contribute greatly to a safe and trouble free operation. Always hold the plug when disconnecting a cable,never pull the cable.Never use cables 
or connectors in bad condition,check them before installation and periodically thereafter.Never tie power supply and data cables together. 
ELECTRICAL CONNECTION 
This luminaire is designed for operating at a nominal voltage of 230V.It is fitted with a 1.2msilicone power supply cable(3*1.5mm²) For your own safety,make sure the earth wire(yellow-green)is ALWAYS connected to earth.
OVERVIEW
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1.Big light blocking leaf
2.Small light blocking leaf
3.Frosted lens
4.Cast aluminum housing
5.Handle
6.Fixing plate of light barrier blade
7.Power box
8.Light barrier bracket
9.Slotted nut
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DISPLAY 
	NO.
	MENU
	INSTRUCTION

	1
	DMX Address Code

001
	Press the Up/Down keys to adjust the address code, then press the Confirm key to save.

	2
	Brightness: 000-100
	(0-100) Brightness from dark to bright. Press the Up/Down keys to adjust brightness, then press the Confirm key to save.

	3
	Color Temperature: 2000-12000K
	Press the Up/Down keys to adjust color temperature, then press the Confirm key to save.

	4
	Fine Tuning: -100 ~ +100
	Press the Up/Down keys to adjust color temperature/color fineness, then press the Confirm key to save.

	5
	Saturation: 000-100
	(0-100) Saturation from low to high. Press the Up/Down keys to adjust saturation, then press the Confirm key to save.

	6
	R Dimming: 000-100
	(0-100) Brightness from dark to bright. Press the Up/Down keys to adjust R brightness, then press the Confirm key to save.

	7
	G Dimming: 000-100
	(0-100) Brightness from dark to bright. Press the Up/Down keys to adjust G brightness, then press the Confirm key to save.

	8
	B Dimming: 000-100
	(0-100) Brightness from dark to bright. Press the Up/Down keys to adjust B brightness, then press the Confirm key to save.

	9
	3200K Dimming: 000-100
	(0-100) Brightness from dark to bright. Press the Up/Down keys to adjust W brightness, then press the Confirm key to save.

	10
	5600K Dimming: 000-100
	(0-100) Color temperature from low to high. Press the Up/Down keys to adjust Y color temperature, then press the Confirm key to save.

	11
	Strobe: 000-100
	(0-100) Strobe from slow to fast. Press the Up/Down keys to adjust strobe, then press the Confirm key to save.

	12
	Effect: 000-010
	(0-10) 10 types of effects. Press the Up/Down keys to select effect, then press the Confirm key to save.。

	13
	Speed: 000-100
	(0-100) Effect from slow to fast. Press the Up/Down keys to adjust effect speed, then press the Confirm key to save.

	14
	Fan: On/Off
	Press the Up/Down keys to select On/Off, then press the Confirm key to save.

	15
	DMX Hold: On/Off
	Press the Up/Down keys to select On/Off, then press the Confirm key to save.

	16
	Language (Lang)
	Press the Up/Down keys to set Chinese/English display, then press the Confirm key to save.

	17
	Fixture Operating 

Time: 0000:00
	/


CHANNEL LIST

	CH
	FUNCTION
	VALUE
	DESCRIPTION
	REMARK

	CH1
	Brightness
	000-255
	0-100%
	

	CH2
	Color Temp
	000-255
	2000-12000K
	

	CH3
	Fine color
	000-255
	-100-+100
	

	CH4
	Saturation degree
	000-255
	0-100%
	

	CH5
	R
	000-255
	0-100%
	

	CH6
	G
	000-255
	0-100%
	

	CH7
	B
	000-255
	0-100%
	

	CH8
	3200K
	000-255
	0-100%
	

	CH9
	5600K
	000-255
	Color temperature adjustable from 2700K to 6500K


	

	CH10
	Fan
	000-255
	000-127: Fan Off, 

128-255: Fan On;
	

	CH11
	Strobe
	000-255
	Higher value means faster speed.
	

	CH12
	Effect
	000-255
	10 kinds of effects
	Valid for RGBWY.

	CH13
	Effect Speed
	000-255
	Higher value means faster speed.
	Valid for RGBWY.


TECHNICAL PARAMETERS

Input power : AC100-240V, 50-60Hz

input power : 200W

Light source : 1200pcs LED

Color: R,G,B,3200K,5600K

Color temperature : 2000-12000K

CRI:  ≥ 95

Control panel : digital display screen

Life of lamp beads : 50000h

Dimming : 0-255,0 % -100 % linear dimming, smooth without flicker

Optical Material : Glass Threaded Concentretor

Optical angle : 120 °

Protection level : IP20

Control mode : international standard DMX512 signal, self-propelled, master-slave

Number of channels : 13 DMX channels

Product size : 530* 130*312mm ( LW H )

Product net weight : 6.7kg

FIXTURE SIZE
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ILLUMINATION DIAGRAM
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REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.

Thank you again for your patronage!
We will be offering sincere service as always,

Wish you have a good lighting journey!


