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USER MANUAL

	KEEP THIS USER MANUAL FOR FUTURE NEEDS




1

MENU：


2
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A            B          C         D


A． Menu
B． Up
C． Down
D． Enter

Operation instructions: Press the function key A to circulate 10 different function effects, the first two digits of the digital tube represent the current function (refer to the function table). The last two digits represent the location of the function. Address code, or speed, parameters. Press B or C to change its parameter value. Press D to confirm.
DMX DISPLAY （Press D to confirm all functions selected）

	NO.
	DISPLAY
	DETAIL

	1
	A001
	DMX address，（001—512）
B 、C Key to add or subtract address values

	2
	6/12/8 /4/2CH
	Multiple channel modes to choose

	3
	CC00
	Jumping （00—12）
B 、C to change effect

	4
	LL50
	Jumping speed （00—12）
B 、C to change effect speed

	5
	CP 99
	fade，（01—99）
B 、C fade,pulse speed

	6
	DE99
	Strobe（01—99） 
B、C to change fade,pulse speed

	7
	BEBE
	Sound

	8
	o255
	WW color, （000—255）
B 、C change

	9
	Y255
	CW color，（000—255）
B 、C change

	10
	n255
	Strobe，（000—255）
B 、C change

	11
	ON/OFF
	
Display saver on/off




FUNCTION DISPLAY (D to save)
	NO.
	DISPLAY
	DETAIL

	1
	R235
	COB1 WW current 20-255,B、C to change

	2
	G235
	COB1 CW current 20-255,B、C to change

	3
	B235
	COB2 WW current 20-255,B、C to change

	4
	o235
	COB2 CW current 20-255,B、C to change

	5
	Y255
	COB3 WW current 20-255,B、C to change

	6
	P235
	COB3 CW current 20-255,B、C to change

	7
	A235
	COB4 WW current 20-255,B、C to change

	8
	n235
	COB4 CW current 20-255,B、C to change

	9
	T080
	DMX dimmer speed 0-255,B、C to change

	10
	C-60
	Temperature control sets the temperature 40-70 degree,B、C to change




DMX512 CHANNEL (6CH)

	NO.
	FUNCTION
	DETAIL

	1CH
	Dimmer
	COB dimmer,liner dimmer,from the dark to bright

	2CH
	Strobe
	Strobe from slow to fast

	








3CH
	








Function
	0-5 Null
6--20：   Jumping 1；
21—35: Jumping 2；
36—50: Jumping 3；
51—65: Jumping 4；
66—80: Jumping 5；
81—95: Jumping 6；
96—105: Jumping 7；
106—110: Jumping 8；
111—125: Jumping 9；
126—140: Jumping 10；
141—155: Jumping 11；
156—170: Jumping 12；
170—185: Jumping 1；
186—200: Jumping 2；
201—215: Jumping 3；

216—230: Strobe ;
231—255: Strobe by sound

	4CH
	Function
Speed
	Function speed, from slow to fast

	5CH
	WW color
dimmer
	WW color dimmer,liner dimmer,from the dark to bright

	6CH
	CW color
dimmer
	CW color dimmer,liner dimmer,from the dark to bright



DMX512 CHANNEL (12CH)

	NO.
	FUNCTION
	DETAIL

	1CH
	Dimmer
	COB dimmer,liner dimmer,from the dark to bright

	2CH
	Strobe
	Strobe from slow to fast

	










3CH
	










Function
	0-5 Null
6--20：   Jumping 1；
21—35: Jumping 2；
36—50: Jumping 3；
51—65: Jumping 4；
66—80: Jumping 5；
81—95: Jumping 6；
96—105: Jumping 7；
106—110: Jumping 8；
111—125: Jumping 9；
126—140: Jumping 10；
141—155: Jumping 11；
156—170: Jumping 12；
170—185: Jumping 1；
186—200: Jumping 2；
201—215: Jumping 3；
216—230: Strobe ;
231—255: Strobe by sound

	4CH
	Function
Speed
	Function speed, from slow to fast

	5CH
	WW 1 color
dimmer
	WW 1 color dimmer,liner dimmer,from the dark to bright

	6CH
	CW 1 color dimmer
	CW1 color dimmer,liner dimmer,from the dark to bright

	7CH
	WW 2 color
dimmer
	WW 2 color dimmer,liner dimmer,from the dark to bright

	8CH
	CW 2 color dimmer
	CW 2 color dimmer,liner dimmer,from the dark to bright

	9CH
	WW 3 color
dimmer
	WW  3 color dimmer,liner dimmer,from the dark to bright

	10CH
	CW 3 color dimmer
	CW 3 color dimmer,liner dimmer,from the dark to bright

	11CH
	WW 4 color
dimmer
	WW 4 color dimmer,liner dimmer,from the dark to bright

	12CH
	CW 4 color dimmer
	CW 4 color dimmer,liner dimmer,from the dark to bright



DMX CHANNEL (8CH)

	NO.
	FUNCTION
	DETAIL

	1CH
	WW 1 color
dimmer
	WW 1 color dimmer,liner dimmer,from the dark to bright

	2CH
	CW 1 color dimmer
	CW1 color dimmer,liner dimmer,from the dark to bright

	3CH
	WW 2 color
dimmer
	WW 2 color dimmer,liner dimmer,from the dark to bright

	4CH
	CW 2 color dimmer
	CW 2 color dimmer,liner dimmer,from the dark to bright

	5CH
	WW 3 color
dimmer
	WW  3 color dimmer,liner dimmer,from the dark to bright

	6CH
	CW 3 color dimmer
	CW 3 color dimmer,liner dimmer,from the dark to bright

	7CH
	WW 4 color
dimmer
	WW 4 color dimmer,liner dimmer,from the dark to bright

	8CH
	CW 4 color dimmer
	CW 4 color dimmer,liner dimmer,from the dark to bright




DMX CHANNEL (4CH)

	NO.
	FUNCTION
	DETAIL

	1CH
	Dimmer
	COB dimmer,liner dimmer,from the dark to bright

	2CH
	WW dimmer
	WW dimmer,liner dimmer,from the dark to bright

	3CH
	CW dimmer
	CW dimmer,liner dimmer,from the dark to bright

	4CH
	Strobe 
	Strobe from slow to fast
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DMX CHANNEL (2CH)

	NO.
	FUNCTION
	DETAIL

	1CH
	WW dimmer
	WW dimmer,liner dimmer,from the dark to bright

	2CH
	CW dimmer
	CW dimmer,liner dimmer,from the dark to bright




RDM

	NO.
	FUNCTION
	DETAIL

	1
	Feedback (address code)
	Can be changed freely

	2
	Feedback (channel mode)
	Can be changed freely

	3
	Feedback(device temperature)
	Can’t be changed freely



TECHNICAL PARAMETER
[bookmark: OLE_LINK5]Voltage: AC100~240V,50/60HZ
Power consumption: 400W
Light source: 4pcs 100W WW+CW
LED control: individual controllable
[bookmark: _GoBack]DMX channels: 6/12/8//4/2CH
Color temperature:3200K~7000 Adjustable
Dimmer: 16bit 0~100% linear dimmer
Beam angle: 38 degree
Work temperature: -30degreee~50degree
Control model: DMX512,Auto,Master-Slave,Sound active
Strobe: 1~30HZ
House: Metal,black
Connection model: DMX in/out, Power IN/OUT
IP grade: IP65
Size: 394*245*392
Weight: 17kg









FIXTURE SIZE
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REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.





Thank you again for your patronage!
We will be offering sincere service as always,
Wish you have a good lighting journey!
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