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USER MANUAL

	KEEP THIS USER MANUAL FOR FUTURE NEEDS



MENU
1.Keystroke diagram
[image: ]

MENU： function key         
UP： additional key
DOWN： Subtract key    
ENTER： Confirmation key
2.  Button Description MENU function key:
Press the function  key  MENU will  loop  out of the table  (1) function, digital tube in front of 1-2 to represent the current function. The latter 2-3  digits  represent  the  speed,  effect  and  other  parameters  of  the function;  the  parameter  values  can  be  modified  by  pressing  UP  or DOWN  key;  and  the  parameter  value  can  be  confirmed  by  pressing ENTER key.
UP additional key:
Press the key can be added, the length of more than 2 seconds if added continuously;
DOWN Subtract key:
According to the invention, the key can be reduced, and the length can be reduced continuously for more than 2 seconds;
ENTER Confirmation key:
Press the key to save the currently set parameter function, the next boot automatically run the save function.









	NO
	DIS
	VALUE
	FUNCTION

	1
	d001
	001- 512
	DMX512 Address code setting -4 channel mode

	2
	A001
	001- 512
	DMX512 Address code setting -8 channel mode

	3
	U255
	000 - 255
	Cold  white  dials,  from  dark  to bright.

	4
	C255
	000 - 255
	Warm  white  dials  from  dark  to bright.

	5
	FH99
	01 - 99
	Stroboscopic, from slow to fast.

	6
	CC99
	01 - 99
	Jump, from slow to fast.

	7
	DE99
	01 - 99
	Gradient, from slow to fast.

	8
	CP99
	01 - 99
	Pulse change, from slow to fast.

	9
	S0UD
	-
	Sound control



CHANNEL LIST
	CH 8
	FUNCTION
	DESCRIPTION

	CH1
	Dimming
	dimming， From dark to bright

	CH2
	CW1 dimming
	WW1 dimming， From dark to bright

	CH3
	WW2 dimming
	WW2 dimming， From dark to bright

	CH4
	CW1 dimming
	WW1 dimming， From dark to bright

	CH5
	WW2 dimming
	WW2 dimming， From dark to bright

	CH6
	Total strobe
	Total strobe, slow to fast

	
CH7
	
Function
	0-50:DMX dimming; 51-100: common color output (8); 101-150: jump;
151-200: gradual; 201-250 pulse;
251-255: voice control

	CH8
	Function speed
	Functional speed, from slow to fast




	CH 4
	FUNCTION
	DESCRIPTION

	CH1
	CW1 dimming
	WW1 dimming， From dark to bright

	CH2
	WW2 dimming
	WW2 dimming， From dark to bright

	CH3
	CW1 dimming
	WW1 dimming， From dark to bright

	CH4
	WW2 dimming
	WW2 dimming， From dark to bright



TECHNICAL PARAMETER
[bookmark: OLE_LINK5]Voltage: AC100~240V,50/60HZ
Power consumption: 200W
Light source: 2pcs 100W Warm white 
LED control: individual controllable
DMX channels: 4/8CH
Color temperature:3200K~7000 Adjustable
Dimmer: 16bit 0~100% linear dimmer
Beam angle: 38 degree
Work temperature: -30degreee~50degree
Control model: DMX512,Auto,Master-Slave,Sound active
Strobe: 1~30HZ
House: Metal,black
Connection model: DMX in/out, Power IN/OUT
IP grade: IP20
Size: 375*301*180MM
Weight: 3kg

FIXTURE SIZE
[bookmark: _GoBack]
[image: 截屏2026-07-07 18.17.54]












REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.





Thank you again for your patronage!
We will be offering sincere service as always,
Wish you have a good lighting journey!
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