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USER MANUAL

	KEEP THIS USER MANUAL FOR FUTURE NEEDS
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A．Function key B．UP key C．Down key
D．Enter key



A	B	C	D
Operate introduce: Press function key “A” will circulate seven different function effects, The line of words upside LCD stand for the present working function ( please refer to the function table.), the under line stands for LCD shows what address code or speed parameter of this function is at.

DISPLAY MENU FUNCTION ( Press D key to confirm after choosing certain function)
	NO.
	DISPLAY
	FUNCTION

	1
	A002
	12 channel address code, UP/DOWN key selects the address code (A001 ~ A512), press the confirmation key (ENTER key) to save the address code 

	2
	L001
	4 channel mode, UP/DOWN key selects the address code (L001 ~ L512), press the confirmation key (ENTER key) to save the address code 

	3
	d002
	2 channel mode, the UP/DOWN key selects the address code (d001 ~ d512), press the confirmation key (ENTER key) to save the address code 

	4
	M000
	macro

	5
	S000
	Functional mode speed

	6
	P000
	The frequency flash is from slow to fast

	7
	R255
	(r000-r255) up, manually modify the bulb 1 cold white brightness 

	8
	G255
	(G000 - G255) upward, downward manually modify the lamp bead 1 warm white brightness 

	9
	B255
	(B000 - B255) upward, manually modify the lamp bead 2 cold white brightness 

	10
	W255
	(w00-w255) upward, downward manually modify the lamp ball 2 warm and white brightness 

	11
	Y255
	(y000-y255) upward, downward manually modify the bulb 3 cold white brightness 

	12
	I255
	(i000-i255) upward, downward manually modify the bulb 3 warm white brightness 

	13
	F255
	(F000 - F255) up and down manually modify the bulb 4 cold white brightness 

	14
	H255
	(H000 - H255) upward, downward manually modify the bulb 4 warm white brightness 



CHANNEL LIST

12CH Description
	NO.
	FUNCTION
	DESCRIPTION

	1CH
	000-255
	The total dimming

	2CH
	000-255
	0-9 no stroboscopic
10-255 strobes speed from slow to fast

	3CH
	250-255
	macro

	4CH
	000-255
	Built-in mode speed adjustment

	5CH
	000-255
	R - light bulb 1 cold white linear dimming, from dark to light

	6CH
	000-255
	G - light bulb 1 warm white linear dimming, from dark to light

	7CH
	000-255
	B-lamp 2 cold white linear dimming, from dark to light

	8CH
	000-255
	W - bulb 2 warm white linear dimming, from dark to light

	9CH
	000-255
	Y - light bulb 3 cold white linear dimming, from dark to light

	10CH
	000-255
	I - light bulb 3 warm white linear dimming, from dark to light

	11CH
	000-255
	F - bulb 4 cold white linear dimming, from dark to light

	[bookmark: _GoBack]12CH
	000-255
	H - bulb 4 warm white linear dimming, from dark to light




4CH Description
	NO.
	FUNCTION
	DESCRIPTION

	1CH
	000-255
	Tuned light

	2CH
	000-255
	R/G/Y/F brightness is adjusted from dark to light

	3CH
	000-255
	B/W/I/H brightness is adjusted from dark to light

	4CH
	000-255
	0-9 no stroboscopic
10-255 strobes speed from slow to fast




2CH Description
	NO.
	FUNCTION
	DESCRIPTION

	1CH
	All Dimmer
	From dark to bright

	2CH
	000-255
	0-9 no stroboscopic
10-255 strobes speed from slow to fast



















TECHNICAL PARAMETER

[bookmark: OLE_LINK5]Voltage: AC100~240V,50/60HZ
Power consumption: 400W
Light source: 4pcs 100W Warm white 
LED control: individual controllable
DMX channels: 12/4/2CH
Color temperature:3200K~7000 Adjustable
Dimmer: 16bit 0~100% linear dimmer
Beam angle: 38 degree
Work temperature: -30degreee~50degree
Control model: DMX512,Auto,Master-Slave,Sound active
Strobe: 1~30HZ
House: Metal,black
Connection model: DMX in/out, Power IN/OUT
IP grade: IP20
Size:36x38x20CM
Weight: 9.0K


FIXTURE SIZE
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REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.







Thank you again for your patronage!
We will be offering sincere service as always,
Wish you have a good lighting journey!
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