

MINI P1 IP




[bookmark: _GoBack]



[image: 截屏2026-07-07 18.02.49]








USER MANUAL

	KEEP THIS USER MANUAL FOR FUTURE NEEDS








1

DISPLAY

[image: 转换高清线条图]     

A．Function
B．UP
C．DOWN
D．ENTER
 
Function list

	MAIN MENU
	SUBMENU
	MENU FUNCTION DESCRIPTION

	System settings
	1. DMA
address
	Modify the DMA address code up or down (optional range of address codes 001-512), confirm to save, default to 001.

	
	2. Encoder
	Modify encoder on/off up or down, confirm key to save, default to on.

	
	3. X reversal
	Modify X up or down to reverse on/off, confirm to save, default to off.

	
	4. Y reversal
	Modify Y up or down to reverse on/off, confirm to save, default to off.

	Operating mode
	1.       Operation mode
	Select the operating mode up or down, such as MAX/voice control/automatic, and press the confirm button to save. The default mode is MAX.

	
	2.         Channel selection
	Select channel CH4. CH16. CH22. CH28. CH40 up or down to save

	










Manual
	1. Dimming
	Modify the dimming value up or down (adjustable range 000-255), confirm and save, default to 255.

	
	2.               RGB dimming
	Modify the RGB dimming value up or down (adjustable range 000-255), confirm to save, default to 000.

	
	3. RGB strobe
	Modify the RGB  flicker value up or down (adjustable range 000-255), confirm to save, default to 000.

	
	4. Red
	Modify the brightness of the red light bead up or down (adjustable range 000-255), confirm to save, default to 128.

	
	5. Green
	Modify the brightness of the green light bead up or down (adjustable range 000-255), confirm to save, default to 128.

	
	6. Blue
	Modify the brightness of the blue light bead up or down (adjustable range 000-255), confirm to save, default to 128.

	
	7. RGB mode
	Modify the RGB mode values up or down (adjustable range 000-255), confirm and save

	
	8. RGB speed
	Modify RGB speed values up or down (adjustable range 000-255), confirm and save

	
	9.   Background color
	Modify the background color parameter value up or down (adjustable range 000-255), confirm to save, default to 000.

	
	10. Background color tone light
	Modify  the  background  color tone  light parameter  values  up  or  down  (adjustable range 000-255), confirm to save, default to 000.


	
	11.   W   strobe white
	Modify the brightness of the white light beads up or down (adjustable range 000-255), confirm to save, default to 128.

	
	12. W strobe
	Modify the W strobe value up or down (adjustable range 000-255), confirm and save

	
	13. W mode
	Modify the W mode value up or down (adjustable range 000-255), confirm and save

	
	14. W speed
	Modify the W speed value up or down (adjustable range 000-255), confirm and save

	
	15.         RGBW mode
	Modify the RGBW mode value up or down (adjustable range 000-255), confirm and save

	
	16.         RGBW speed
	Modify the RGBW speed value up or down (adjustable range 000-255), confirm and save

	Display Settings
	1.       Language selection
	Select Chinese/EN (English) up or down, confirm to save, default to Chinese.

	
	2.         Inverted Display
Settings
	Select up or down to turn off/on the inverted display setting, confirm to save, default to off.

	
	3. Screen saver
	Select up or down to turn off/on screen saver, confirm to save, default to on.

	
	4.        Software version
	G45A program identification code, cannot be modified.

	Factory settings
	Display,  please enter password! Change   up   or down   to   138, then  press  the confirm  button
to     enter     the
factory settings.
	1. Red
	Modify  parameters  up  or  down  (range  000-255),  confirm  to  save, default to 255.

	
	
	2. Green
	Modify  parameters  up  or  down  (range  000-255),  confirm  to  save, default to 255.

	
	
	3. Blue
	Modify the red light bead current (032-255) up or down, confirm and save, default to 255.

	
	
	4. White
	Modify the green light bead current (032-255) up or down, confirm and save, default to 255.

	
	
	5. Direction
	Modify direction up or down

	
	
	6. LED
	LED sequence selection

	
	
	7. Logo
	Select 000/001 up or down, confirm to save, default to 000.

	
	
	8.
Temperature
	Select 000-070 up or down, confirm to save, default to 060.

	
	
	9.
Temperature - Fan
	Temperature Fan Control
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CHANNEL LIST 
(After power on, set the address codes for all lighting fixtures. Connect all lighting fixtures in parallel with a three core signal wire to the DMX512 console. The address code will stop flashing, indicating that the DMX512 console signal has been sent to the lighting fixtures. Use the DMX512 console to control the relevant functions according to the instructions of each channel.)

CH4Channel Description：
	CH
	VALUE
	FUNCTION

	1
	000-255
	R

	2
	000-255
	G

	3
	000-255
	B

	4
	000-255
	W




CH16Channel Description：
	CH
	VALUE
	FUNCTION

	1
	000-255
	Total dimming

	2
	000-255
	RGB overall dimming

	3
	000-255
	R

	4
	000-255
	G

	5
	000-255
	B

	6
	000-255
	RGB strobe

	7
	000-255
	RGB mode

	8
	000-255
	RGB speed

	9
	000-255
	Background color

	10
	000-255
	Background color tone light

	11
	000-255
	white

	12
	000-255
	W strobe

	13
	000-255
	W mode

	14
	000-255
	W speed

	15
	000-255
	RGBW mode

	16
	000-255
	RGBW speed




CH22Channel Description：
	CH
	VALUE
	FUNCTION

	1
	000-255
	Total dimming

	2
	000-255
	RGB overall dimming

	3
	000-255
	R

	4
	000-255
	G

	5
	000-255
	B
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	6
	000-255
	RGB strobe

	7
	000-255
	RGB mode

	8
	000-255
	RGB speed

	9
	000-255
	Background color

	10
	000-255
	Background color tone light

	11
	000-255
	White 1

	12
	000-255
	White 2

	13
	000-255
	White 3

	14
	000-255
	White 4

	15
	000-255
	White 5

	16
	000-255
	White 6

	17
	000-255
	White 7

	18
	000-255
	W strobe

	19
	000-255
	W mode

	20
	000-255
	W speed

	21
	000-255
	RGBW mode

	22
	000-255
	RGBW speed




CH28Channel Description：
	CH
	VALUE
	FUNCTION

	1
	000-255
	R1

	2
	000-255
	G1

	3
	000-255
	B1

	4
	000-255
	R2

	5
	000-255
	G2

	6
	000-255
	B2

	7
	000-255
	R3

	8
	000-255
	G3

	9
	000-255
	B3

	10
	000-255
	R4

	11
	000-255
	G4

	12
	000-255
	B4

	13
	000-255
	R5

	14
	000-255
	G5

	15
	000-255
	B5

	16
	000-255
	R6

	17
	000-255
	G6

	18
	000-255
	B6

	19
	000-255
	R7

	20
	000-255
	G7

	21
	000-255
	B7

	22
	000-255
	White 1

	23
	000-255
	White 2
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	24
	000-255
	White 3

	25
	000-255
	White 4

	26
	000-255
	White 5

	27
	000-255
	White 6

	28
	000-255
	White 7




CH40Channel Description
	CH
	VALUE
	FUNCTION

	1
	000-255
	Total dimming

	2
	000-255
	RGB overall dimming

	3
	000-255
	R1

	4
	000-255
	G1

	5
	000-255
	B1

	6
	000-255
	R2

	7
	000-255
	G2

	8
	000-255
	B2

	9
	000-255
	R3

	10
	000-255
	G3

	11
	000-255
	B3

	12
	000-255
	R4

	13
	000-255
	G4

	14
	000-255
	B4

	15
	000-255
	R5

	16
	000-255
	G5

	17
	000-255
	B5

	18
	000-255
	R6

	19
	000-255
	G6

	20
	000-255
	B6

	21
	000-255
	R7

	22
	000-255
	G7

	23
	000-255
	B7

	24
	000-255
	RGB strobe

	25
	000-255
	RGB mode

	26
	000-255
	RGB speed

	27
	000-255
	Background color

	28
	000-255
	Background color tone light

	29
	000-255
	White 1

	30
	000-255
	White 2

	31
	000-255
	White 3

	32
	000-255
	White 4

	33
	000-255
	White 5

	34
	000-255
	White 6
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	35
	000-255
	White 7

	36
	000-255
	W strobe

	37
	000-255
	W mode

	38
	000-255
	W speed

	39
	000-255
	RGBW mode

	40
	000-255
	RGBW speed




TECHNICAL PARAMETERS
Voltage: AC100~240V 50/60HZ
Power: 350W
Lamp beads: 63 pieces 5050-RGB 0.3W
Control mode: DMX512, self-propelled, master-slave, voice control, with RDM function
Channel: CH4.CH16.CH22.CH28.CH40
Dimming: 16bit 0-100% linear dimming
Features: auxiliary lighting+dyeing+flash+running horse
Working temperature: -30  ° C~50  ° C
Strobe frequency: 1-30Hz
Appearance: Metal, black
Connection method: DMX512 input/output
Power input and output.
IP level: IP67
Size: 550*121*510MM
Net weight:


FIXTURE SIZE
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REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.











Thank you again for your patronage!
We will be offering sincere service as always,
Wish you have a good lighting journey!
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