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USER MANUAL


	KEEP THIS USER MANUAL FOR FUTURE NEEDS
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Thank you for your patronage!
We are confident that our excellent products and service can satisfy you.
For your own safety, please read this user manual carefully before installing the device.
In order to install, operate, and maintain the lighting safety correctly.
We suggest that the installation and operation should be done by the verified technician and follow the instruction strictly.
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CAUTION!
Keep this device away from rain and moisture!
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	CAUTION!
Unplug mains lead before opening the housing!


Every person involved with the installation, operation and maintenance of this device has to:
-be qualified
-follow carefully the instructions of this manual
INTRODUCTION:
Thank you for having chosen this professional moving head.
You will see you have acquired a powerful and versatile device.
Unpack the device. Inside the carton box you should find:
1.   One power in cable
2.   One 3-Pin DMX cable
3.   Two folding clamps
4.   One safety cable
5.   One English user manual
（Flight case is optional, please contact your dealer）
Please check carefully that there is no damage caused by transportation. Should there be any questions, please consult your dealer and don’t install this device.
GENERAL GUIDELINES
This device is a lighting effect for a professional use on stages, TV, in discotheques, theaters, etc.

This fixture is only allowed to be operated with the max alternating current which stated in the technical specifications in 6th page of this manual.
Lighting effects are not designed for permanent operation. Consistent operation breaks may ensure that the device will serve you for a long time without defects.

Do not shake the device. Avoid brute force when installing or operating the device.
While choosing the installation-spot, please make sure that the device is not exposed to extreme heat, moisture or dust. Please don’t project the beam onto combustible substances. The minimum distance between light-output from the projector and the illuminated surface must be more than 0,5 meter.
If you use the quick lock cam in hanging up the fixture, please make sure the quick lock fasteners turned in the quick lock holes correctly.
Operate the device only after having familiarized with its functions. Do not permit operation by persons not qualified for operating the device. Most damages are the result of unprofessional operation.

Please use the original packaging if the device is to be transported.
For safety reasons, please be aware that all modifications on the device are forbidden. If this device will be operated in any way different to the one described in this manual, the product may suffer damages and the guarantee becomes void. Furthermore, any other operation may lead to short-circuit, burns, electric shock, crash, etc.
SAFETY INSTRUCTIONS

	Δ
	CAUTION!
Be careful with your operations. With a dangerous voltage you can suffer     a dangerous electric shock when touching wires!



This device has left the factory in perfect condition. In order to maintain this condition and to ensure a safe operation, it is absolutely necessary for the user to follow the safety instructions and warning notes written in this user manual.
1. In order to guarantee the product’s life, please don’t put it in the damp places or even the environment over 60degress.
2. Always mount this unit in safe and stable matter.
The qualified professionals are allowed to carry out the lamp installation, operation and maintenance, but they must guarantee to operate in strict accordance with the instructions referred to.
▲      Important:
Damages caused by the disregard of this user manual are not subject to warranty. The dealer will not accept liability for any resulting defects or problems.
If the device has been exposed to temperature changes due to environmental changes, do not switch it on immediately. The arising condensation could damage the device. Leave the device switched off until it has reached room temperatures.
This device falls under protection-class Ⅰ. Therefore it is essential that the device be earthed.
The electric connection must carry out by qualified person.


Make sure the power cord is never crimped or damaged by  sharp edges. If this would be the case, replacement of the cable must be done by an authorized dealer.
Always disconnect from the mains, when the device is not in use or before cleaning it. Only handle the power cord by the plug. Never pull out the plug by tugging the power cord.
During initial start-up some smoke or smell may arise. This is a normal process and does not necessarily mean that the device is defective, it should decrease gradually.
Please don’t project the beam onto combustible substances.
If the external flexible cable or cord of this luminaire is damaged, it shall be exclusively replaced by the manufacturer or his service agent or a similar qualified person in order to avoid a hazard.

	[image: ]CAUTION!
Never touch the device during operation!
The housing may heat up!
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Never look directly into the light source,
As sensitive persons may suffer an epileptic shock.



Please be aware that damages caused by manual modifications to be the device are not subject to warranty. Keep away from children and non-professionals.
CLEANING AND MAINTENANCE
1. To reduce the risk of electrical shock or fire, do not expose this unit to rain or moisture.
2. Do not spill water or other liquids into or on to your unit.
3. During long periods of non-use, disconnect the unit’s main power.
4. It should be installed in a well-ventilated place, at a distance of 50 centimeters or more with the walls. At the same time, please check if the fan and ventilation holes are unobstructed.

The following points have to be considered during the inspection
1)  All screws for installing the devices or parts of the device have to be tightly connected and must not be corroded.
2)  There  must  not  be  any  deformations  on  the  housing.  Fixations  and  installations  spots(ceiling, suspension, trussing).
3)  Mechanically moved parts must not show any traces of wearing and must not rotate with unbalances.
4)  The electric power supply cables must not show any damage, material fatigue or sediments. Further instructions depending on the installation spot and usage have to be adhered by a skilled installer and any safety problems have to be removed.
	Δ
	CAUTION!
Disconnect from mains before starting maintenance operation!



In order to make the lights in good condition and extend the life time, we suggest a regular cleaning to the lights.
1)  Clean the inside and outside lens each week to avoid the weakness of the lights due to accumulation of dust.
2)  Clean the fan each week.
3)  A detailed electric check by approved electrical engineer each three month, make sure that the circuit contacts are in good condition, prevent the poor contact of circuit from overheating.
We recommend a frequent cleaning of the device. Please use a moist, lint-free cloth. Never use alcohol or solvents
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A. Menu
B. Up
C. Down
D. Enter



A       B       C      D
Operating Instructions: Press function key A to exit the current menu, press D key to confirm, press B or C key to modify its parameter value or enter the next level menu.
LED  DISPLAY FUNCTIONAL CHART 
(All  the  functions  are  according the selected and then press the D to enter.)

	No.
	Display
	Functional Specification

	Addr
	A001-A512
	DMX address selection

	DMX
	5ch-19ch-65ch
	Channel selection

	Auto
	Pro 00-20
	Auto mode

	
	Sp 01-99
	

	Sound
	Pro 00-20
	Sound mode

	
	Se 01-99
	

	Display
	On/Off
	Backlight on/off

	Display Rev
	On/Off
	Display reverse on/off

	DMX Fail
	Blackout/ Manual / Auto / Hold
	The status of the disconnect signal is Off/Manual/Auto/Hold

	Firm Ware
	Vx.xx
	Version

	Time Info
	00H
	Service time of luminaire

	Temperature
	。
xx    c
	Temperature



Channel List
5 Channels 

	CH
	Function
	Value
	Description

	1
	ALL Dimmer
	0-255
	Master dimmer 0-100%

	2
	White Strobe
	0-8
	No function

	
	
	9-255
	Strobe speed from slow to fast

	
3
	Complete Dimmer
	0-39
	Dimmer 0~ 100%

	
	White 1 Dimmer
	40-79
	Dimmer 0~ 100%

	
	White 2 Dimmer
	80-119
	Dimmer 0~ 100%




	
	White 3 Dimmer
	120-159
	Dimmer 0~ 100%

	
	White 4 Dimmer
	160-199
	Dimmer 0~ 100%

	
	White 5 Dimmer
	200-239
	Dimmer 0~ 100%

	
	Complete Dimmer
	240-255
	Dimmer 0~ 100%

	4
	White Auto
	0-7
	No function

	
	
	8-255
	Auto effects

	5
	White Auto Speed
	0-255
	Auto speed from slow to fast



19 Channels 

	CH
	Function
	Value
	Description

	1
	ALL Dimmer
	0-255
	Master dimmer 0-100%

	2
	White Dimmer
	0-255
	Dimmer 0~ 100%

	




3
	




White Strobe
	0-16
	No strobe

	
	
	17-131
	Strobe from slow to fast

	
	
	132-139
	No strobe

	
	
	140-181
	Strobe slow open fast close, speed from slow to fast

	
	
	182-189
	No strobe

	
	
	190-231
	Strobe fast open slow close, speed from slow to fast

	
	
	232-255
	No strobe

	4
	White Auto
	0-7
	No function

	
	
	8-255
	Auto effects

	5
	White Auto Speed
	0-255
	Auto speed from slow to fast

	6
	RGB 1 Dimmer
	0-255
	Dimmer 0~ 100%

	7
	RGB 1 Strobe
	0-15
	No strobe

	
	
	16-255
	Strobe speed from slow to fast

	8
	Red 1
	0-255
	Red dimmer 0~ 100%

	9
	Green 1
	0-255
	Green dimmer 0~ 100%

	10
	Blue 1
	0-255
	Blue dimmer 0~ 100%

	11
	RGB 1 Auto
	0-7
	No function

	
	
	8-255
	Auto effects

	12
	RGB 1 Auto Speed
	0-255
	Auto speed selection

	13
	RGB 2 Dimmer
	0-255
	Dimmer 0~ 100%

	14
	RGB 2 Strobe
	0-15
	No strobe

	
	
	16-255
	Strobe speed from slow to fast

	15
	BackGround R
	0-255
	Background Red from dark to bright

	16
	BackGround G
	0-255
	Background Green from dark to bright




	17
	BackGround B
	0-255
	Background Blue from dark to bright

	18
	RGB 2 Auto
	0-7
	No function

	
	
	8-255
	Auto effects

	19
	RGB 2 Auto Speed
	0-255
	Auto speed from slow to fast



65 Channels 

	CH
	Function
	Value
	Description

	1
	White 1
	0-255
	Dimmer 0~ 100%

	2
	White 2
	0-255
	Dimmer 0~ 100%

	3
	White 3
	0-255
	Dimmer 0~ 100%

	4
	White 4
	0-255
	Dimmer 0~ 100%

	5
	White 5
	0-255
	Dimmer 0~ 100%

	6
	Red 1
	0-255
	Red 1 dimmer 0~ 100%

	7
	Green 1
	0-255
	Green 1 dimmer 0--100%

	8
	Blue 1
	0-255
	Blue 1 dimmer 0~ 100%

	9
	Red 2
	0-255
	Red 2 dimmer 0~ 100%

	10
	Green 2
	0-255
	Green 2 dimmer 0--100%

	11
	Blue 2
	0-255
	Blue 2 dimmer 0~ 100%

	12
	Red 3
	0-255
	Red 3 dimmer 0~ 100%

	13
	Green 3
	0-255
	Green 3 dimmer 0--100%

	14
	Blue 3
	0-255
	Blue 3 dimmer 0~ 100%

	....
	...
	...
	....

	63
	Red 20
	0-255
	Red 20 dimmer 0~ 100%

	64
	Green 20
	0-255
	Green 20 dimmer 0--100%

	65
	Blue 20
	0-255
	Blue 20 dimmer 0~ 100%

















TECHNICAL SPECIFICATION
Voltage：AC100-240V50/60Hz
Power： 350W
Light source：5*60W warm white or amber COB LEDs ，120PCS 5050 RGB 3in1 LEDs
Lifespan： 50000 hours
Channel： 5/19/65CH selection
Dimming frequency： up to 10KHz dimming refresh PWM frequency, no flicker camera shooting
Strobe：Independent electronic strobe
Control：DMX512/Artnet/Auto/Sound mode
IP Rating: IP20
Size： 880*140*190mm
Weight： 6.7KG








REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.
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Thank you again for your patronage!
We will be offering sincere service as always,
Wish you have a good lighting journey!
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