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USER MANUAL
	KEEP THIS USER MANUAL FOR FUTURE NEEDS


Thank you for your patronage!
We are confident that our excellent products and service can satisfy you. 

For your own safety, please read this user manual carefully before installing the device.

In order to install, operate, and maintain the lighting safety correctly. 

We suggest that the installation and operation should be done by the verified technician and follow the instruction strictly.

	                                                                           CAUTION! 
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            Keep this device away from rain and moisture!


	[image: image3.jpg]


CAUTION!

Unplug mains lead before device’s installation,cleaning and maintenance!


Every person involved with the installation, operation and maintenance of this device has to:

-be qualified

-follow carefully the instructions of this manual
INTRODUCTION

Thank you for having chosen this professional moving head.

You will see you have acquired a powerful and versatile device.

Unpack the device. Inside the carton box you should find:

One power in cable
One 3 Pin DMX cable(5 Pin optional)
One mounted bracket
One IR remote
One English user manual

（Flight case, Clamps are optional, please contact your dealer）

Please check carefully that there is no damage caused by transportation. Should there be any questions, please consult your dealer and don’t install this device.     
GENERAL GUIDELINES

This device is a lighting effect for a professional use on stages, TV, in discotheques, theaters, etc., The device was designed for indoor use only.

This fixture is only allowed to be operated with the max alternating current which stated in the technical specifications in 6th page of this manual.

Lighting effects are not designed for permanent operation. Consistent operation breaks may ensure that the device will serve you for a long time without defects.

Do not shake the device. Avoid brute force when installing or operating the device.

While choosing the installation-spot, please make sure that the device is not exposed to extreme heat, moisture or dust. Please don’t project the beam onto combustible substances. The minimum distance between light-output from the projector and the illuminated surface must be more than 0,5 meter.

If you use the quick lock cam in hanging up the fixture, please make sure the quick lock fasteners turned in the quick lock holes correctly.

Operate the device only after having familiarized with its functions. Do not permit operation by persons not qualified for operating the device. Most damages are the result of unprofessional operation.

Please use the original packaging if the device is to be transported.

For safety reasons, please be aware that all modifications on the device are forbidden. If this device will be operated in any way different to the one described in this manual, the product may suffer damages and the guarantee becomes void. Furthermore, any other operation may lead to short-circuit, burns, electric shock, crash, etc.

SAFETY INSTRUCTIONS
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CAUTION!

              Be careful with your operations. With a dangerous voltage you can suffer a dangerous electric shock when touching wires!


This device has left the factory in perfect condition. In order to maintain this condition and to ensure a safe operation, it is absolutely necessary for the user to follow the safety instructions and warning notes written in this user manual.

1. In order to guarantee the product’s life, please don’t put it in the damp places or even the environment over 60degress.

2. Always mount this unit in safe and stable matter.

The qualified professionals are allowed to carry out the lamp installation, operation and maintenance, but they must guarantee to operate in strict accordance with the instructions referred to.

Important:

Damages caused by the disregard of this user manual are not subject to warranty. The dealer will not accept liability for any resulting defects or problems.

If the device has been exposed to temperature changes due to environmental changes, do not switch it on immediately. The arising condensation could damage the device. Leave the device switched off until it has reached room temperatures.

This device falls under protection-classⅠ. Therefore it is essential that the device be earthed.

The electric connection must carry out by qualified person.

Make sure the power cord is never crimped or damaged by sharp edges. If this would be the case, replacement of the cable must be done by an authorized dealer.

Always disconnect from the mains, when the device is not in use or before cleaning it. Only handle the power cord by the plug. Never pull out the plug by tugging the power cord.

During initial start-up some smoke or smell may arise. This is a normal process and does not necessarily mean that the device is defective, it should decrease gradually.

Please don’t project the beam onto combustible substances.

If the external flexible cable or cord of this luminaire is damaged, it shall be exclusively replaced by the manufacturer or his service agent or a similar qualified person in order to avoid a hazard.
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CAUTION!

Never touch the device during operation!
The housing may heat up!


	                                             C                  CAUTION!
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          N     Never look directly into the light source,

           A  As sensitive persons may suffer an epileptic shock.


Please be aware that damages caused by manual modifications to be the device are not subject to warranty. Keep away from children and non-professionals.
CLEANING AND MAINTENANCE

1. To reduce the risk of electrical shock or fire, do not expose this unit to rain or moisture.

2. Do not spill water or other liquids into or on to your unit.

3. During long periods of non-use, disconnect the unit’s main power.

4. It should be installed in a well-ventilated place, at a distance of 50 centimeters or more with the walls. At the same time, please check if the fan and ventilation holes are unobstructed.

The following points have to be considered during the inspection

All screws for installing the devices or parts of the device have to be tightly connected and must not be corroded.

There must not be any deformations on the housing. Fixations and installations spots(ceiling, suspension, trussing).

Mechanically moved parts must not show any traces of wearing and must not rotate with unbalances.

The electric power supply cables must not show any damage, material fatigue or sediments. Further instructions depending on the installation spot and usage have to be adhered by a skilled installer and any safety problems have to be removed.

	CAUTION!

                Disconnect from mains before starting maintenance operation!


In order to make the lights in good condition and extend the life time, we suggest a regular cleaning to the lights.

Clean the inside and outside lens each week to avoid the weakness of the lights due to accumulation of dust.

Clean the fan each week.

A detailed electric check by approved electrical engineer each three month, make sure that the circuit contacts are in good condition, prevent the poor contact of circuit from overheating.

We recommend a frequent cleaning of the device. Please use a moist, lint-free cloth. Never use alcohol or solvents !

DIAGRAM SECTION 
                            A．Function keys

                        B．Keying

                        C．Reduce key

                        D．Confirm key

                        E．LED display window

A    B    C   D


Operating instructions: Pressing function key A will cycle through fourteen different functional effects, and the first two digits of the digital display represent the current function (refer to the menu). The last two digits represent the parameters of the address code or speed where the function is located. Press the B or C key to modify its parameter values. Press the D key to confirm

Comparison Table of LED Display Window Functions（After selecting all functions, press the D key to confirm）

	Serial Number
	Display
	Function Description

	1
	A001
	Channel address code, (001-512)

B. Add or subtract address code values with the C key

	2
	7ch/12ch/15ch/25ch
	Channel selection (7 channels, 12 channels, 15 channels,25 channels)

B. C key addition and subtraction

	3
	CC32
	（32—80）

B、C

	4
	Tr01
	Effect，（01—20）

B、C Key modification effect

	5
	To99
	Effect speed，（00—99）

C Key to modify pulse speed

	6
	R255
	Red color selection, (000-255)

B. C key to modify color selection

	7
	G255
	Green color selection, (000-255)

B. C key to modify color selection

	8
	B255
	Blue color selection, (000-255)

B. C key to modify color selection

	9
	O255
	White color selection, (000-255)

B. C key to modify color selection

	10
	F255
	Focusing, (000-255)

B. C key to modify color selection


Comparison Table of LED Background Display Window Functions（Press the A key frequently for 3-4 seconds in A001 state to enter and press the D key to exit）
	Serial Number
	Display
	Function Description

	1
	A128
	Motor calibration, (000-255) default value (128)

	2
	T128
	Motor travel, (000-255) default value (128)

	3
	SP10
	Motor speed，（002—20）default value(10)

	4
	ST10
	Mode strength，（002—20）default value(10)

	5
	R240
	Red current, (020-255) default value (240)

	6
	G205
	Green current, (020-255) default value (205)

	7
	B205
	Blue current, (020-255) default value (205)

	8
	O205
	White current, (020-255) default value (205)

	9
	n255
	Total power limit, (050-255) default value (255 not limited)

	10
	LEdF
	LEdF (Host Backend Setting Parameter) does not push default values to the slave (LEdF)

	
	
	The LEdO host pushes to the slave to update the backend parameters of the slave

Attention: The signal line between the host and the slave is connected and powered on. The slave is set to DMX512 mode. After entering this option, the host should not rush to exit. Wait for the slave light to flash to indicate that the slave update is successful. At this time, the host can exit

	11
	C-55
	Lamp body temperature value setting, (40-70) default value (55) Note: This function only works when the lamp body is connected to a temperature control resistor

	12
	doFF
	DoFF dmx512 segment signal not maintained (the light enters the off state after the segment signal) default value (doFF)

	
	
	Don dmx512 segment signal retention (the light remains in the state before the segment signal after the segment signal)

	13
	S000
	The dimming speed (000-255) is only valid when selecting the 16bt dimming mode, and this menu will not appear when selecting the -8bt dimming mode

	14
	bt-16
	Default Dimming Bit Number (16)

When dimming to 16 bits, the LED changes smoothly; When it is 8-bit, the LED changes sharply.

	15
	F-15
	Default dimming frequency value (15K)

The larger the dimming frequency value, the finer the grayscale level division

	16
	L-01
	Dimming curves (1-4), default value (01)

01 Linear dimming. 02 square dimming. 03 Anti square dimming. 04 S-shaped dimming.

	17
	LoFF

（password：ABCD）
	Disable the password lock default value LoFF.

	
	
	Open password lock Lon-

	18
	Eon-
	EoFF   The backlight of the display screen is always on

	
	
	Eon-   Display screen backlight enters screensaver default value (Eon -) after 30 seconds

	19
	FAN1
	FAN1 fan is controlled by temperature and lighting default values (FAN1). Note: When the temperature display is above 45 degrees and the light bulb is on, the fan starts. If the temperature display drops by 40 degrees, the fan stops regardless of whether the light bulb is on or off. If there is no temperature control, the fan is only controlled by the light, that is, the fan starts when the light is turned on and stops after 20 seconds when the light is turned off

	
	
	FAN0 fan is not subject to temperature control and lighting control (normal rotation)

	20
	HoFF
	HoFF

	
	
	Hon

	21
	LoAd
	LoAd

	
	
	LdEd 


TECHNICAL PARAMETERS

Voltage: AC 110–240V ±10% / 50–60Hz

Power Supply: 24V

Fan: 24V

Power Consumption: 220W

LED Type: RGBW (15W)

Colors: RGBW

Light Source Lifespan: >50,000 hours

Dimming: 0–100% linear adjustment

Number of LEDs: 19 (RGBW)

Strobe: 1–30Hz (standard strobe)

Control Modes: DMX512, RDM, Master/Slave

Channels: 06/10/18 CH

Motor: 2-phase stepper motor (8Ω x 3 in series)

Display: Digital LED display

Zoom Angle: 4.5°–50°

WEIGHT & SIZE

Fixture size:
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CHANNEL LIST

6CH LIST

	CH
	FUNCTION
	DESCRIPTION

	1
	R
	R dimming, dark to bright

	2
	G
	G dimming, dark to bright

	3
	B
	B dimming, dark to bright

	4
	W
	W dimming, dark to bright

	5
	Zoom
	from small to big

	6
	Reset
	Value 200-240, 10 seconds reset


10CH LIST
	CH
	FUNCTION
	DESCRIPTION

	1
	Total dim
	dark to bright

	2
	Total strobe
	slow to fast

	3
	R
	R dimming, dark to bright

	4
	G
	G dimming, dark to bright

	5
	B
	B dimming, dark to bright

	6
	W
	W dimming, dark to bright

	7
	RGBW running
	40 kinds effect

	8
	RGBS running speed
	slow to fast

	9
	Zoom
	from small to big

	10
	Reset
	Value 200-240, 10 seconds reset


18CH LIST
	CH
	FUNCTION
	DESCRIPTION

	1
	Total dim
	dark to bright

	2
	Total strobe
	slow to fast

	3
	R 1
	R 1 dimming, dark to bright

	4
	G 1
	G 1 dimming, dark to bright

	5
	B 1
	B 1 dimming, dark to bright

	6
	W 1
	W 1 dimming, dark to bright

	7
	...
	...

	11
	R 3
	R 3 dimming, dark to bright

	12
	G 3
	G 3 dimming, dark to bright

	13
	B 3
	B 3 dimming, dark to bright

	14
	W 3
	W 3 dimming, dark to bright

	15
	RGBW running
	40 kinds effect

	16
	RGBS running speed
	slow to fast

	17
	Zoom
	from small to big

	18
	Reset
	Value 200-240, 10 seconds reset


REMARK 
The product has perfect performance and intergrity packing. All users should be strictly comply with the warning 
and operating instructions as stated. Or we aren’t in charge of any result by misusing. 
Any damage resulting by misuse is not within the Company’s warranty. 
Any fault or problem caused by neglecting the manual is also not in the charge of dealers. 
Errors and omissions for every information given in this manual excepted. 
All information is subject to change without prior notice.

Thank you again for your patronage!
We will be offering sincere service as always,

Wish you have a good lighting journey!
