,Sales Region##OTHER##TEXT,Humidity##OTHER##TEXT,Image Sensor##OTHER##TEXT,Lens Type##OTHER##TEXT,Resolution##OTHER##TEXT,Signal to Noise Ratio##OTHER##TEXT,Storage Temperature##OTHER##TEXT,Wide Dynamic Range##OTHER##TEXT,z Part Number##OTHER##TEXT,z Part Description##OTHER##TEXT,Product Page URL##OTHER##TEXT,Product Documentation Link##OTHER##TEXT,z Type Camera Series##OTHER##TEXT,Camera Material##OTHER##TEXT,Camera Trim Material##OTHER##TEXT
"AVBMP, 12x Zoom, North America, Silver",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.34 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Optical Zoom with 73.0ø (wide end) to 6.6ø (tele end), f=3.91mm to 47mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9900-500,"Vaddio AVBMP, 12x Zoom, North America, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-avbmp,http://www.vaddio.com/library?path=d&file=roboshot-12-tech-spec-rev-a.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"AVBMP, 30x Zoom, North America, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor",30X Optical Zoom,1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9910-500,"Vaddio AVBMP, 30x Zoom, North America, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30-black-avbmp,http://www.vaddio.com/library?path=d&file=roboshot-30-tech-spec-rev-a.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"AVBMP, 30x Zoom, North America, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor",30X Optical Zoom,1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9910-500W,"Vaddio AVBMP, 30x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot-30-black-avbmp,http://www.vaddio.com/library?path=d&file=roboshot-30-tech-spec-rev-a.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"AVBMP, 12x Zoom, North America, Elite, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.34 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Optical Zoom with 73.0ø (wide end) to 6.6ø (tele end), f=3.91mm to 47mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99000-500,"Vaddio AVBMP, 12x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-avbmp,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"AVBMP, 12x Zoom, North America, Elite, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.34 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Optical Zoom with 73.0ø (wide end) to 6.6ø (tele end), f=3.91mm to 47mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99000-500W,"Vaddio AVBMP, 12x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-avbmp,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"AVBMP, 30x Zoom, North America, Elite, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor",30X Optical Zoom,1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99100-500,"Vaddio AVBMP, 30x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-black-avbmp,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"AVBMP, 30x Zoom, North America, Elite, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixel, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor",30X Optical Zoom,1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99100-500W,"Vaddio AVBMP, 30x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-black-avbmp,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 30x Zoom, North America, Black",North America,"20% to 80% RH, non-condensing",1/2.8-Type Exmor R? backlit CMOS sensor,"30X optical zoom, 65ø (wide) to 2.3ø (tele), F1.6 to F4.7",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9963-000,"Vaddio HDBT, 30x Zoom, North America, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-10-rev-c-roboshot-hdbt-tech-spec.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 30x Zoom, North America, White",North America,"20% to 80% RH, non-condensing",1/2.8-Type Exmor R? backlit CMOS sensor,"30X optical zoom, 65ø (wide) to 2.3ø (tele), F1.6 to F4.7",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9963-000W,"Vaddio HDBT, 30x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot-30-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-10-rev-c-roboshot-hdbt-tech-spec.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 30x Zoom, Europe/UK, Black",Europe/UK,"20% to 80% RH, non-condensing",1/2.8-Type Exmor R? backlit CMOS sensor,"30X optical zoom, 65ø (wide) to 2.3ø (tele), F1.6 to F4.7",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9963-001,"Vaddio HDBT, 30x Zoom, Europe/UK, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-10-rev-c-roboshot-hdbt-tech-spec.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 30x Zoom, Europe/UK, White",Europe/UK,"20% to 80% RH, non-condensing",1/2.8-Type Exmor R? backlit CMOS sensor,"30X optical zoom, 65ø (wide) to 2.3ø (tele), F1.6 to F4.7",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9963-001W,"Vaddio HDBT, 30x Zoom, Europe/UK, White PTZ Camera",http://www.vaddio.com/product/roboshot-30-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-10-rev-c-roboshot-hdbt-tech-spec.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 30x Zoom, Australia/New Zealand, Black",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.8-Type Exmor R? backlit CMOS sensor,"30X optical zoom, 65ø (wide) to 2.3ø (tele), F1.6 to F4.7",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9963-009,"Vaddio HDBT, 30x Zoom, Australia/New Zealand, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-10-rev-c-roboshot-hdbt-tech-spec.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 30x Zoom, Australia/New Zealand, White",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.8-Type Exmor R? backlit CMOS sensor,"30X optical zoom, 65ø (wide) to 2.3ø (tele), F1.6 to F4.7",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9963-009W,"Vaddio HDBT, 30x Zoom, Australia/New Zealand, White PTZ Camera",http://www.vaddio.com/product/roboshot-30-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-10-rev-c-roboshot-hdbt-tech-spec.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 12x Zoom, North America, Silver",North America,"20% to 80% RH, non-condensing",1/2.8-Type Exmor? CMOS sensor,"12X optical zoom, 73.0ø (wide) to 6.6ø (tele), f=3.91mm to 47.0mm,ÿ F1.8 to F3.4",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9960-000,"Vaddio HDBT, 12x Zoom, North America, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-20-rev-b-roboshot-12-hdbt-a-and-e-spec.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDBT, 12x Zoom, Europe/UK, Silver",Europe/UK,"20% to 80% RH, non-condensing",1/2.8-Type Exmor? CMOS sensor,"12X optical zoom, 73.0ø (wide) to 6.6ø (tele), f=3.91mm to 47.0mm,ÿ F1.8 to F3.4",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9960-001,"Vaddio HDBT, 12x Zoom, Europe/UK, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-20-rev-b-roboshot-12-hdbt-a-and-e-spec.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDBT, 12x Zoom, Australia/New Zealand, Silver",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.8-Type Exmor? CMOS sensor,"12X optical zoom, 73.0ø (wide) to 6.6ø (tele), f=3.91mm to 47.0mm,ÿ F1.8 to F3.4",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9960-009,"Vaddio HDBT, 12x Zoom, Australia/New Zealand, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-hdbt,http://www.vaddio.com/library?path=d&file=411-0003-20-rev-b-roboshot-12-hdbt-a-and-e-spec.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDBT, 12x Zoom, North America, Elite, Black",North America,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"12x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99600-000,"Vaddio HDBT, 12x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 12x Zoom, North America, Elite, White",North America,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"12x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99600-000W,"Vaddio HDBT, 12x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 30x Zoom, North America, Elite, Black",North America,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"30x zoom, 20 x optical zoom + 10x IntelliZoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99630-000,"Vaddio HDBT, 30x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 30x Zoom, North America, Elite, White",North America,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"30x zoom, 20 x optical zoom + 10x IntelliZoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99630-000W,"Vaddio HDBT, 30x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 12x Zoom, Europe/UK, Elite, Black",Europe/UK,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"12x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99600-001,"Vaddio HDBT, 12x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 12x Zoom, Europe/UK, Elite, White",Europe/UK,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"12x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99600-001W,"Vaddio HDBT, 12x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 30x Zoom, Europe/UK, Elite, Black",Europe/UK,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"30x zoom, 20 x optical zoom + 10x IntelliZoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99630-001,"Vaddio HDBT, 30x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 30x Zoom, Europe/UK, Elite, White",Europe/UK,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"30x zoom, 20 x optical zoom + 10x IntelliZoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99630-001W,"Vaddio HDBT, 30x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 12x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"12x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99600-009,"Vaddio HDBT, 12x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 12x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"12x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99600-009W,"Vaddio HDBT, 12x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDBT, 30x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"30x zoom, 20 x optical zoom + 10x IntelliZoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99630-009,"Vaddio HDBT, 30x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDBT, 30x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,"20% to 80% RH, non-condensing",1/2.5 Type Exmor R CMOS Sensor,"30x zoom, 20 x optical zoom + 10x IntelliZoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",1080 x 1920,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-99630-009W,"Vaddio HDBT, 30x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdbt,http://www.vaddio.com/library?path=d&file=us-datasheet-roboshot-elite-12-30-hdbt-190045.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 30x Zoom, North America, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9943-000,"Vaddio HDMI, 30x Zoom, North America, Black PTZ Camera",http://www.vaddio.com/product/roboshot30-hdmi,http://www.vaddio.com/library?path=d&file=roboshot_hdmi_prelim-techspectech_rev-01--1---1-.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 30x Zoom, North America, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9943-000W,"Vaddio HDMI, 30x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot30-hdmi,http://www.vaddio.com/library?path=d&file=roboshot_hdmi_prelim-techspectech_rev-01--1---1-.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 30x Zoom, Europe/UK, Black",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9943-001,"Vaddio HDMI, 30x Zoom, Europe/UK, Black PTZ Camera",http://www.vaddio.com/product/roboshot30-hdmi,http://www.vaddio.com/library?path=d&file=roboshot_hdmi_prelim-techspectech_rev-01--1---1-.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 30x Zoom, Europe/UK, White",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9943-001W,"Vaddio HDMI, 30x Zoom, Europe/UK, White PTZ Camera",http://www.vaddio.com/product/roboshot30-hdmi,http://www.vaddio.com/library?path=d&file=roboshot_hdmi_prelim-techspectech_rev-01--1---1-.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, North America, Cisco SX Codecs, Silver",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-400,"Vaddio HDMI, 12x Zoom, North America, Cisco SX Codecs, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi-cisco,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, North America, Polycom Codecs, Silver",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-500,"Vaddio HDMI, 12x Zoom, North America, Polycom Codecs, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi-polycom,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, North America, Silver",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-000,"Vaddio HDMI, 12x Zoom, North America, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Europe/UK, Cisco SX Codecs, Silver",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-401,"Vaddio HDMI, 12x Zoom, Europe/UK, Cisco SX Codecs, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi-cisco,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Europe/UK, Polycom Codecs, Silver",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-501,"Vaddio HDMI, 12x Zoom, Europe/UK, Polycom Codecs, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi-polycom,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Europe/UK, Silver",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-001,"Vaddio HDMI, 12x Zoom, Europe/UK, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Australia/New Zealand, Silver",Australia/New Zealand,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-9940-009,"Vaddio HDMI, 12x Zoom, Australia/New Zealand, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-hdmi,http://www.vaddio.com/library?path=d&file=roboshot-hdmi-tech-spec-reva.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HDMI, 12x Zoom, North America, Elite, Cisco SX Codecs, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-400,"Vaddio HDMI, 12x Zoom, North America, Elite, Cisco SX Codecs, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-cisco,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, North America, Elite, Cisco SX Codecs, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-400W,"Vaddio HDMI, 12x Zoom, North America, Elite, Cisco SX Codecs, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-cisco,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, North America, Elite, Polycom Codecs, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-500,"Vaddio HDMI, 12x Zoom, North America, Elite, Polycom Codecs, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-polycom,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, North America, Elite, Polycom Codecs, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-500W,"Vaddio HDMI, 12x Zoom, North America, Elite, Polycom Codecs, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-polycom,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, North America, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-000,"Vaddio HDMI, 12x Zoom, North America, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, North America, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-000W,"Vaddio HDMI, 12x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 30x Zoom, North America, Elite, Black",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99430-000,"Vaddio HDMI, 30x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdmi,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 30x Zoom, North America, Elite, White",North America,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99430-000W,"Vaddio HDMI, 30x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdmi,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, Europe/UK, Elite, Cisco SX Codecs, Black",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-401,"Vaddio HDMI, 12x Zoom, Europe/UK, Elite, Cisco SX Codecs, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-cisco,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Europe/UK, Elite, Cisco SX Codecs, White",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-401W,"Vaddio HDMI, 12x Zoom, Europe/UK, Elite, Cisco SX Codecs, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-cisco,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, Europe/UK, Elite, Polycom Codecs, Black",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-501,"Vaddio HDMI, 12x Zoom, Europe/UK, Elite, Polycom Codecs, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-polycom,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Europe/UK, Elite, Polycom Codecs, White",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-501W,"Vaddio HDMI, 12x Zoom, Europe/UK, Elite, Polycom Codecs, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi-polycom,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, Europe/UK, Black",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-001,"Vaddio HDMI, 12x Zoom, Europe/UK, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Europe/UK, White",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4 ",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-001W,"Vaddio HDMI, 12x Zoom, Europe/UK, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 30x Zoom, Europe/UK, Elite, Black",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99430-001,"Vaddio HDMI, 30x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdmi,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 30x Zoom, Europe/UK, Elite, White",Europe/UK,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","65ø wide end to 2.3ø tele end, f=4.3mm to 129mm, F1.6 to F4.7",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99430-001W,"Vaddio HDMI, 30x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-hdmi,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HDMI, 12x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-009,"Vaddio HDMI, 12x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HDMI, 12x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,20% to 80% Humidity,"Exmor 1/2.8?, 2.38 Megapixels, Full HD (1080p/60 native) High-speed, Low Noise CMOS Image Sensor","12X Mode: f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,> 50 dB,0øC to +40øC (32øF to 104øF),No,999-99400-009W,"Vaddio HDMI, 12x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-hdmi,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"HD-SDI, 12x Zoom, North America, Silver",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9930-000,"Vaddio HD-SDI, 12x Zoom, North America, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HD-SDI, 30x Zoom, North America, Black",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9933-000,"Vaddio HD-SDI, 30x Zoom, North America, Black PTZ Camera",http://www.vaddio.com/product/roboshot30-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HD-SDI, 30x Zoom, North America, White",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9933-000W,"Vaddio HD-SDI, 30x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot30-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HD-SDI, 12x Zoom, Europe/UK, Silver",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9930-001,"Vaddio HD-SDI, 12x Zoom, Europe/UK, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HD-SDI, 30x Zoom, Europe/UK, Black",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9933-001,"Vaddio HD-SDI, 30x Zoom, Europe/UK, Black PTZ Camera",http://www.vaddio.com/product/roboshot30-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HD-SDI, 30x Zoom, Europe/UK, White",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9933-001W,"Vaddio HD-SDI, 30x Zoom, Europe/UK, White PTZ Camera",http://www.vaddio.com/product/roboshot30-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"HD-SDI, 12x Zoom, Australia/New Zealand, Silver",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9930-009,"Vaddio HD-SDI, 12x Zoom, Australia/New Zealand, Silver PTZ Camera",http://www.vaddio.com/product/roboshot12-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"HD-SDI, 30x Zoom, Australia/New Zealand, Black",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9933-009,"Vaddio HD-SDI, 30x Zoom, Australia/New Zealand, Black PTZ Camera",http://www.vaddio.com/product/roboshot30-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"HD-SDI, 30x Zoom, Australia/New Zealand, White",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-9933-009W,"Vaddio HD-SDI, 30x Zoom, Australia/New Zealand, White PTZ Camera",http://www.vaddio.com/product/roboshot30-sdi,http://www.vaddio.com/library?path=d&file=342-1100-revb-roboshot-hd-sdi-tech-spec--1-.pdf,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"SDI, 30x Zoom, North America, Elite, Black",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99330-000,"Vaddio SDI, 30x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-sdi,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"SDI, 30x Zoom, North America, Elite, White",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99330-000W,"Vaddio SDI, 30x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-sdi,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"SDI, 30x Zoom, Europe/UK, Elite, Black",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99330-001,"Vaddio SDI, 30x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-sdi,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"SDI, 30x Zoom, Europe/UK, Elite, White",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99330-001W,"Vaddio SDI, 30x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-sdi,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"SDI, 30x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99330-009,"Vaddio SDI, 30x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-sdi,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"SDI, 30x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99330-009W,"Vaddio SDI, 30x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-sdi,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"SDI, 12x Zoom, North America, Elite, Black",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99300-000,"Vaddio SDI, 12x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-sdi,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"SDI, 12x Zoom, North America, Elite, White",North America,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99300-000W,"Vaddio SDI, 12x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-sdi,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"SDI, 12x Zoom, Europe/UK, Elite, Black",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99300-001,"Vaddio SDI, 12x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-sdi,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"SDI, 12x Zoom, Europe/UK, Elite, White",Europe/UK,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99300-001W,"Vaddio SDI, 12x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-sdi,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"SDI, 12x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99300-009,"Vaddio SDI, 12x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-sdi,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"SDI, 12x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,20% to 80% Relative Humidity,1/2.8-Type Exmor CMOS sensor,"12X Optical Zoom, 73.0ø (wide) to 6.6ø (tele),f=3.91mm to 47.0mm, F1.8 to F3.4",1080 x 1920,Greater than 50 dB,0øC to +40øC (32øF to 104øF),No,999-99300-009W,"Vaddio SDI, 12x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-sdi,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"UHD, 40x Zoom, North America, Black",North America,"20% to 80% RH, non-condensing","1/2.5 Type Exmor R CMOS Sensor, 4K","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-9952-000,"Vaddio UHD, 40x Zoom, North America, Black PTZ Camera",http://www.vaddio.com/product/roboshot-40-uhd,http://www.vaddio.com/library?path=d&file=180377-us-datasheet-roboshot_40_uhd.pdf,40,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"UHD, 40x Zoom, North America, White",North America,"20% to 80% RH, non-condensing","1/2.5 Type Exmor R CMOS Sensor, 4K","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-9952-000W,"Vaddio UHD, 40x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot-40-uhd,http://www.vaddio.com/library?path=d&file=180377-us-datasheet-roboshot_40_uhd.pdf,40,Plastic - Vaddio - White,Plastic - Vaddio - White
"UHD, 40x Zoom, Europe/UK, Black",Europe/UK,"20% to 80% RH, non-condensing","1/2.5 Type Exmor R CMOS Sensor, 4K","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-9952-001,"Vaddio UHD, 40x Zoom, Europe/UK, Black PTZ Camera",http://www.vaddio.com/product/roboshot-40-uhd,http://www.vaddio.com/library?path=d&file=180377-us-datasheet-roboshot_40_uhd.pdf,40,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"UHD, 40x Zoom, Europe/UK, White",Europe/UK,"20% to 80% RH, non-condensing","1/2.5 Type Exmor R CMOS Sensor, 4K","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-9952-001W,"Vaddio UHD, 40x Zoom, Europe/UK, White PTZ Camera",http://www.vaddio.com/product/roboshot-40-uhd,http://www.vaddio.com/library?path=d&file=180377-us-datasheet-roboshot_40_uhd.pdf,40,Plastic - Vaddio - White,Plastic - Vaddio - White
"UHD, 40x Zoom, Australia/New Zealand, Black",Australia/New Zealand,"20% to 80% RH, non-condensing","1/2.5 Type Exmor R CMOS Sensor, 4K","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-9952-009,"Vaddio UHD, 40x Zoom, Australia/New Zealand, Black PTZ Camera",http://www.vaddio.com/product/roboshot-40-uhd,http://www.vaddio.com/library?path=d&file=180377-us-datasheet-roboshot_40_uhd.pdf,40,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"UHD, 40x Zoom, Australia/New Zealand, White",Australia/New Zealand,"20% to 80% RH, non-condensing","1/2.5 Type Exmor R CMOS Sensor, 4K","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,More than 50 dB,0øC to +40øC (32øF to 104øF),Yes,999-9952-009W,"Vaddio UHD, 40x Zoom, Australia/New Zealand, White PTZ Camera",http://www.vaddio.com/product/roboshot-40-uhd,http://www.vaddio.com/library?path=d&file=180377-us-datasheet-roboshot_40_uhd.pdf,40,Plastic - Vaddio - White,Plastic - Vaddio - White
"UHD, 20x Zoom, North America, Silver",North America,20% to 80% RH (non-condensing),"1/2.3-Type Exmor R High-speed, Low-noise CMOS Sensor","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,Over 50 dB,-20ø to +60ø C (-4øF to 140øF),No,999-9950-000,"Vaddio UHD, 20x Zoom, North America, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-20-uhd,http://www.vaddio.com/library?path=d&file=342-1189-revb-roboshot-20-uhd-tech-spec.pdf,20,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"UHD, 20x Zoom, North America, White",North America,20% to 80% RH (non-condensing),"1/2.3-Type Exmor R High-speed, Low-noise CMOS Sensor","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,Over 50 dB,-20ø to +60ø C (-4øF to 140øF),No,999-9950-000W,"Vaddio UHD, 20x Zoom, North America, White PTZ Camera",http://www.vaddio.com/product/roboshot-20-uhd,http://www.vaddio.com/library?path=d&file=342-1189-revb-roboshot-20-uhd-tech-spec.pdf,20,Plastic - Vaddio - White,Plastic - Vaddio - White
"UHD, 20x Zoom, Europe/UK, Silver",Europe/UK,20% to 80% RH (non-condensing),"1/2.3-Type Exmor R High-speed, Low-noise CMOS Sensor","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,Over 50 dB,-20ø to +60ø C (-4øF to 140øF),No,999-9950-001,"Vaddio UHD, 20x Zoom, Europe/UK, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-20-uhd,http://www.vaddio.com/library?path=d&file=342-1189-revb-roboshot-20-uhd-tech-spec.pdf,20,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"UHD, 20x Zoom, Europe/UK, White",Europe/UK,20% to 80% RH (non-condensing),"1/2.3-Type Exmor R High-speed, Low-noise CMOS Sensor","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,Over 50 dB,-20ø to +60ø C (-4øF to 140øF),No,999-9950-001W,"Vaddio UHD, 20x Zoom, Europe/UK, White PTZ Camera",http://www.vaddio.com/product/roboshot-20-uhd,http://www.vaddio.com/library?path=d&file=342-1189-revb-roboshot-20-uhd-tech-spec.pdf,20,Plastic - Vaddio - White,Plastic - Vaddio - White
"UHD, 20x Zoom, Australia/New Zealand, Silver",Australia/New Zealand,20% to 80% RH (non-condensing),"1/2.3-Type Exmor R High-speed, Low-noise CMOS Sensor","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,Over 50 dB,-20ø to +60ø C (-4øF to 140øF),No,999-9950-009,"Vaddio UHD, 20x Zoom, Australia/New Zealand, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-20-uhd,http://www.vaddio.com/library?path=d&file=342-1189-revb-roboshot-20-uhd-tech-spec.pdf,20,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"UHD, 20x Zoom, Australia/New Zealand, White",Australia/New Zealand,20% to 80% RH (non-condensing),"1/2.3-Type Exmor R High-speed, Low-noise CMOS Sensor","20x optical zoom, f=4.4mm wide end to 88.4mm tele end, F2 to F3.8",3840 x 2160,Over 50 dB,-20ø to +60ø C (-4øF to 140øF),No,999-9950-009W,"Vaddio UHD, 20x Zoom, Australia/New Zealand, White PTZ Camera",http://www.vaddio.com/product/roboshot-20-uhd,http://www.vaddio.com/library?path=d&file=342-1189-revb-roboshot-20-uhd-tech-spec.pdf,20,Plastic - Vaddio - White,Plastic - Vaddio - White
"USB, 12x Zoom, North America, Silver",North America,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-9920-000,"Vaddio USB, 12x Zoom, North America, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-usb,http://www.vaddio.com/library?path=d&file=411-0000-10-rev-b-roboshot-12-usb-techspec.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"USB, 12x Zoom, Europe/UK, Silver",Europe/UK,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-9920-001,"Vaddio USB, 12x Zoom, Europe/UK, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-usb,http://www.vaddio.com/library?path=d&file=411-0000-10-rev-b-roboshot-12-usb-techspec.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"USB, 12x Zoom, Australia/New Zealand, Silver",Australia/New Zealand,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-9920-009,"Vaddio USB, 12x Zoom, Australia/New Zealand, Silver PTZ Camera",http://www.vaddio.com/product/roboshot-12-usb,http://www.vaddio.com/library?path=d&file=411-0000-10-rev-b-roboshot-12-usb-techspec.pdf,12,Plastic - Vaddio - Silver,Plastic - Vaddio - Black
"USB, 12x Zoom, North America, Elite, Black",North America,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99200-000,"Vaddio USB, 12x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-usb,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"USB, 12x Zoom, North America, Elite, White",North America,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99200-000W,"Vaddio USB, 12x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-usb,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"USB, 30x Zoom, North America, Elite, Black",North America,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99230-000,"Vaddio USB, 30x Zoom, North America, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-usb,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"USB, 30x Zoom, North America, Elite, White",North America,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99230-000W,"Vaddio USB, 30x Zoom, North America, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-usb,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"USB, 12x Zoom, Europe/UK, Elite, Black",Europe/UK,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99200-001,"Vaddio USB, 12x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-usb,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"USB, 12x Zoom, Europe/UK, Elite, White",Europe/UK,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99200-001W,"Vaddio USB, 12x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-usb,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"USB, 30x Zoom, Europe/UK, Elite, Black",Europe/UK,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99230-001,"Vaddio USB, 30x Zoom, Europe/UK, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-usb,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"USB, 30x Zoom, Europe/UK, Elite, White",Europe/UK,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99230-001W,"Vaddio USB, 30x Zoom, Europe/UK, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-usb,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
"USB, 12x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99200-009,"Vaddio USB, 12x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-12e-usb,,12,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"USB, 12x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"12X optical zoom, 73ø wide to 6.6ø tele, f=3.91 mm to 47 mm, F1.8 to F3.4",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99200-009W,"Vaddio USB, 12x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-12e-usb,,12,Plastic - Vaddio - White,Plastic - Vaddio - White
"USB, 30x Zoom, Australia/New Zealand, Elite, Black",Australia/New Zealand,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99230-009,"Vaddio USB, 30x Zoom, Australia/New Zealand, Elite, Black PTZ Camera",http://www.vaddio.com/product/roboshot-30e-usb,,30,Plastic - Vaddio - Black,Plastic - Vaddio - Black
"USB, 30x Zoom, Australia/New Zealand, Elite, White",Australia/New Zealand,20% to 80% non-condensing,1/2.8-type Exmor CMOS sensor,"30X optical zoom, 65ø (wide end) to 2.3ø (tele end), F1.6 to F4.7",1080 x 1920,Over 50 dB,-20øC to +60øC (-4øF to 140øF),No,999-99230-009W,"Vaddio USB, 30x Zoom, Australia/New Zealand, Elite, White PTZ Camera",http://www.vaddio.com/product/roboshot-30e-usb,,30,Plastic - Vaddio - White,Plastic - Vaddio - White
