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GYS08J型单钢轮振动压路机
GYS08J SINGLE DRUMVIBRATORY ROLLER
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	规格型号：GYS08J型单钢轮振动压路机

	Model: GYS08J Single Drum Vibratory Roller

	主要性能特点Performance characteristics：
1、机械驱动，三档行驶速度。
Mechanical drive, multi-step traveling speed.
2、液压振动，单频双幅，电控延时起振，激振力大，压实效率高；
Hydraulic vibration, single-frequency double amplitude, electronically controlled delayed vibration, large excitation force, high compaction efficiency.
3、液压转向，铰接式车架，操作轻便灵活；
Hydraulic steering, articulated frame, light and flexible operation.
4、配置带同步器的压路机专用变速箱，传动扭矩大，换挡轻便；
Equipped with special gearbox for road rollers with synchronizer, high transmission torque and easy to shift.
5、气助力液压钳盘行车制动，内涨鼓式机械停车制动，安全可靠；
Air-assisted hydraulic caliper disk running brake, internal drum mechanical parking brake, safe and reliable.
6、后机罩可大角度翻起，维修保养方便；
Rear hood can be flipped up at a wide angle for easy maintenance.
7、液压元件采用知名品牌，性能可靠；
Hydraulic components adopt famous brand, reliable performance.
8、标配驾驶室，可选装空调。
Standard cab, optional A/C.

	主要技术参数 Main Parameters：
	GYS08J

	1、整机重量 Operating weight
	8000 kg

	2、振动轮直径 Vibratory drum diameter
	1200 mm

	3、振动轮宽度 Vibratory drum width
	1650 mm

	4、振动频率  Vibratory frequency
	42 Hz
	48 Hz

	5、理论振幅  Vibratory amplitude
	0.7 mm
	0.5 mm

	6、激振力 Centrifugal force
	85 kN

	7、行驶速度 Traveling speed

	前进 Forward
	2.2/4.2/7.5/12.5/15.5 km/h

	后退 Reverse
	2.5 km/h

	8、最小离地间隙 Min. ground clearance
	300 mm

	9、轴距 Wheel base
	2680 mm

	10、静线载荷 Static line pressure
	228 N/cm

	11、最小转弯半径 Min. turning radius
	5500 mm

	14、最大爬坡能力 Gradeability
	25%

	15、外形尺寸（长×宽×高）Dimensions
	5130×1830×2570 mm

	16、发动机型号 Engine model
	A498BG
	4D32G31

	型式 Type
	直列、四缸、四冲程、水冷
4 cylinder inline，4 stroke, water cooled

	功率 Power
	42 kW
	36.8 kW

	转速 Rated speed
	2200 r/min
	2500 r/min

	17、燃油箱容积 Fuel tank capacity
	145 L

	18、液压油箱 Hydraulic oil tank
	120 L

	19、轮胎 Tire type
	12.00-20


主要配置说明 Main configuration
	序号
S/N
	部件名称
Part name

	型号规格
MODEL
	数量
No.
	制造商
Manufacturer

	1
	柴油机
Engine
	A498BG
4D32G31
	1
	新柴
XINCHAI

	2
	振动泵
Vibratory pump
	GPC4-32
	1
	天津特精
PARKER

	3
	振动马达
Vibratory motor
	GMC4-25
	1
	天津特精
PARKER
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