{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Mitoitus","Kertoimet"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mitoitus","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[[13,7,13,10]]}
["v0_3"]
[null,null,null,null,null,"VALLOX AITO KOTILÄMPÖ"]
[null,null,null,null,null,"HUONEEN TULOILMAVIRRAN MITOITUS"]
[]
[]
[null,"Patterille menevän veden lämpötila °C"]
[null,40]
[]
[]
[]
[]
[]
[]
[null,"Huone","Ulkoseiniä",null,"Lattiapinta-ala",null,null,"Tuloilmavirta"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[null,null,null,"kpl",null,"m2",null,null,"l/s",null,"m3/h"]
[]
[null,null,null,null,null,"YHT.",null,null,"l/s",null,"m3/h"]

{"sheet":"Kertoimet","index":1,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":true,"merged":[[1,1,1,3]]}
[]
[null,"VALINNAT"]
[null,"Ulkoseiniä",null,"Tuloilman lämpötila",null,"suoran yhtälö"]
[null,"0/1",null,40]
[null,2,null,50,null,"b = 0"]
[null,null,null,60]
[]
[]
[]
[]
[]
[]
[null,"Ulkoseiniä 1"]
[null,"y2","y1","x2","x1","Kulmakerroin"]
[35,54,23,28,12,{"$f":"(B15-C15)/(D15-E15)","v":1.9375}]
[40,40,17,28,12,1.4375]
[45,32,14,28,12,1.125]
[50,27,12,28,12,0.9375]
[55,23,10,28,12,0.8125]
[60,21,8,28,12,0.8125]
[65,19,7,28,12,0.75]
[70,17,6,28,12,0.6875]
[]
[null,"Ulkoseiniä 2"]
[null,"y2","y1","x2","x1","Kulmakerroin"]
[35,53,23,21.1,9.3000000000000007,{"$f":"(B26-C26)/(D26-E26)","v":2.5423728813559321}]
[40,40,17,21.1,9.3000000000000007,1.9491525423728813]
[45,32,14,21.1,9.3000000000000007,1.5254237288135593]
[50,27,12,21.1,9.3000000000000007,1.271186440677966]
[55,23,10,21.1,9.3000000000000007,1.1016949152542372]
[60,21,8,21.1,9.3000000000000007,1.1016949152542372]
[65,19,7,21.1,9.3000000000000007,1.0169491525423728]
[70,17,6,21.1,9.3000000000000007,0.93220338983050843]
[]
[]
[null,"FIN",1]
[null,"SWE",0]
[null,"ENG",0]